For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Dome Lamp Lens Tip Use a small flat bladed tool to aid in the removal of the lens.
2 | Dome Lamp Assembly Tip

1. Using a small flat-bladed tool, disengage the dome lamp attaching clips by gently prying at each side of the retaining tab while pulling the tab off of the headliner.
2. Pull the forward edge of the dome lamp downward and rearward to disengage the lamp from the headliner.
3. Disconnect the electrical connector.