For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the rear wiper arm blade. Refer to Rear Window Wiper Blade Replacement .

1 | Rear Wiper Arm Blade
2 | Rear Wiper Arm Blade Bear Claws
3 | Rear Wiper Arm Blade Insert Tip Hold the wiper arm blade firmly and pull blade element from blade bear claws.