For 1990-2009 cars

Connector 1: | C1 Wiring Harness Side to Transmission Side

### C1 Wiring Harness Side to Transmission Side

#### Connector Part Information

- OEM: PBT-GF15
- Service: Non-serviceable
- Description: Conn 16F (BK)

#### Connector Part Information

- OEM: PBT-GF30
- Service: Non-serviceable
- Description: Conn 16M (BK)

#### Terminal Part Information

- Terminal: Non-serviceable
- Core/Insulation Crimp: Non-serviceable
- Release Tool/Test Probe: Non-serviceable

#### Terminal Part Information

- Terminal: Non-serviceable
- Core/Insulation Crimp: Non-serviceable
- Release Tool/Test Probe: Non-serviceable

#### C1 Wiring Harness Side to Transmission Side

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 540 | Battery Positive Voltage | 1 | -- | 540 | Battery Positive Voltage
2-4 | -- | -- | Not Used | 2-4 | -- | -- | Not Used
5 | OG/BK | 1786 | Park/Neutral Signal | 5 | -- | 1786 | Park/Neutral Signal
6 | TN | 2501 | High Speed GMLAN (-) | 6 | -- | 2501 | High Speed GMLAN (-)
7 | TN/BK | 2500 | High Speed GMLAN (+) | 7 | -- | 2500 | High Speed GMLAN (+)
8 | TN/BK | 2500 | High Speed GMLAN (+) | 8 | -- | 2500 | High Speed GMLAN (+)
9 | BK/WH | 451 | Ground | 9 | -- | 451 | Ground
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | PK | 1339 | Ignition Voltage | 11 | -- | 1339 | Ignition Voltage
12 | BN | 4 | Accessory Voltage | 12 | -- | 4 | Accessory Voltage
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | TN | 2501 | High Speed GMLAN (-) | 14 | -- | 2501 | High Speed GMLAN (-)
15-16 | -- | -- | Not Used | 15-16 | -- | -- | Not Used