For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Range Selector Lever Cable Tip For additional information on disconnecting the range selector lever cable from the bracket or lever, refer to Range Selector Lever Cable Replacement.
2 | Range Selector Lever Cable Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
3 | Range Selector Lever Cable Bracket