For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Side Door Window Regulator Bolts | 10 N·m | 89 lb in
Front Side Door Window Regulator Motor Screws | 8 N·m | 71 lb in
Front Side Door Latch Screws | 10 N·m | 89 lb in
Front Side Door Module Bolts | 8 N·m | 71 lb in
Front Side Door Outer Belt Sealing Strip Screws | 1.5 N·m | 1.3 lb in
Front Side Door Window Regulator Motor Bolts | 8 N·m | 71 lb in
Front Side Door Window Run Channel Bolts | 8 N·m | 71 lb in
Rear Side Door Latch Screws | 10 N·m | 89 lb in
Rear Side Door Module Bolts | 8 N·m | 71 lb in
Rear Side Door Outer Belt Sealing Strip Screws | 1.5 N·m | 1.3 lb in
Rear Side Door Window Regulator Motor Bolts | 8 N·m | 71 lb in
Rear Side Door Window Run Channel Seal Bolts, Left and Right Side | 8 N·m | 71 lb in
Rear Side Door Window Run Channel Seal Upper Corner Screw to Door Frame | 6 N·m | 53 lb in
Rear Side Door Window Run Channel Bolts | 8 N·m | 71 lb ft