For 1990-2009 cars

### Removal Procedure

1. Remove the shift control . Refer to Transmission Control Replacement.
2. Slide the center floor air outlet duct forward enough to clear the rear floor air outlet duct, and then up, and rearward to remove.

### Installation Procedure

1. Slide the center floor air outlet duct forward enough to clear rear floor air duct, and then down, and rearward to install.
2. Install the shift control. Refer to Transmission Control Replacement.