For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Air Inlet Assembly Screws | 1.5 N·m | 13 lb in
Air Outlet Duct Screws | 1.5 N·m | 13 lb in
Auxiliary A/C Line to Evaporator Outlet Hose Nut | 20 N·m | 15 lb ft
Auxiliary A/C Line to Liquid Line Nut | 20 N·m | 15 lb ft
Auxiliary A/C Lines to Auxiliary TXV Nut | 20 N·m | 15 lb ft
Auxiliary A/C Lines to Underbody Bolt | 9 N·m | 80 lb in
Auxiliary A/C Lines to Underbody Nuts | 9 N·m | 80 lb in
Auxiliary HVAC Actuator Screws | 1.5 N·m | 13 lb in
Auxiliary HVAC Blower Motor Control Module Screws | 1.5 N·m | 13 lb in
Auxiliary HVAC Blower Motor Screws | 1.5 N·m | 13 lb in
Auxiliary HVAC Ducts to Body Bolts | 8 N·m | 71 lb in
Auxiliary HVAC Ducts to Body Nuts | 8 N·m | 71 lb in
Auxiliary HVAC Heater Core Cover Screw | 1.5 N·m | 13 lb in
Auxiliary HVAC Module Assembly Screws | 1.5 N·m | 13 lb in
Auxiliary HVAC Module to Body Bolts | 9 N·m | 80 lb in
Auxiliary HVAC Side Case Screw | 1.5 N·m | 13 lb in
Auxiliary HVAC TXV Backing Plate Bolts | 3.5 N·m | 31 lb in
Battery Box to Body Bolts | 10 N·m | 89 lb in
Blower Case Assembly Screws | 1.5 N·m | 13 lb in
Blower Motor Control Module Screws | 1.5 N·m | 13 lb in
Blower Motor Screws | 1.5 N·m | 13 lb in
Compressor Clutch Bolt | 21 N·m | 16 lb ft
Compressor Clutch Coil Connector Bracket Screw | 4.3 N·m | 38 lb in
Compressor Clutch Coil Screws | 4.9 N·m | 43 lb in
Compressor Hose Assembly to Battery Box Nut | 9 N·m | 80 lb in
Compressor Hose Assembly to Compressor Nut | 20 N·m | 15 lb ft
Compressor Hose Assembly to Condenser Nut | 20 N·m | 15 lb ft
Compressor Pressure Relief Valve | 8.8 N·m | 78 lb in
Compressor to Engine Bolts | 50 N·m | 37 lb ft
Condenser to Radiator Bolts | 9 N·m | 80 lb in
CRFM Bracket Bolts | 20 N·m | 15 lb ft
Defogger Air Outlet Screw to I/P Upper Trim Panel | 1 N·m | 9 lb in
Defogger Duct Screw to I/P Upper Trim Panel | 1 N·m | 9 lb in
Evaporator Case Assembly Screws | 1.5 N·m | 13 lb in
Evaporator Outlet Hose and Liquid Line Clamp Bracket Nut to TXV | 20 N·m | 15 lb ft
Evaporator Outlet Hose to Compressor Hose Nut | 20 N·m | 15 lb ft
Front of Dash to HVAC Module Seal Nuts | 9 N·m | 80 lb in
Heater Core Cover Screws | 1.5 N·m | 13 lb in
HVAC Module to Cross Car Beam Nuts and Bolts | 8 N·m | 71 lb in
Instrument Panel (I/P) Air Outlet Screw | 2 N·m | 18 lb in
Liquid Line to Condenser Nut | 20 N·m | 15 lb ft
Liquid Line to Strut Tower Nut | 9 N·m | 80 lb in
Mode Actuator to Evaporator Case Screws | 1.5 N·m | 13 lb in
Mode Cam Bracket to Evaporator Case Screws | 1.5 N·m | 13 lb in
Passenger Compartment Air Filter Housing Nuts | 9 N·m | 80 lb in
Receiver Dehydrator to Condenser Bolt | 6.5 N·m | 58 lb in
Receiver Dehydrator Upper Clamp Bolt to Condenser | 4.2 N·m | 37 lb in
Refrigerant Pressure Sensor to Compressor Hose Assembly | 4 N·m | 35 lb in
Surge Tank to Body Bolts | 9 N·m | 80 lb in
TXV Backing Plate Bolts | 3.5 N·m | 31 lb in