For 1990-2009 cars

Table 1: | Indicators
Table 2: | DIC Warning Messages

#### Indicators

Symbol | Reference
--- | ---
| ABS: ABS Description and Operation
| Air Bag: SIR System Description and Operation
| AWD Disabled: All-Wheel Drive Description and Operation
(Export) BRAKE | BRAKE: Brake Warning System Description and Operation
| Change Engine Oil: The IPC displays the indicator when the engine control module (ECM) determines that the engine oil life is below 5 percent. Refer to GM Oil Life System Resetting
| Charge: Charging System Description and Operation
| Cruise: Cruise Control Description and Operation
[DOOR AJAR] | Door Ajar: Power Door Locks Description and Operation
| DRL: Exterior Lighting Systems Description and Operation
| Engine Coolant Temperature: Cooling System Description and Operation
| Fasten Seat Belt: Seat Belt System Description and Operation
| Fasten Passenger Seat Belt: Seat Belt System Description and Operation
| Hatch Ajar: Rear Hatch/Gate Description and Operation
| Front Fog Lamps: Exterior Lighting Systems Description and Operation
| High Beam: Exterior Lighting Systems Description and Operation
| Low Fuel: The instrument panel cluster (IPC) illuminates the Low Fuel indicator when the IPC detects that the fuel level is less than a pre-determined value.
| Low Oil Pressure: The instrument panel cluster (IPC) illuminates the Engine Oil Pressure indicator when the engine control module (ECM) detects a low engine oil pressure condition.
| MIL: Engine Control Module Description
| Passenger Air Bag Off: SIR System Description and Operation
| Passenger Air Bag On: SIR System Description and Operation
| Rear Fog Lamps: Exterior Lighting Systems Description and Operation
| Reduced Engine Power: Throttle Actuator Control (TAC) System Description
| Security: Content Theft Deterrent (CTD) Description and Operation
| Service AWD: All-Wheel Drive Description and Operation
| Service Vehicle Soon: The IPC displays the indicator when the ECM or BCM detects certain vehicle malfunctions that are not related to the emissions system.
| Tire Pressure Monitor: Tire Pressure Monitor Description and Operation
| Turn Signals: Exterior Lighting Systems Description and Operation
| Vehicle Dynamics Caution (VDC): ABS Description and Operation

#### DIC Warning Messages

Message | Reference
--- | ---
ALL WHEEL DRIVE OFF | All-Wheel Drive Description and Operation
BATTERY SAVER ACTIVE | Charging System Description and Operation
BRAKE FLUID LOW | Brake Warning System Description and Operation
BUCKLE PASSENGER SEAT BELT | Seat Belt System Description and Operation
BUCKLE SEATBELT | Seat Belt System Description and Operation
CALIBRATION COMPLETE | When the compass calibration process is complete and successful, the DIC displays CALIBRATION COMPLETE.
CALIBRATING: DRIVE IN CIRCLES | The DIC provides the display that allows the resetting of the currently stored compass calibrations data and establish new calibration data. When the compass calibration is in process, the DIC displays CALIBRATING: DRIVE IN CIRCLES. Refer to Compass Calibration and Magnetic Variance
CHANGE ENGINE OIL SOON | The DIC displays this message when the ECM determines that the engine oil needs to be changed. After the oil is changed, reset the engine oil monitor. Refer to GM Oil Life System Resetting
CHECK TIRE PRESSURE | Tire Pressure Monitor Description and Operation
CHECK LEFT FRONT TIRE PRESSURE | Tire Pressure Monitor Description and Operation
CHECK LEFT REAR TIRE PRESSURE | Tire Pressure Monitor Description and Operation
CHECK RIGHT FRONT TIRE PRESSURE | Tire Pressure Monitor Description and Operation
CHECK RIGHT REAR TIRE PRESSURE | Tire Pressure Monitor Description and Operation
COOLANT LEVEL LOW ADD COOLANT | Cooling System Description and Operation
CRUISE SET TO XXX | Cruise Control Description and Operation
DRIVER DOOR OPEN | Power Door Locks Description and Operation
ENGINE HOT A/C OFF | Cooling System Description and Operation
ENGINE OVERHEATED-IDLE ENGINE | Cooling System Description and Operation
ENGINE OVERHEATED STOP ENGINE | Cooling System Description and Operation
ENGINE POWER REDUCED | Throttle Actuator Control (TAC) System Description
FUEL LEVEL LOW | Refer to Indicator/Warning Message Description and Operation
HOOD OPEN | Content Theft Deterrent (CTD) Description and Operation
ICE POSSIBLE | Refer to Indicator/Warning Message Description and Operation
LIFT GATE OPEN | Rear Hatch/Gate Description and Operation
OIL PRESSURE LOW STOP ENGINE | The DIC displays this message when the ECM detects a low engine oil pressure condition from the engine oil pressure (EOP) switch.
PASSENGER DOOR OPEN (Front and Rear) | Power Door Locks Description and Operation
REMOTE KEY LEARNING ACTIVE | Keyless Entry System Description and Operation
REMOTE KEY LEARNING COMPLETE | Keyless Entry System Description and Operation
REPLACE BATTERY IN REMOTE KEY | Keyless Entry System Description and Operation
SERVICE A/C SYSTEM | Air Temperature Description and Operation
SERVICE AIR BAG | SIR System Description and Operation
SERVICE ALL WHEEL DRIVE | All-Wheel Drive Description and Operation
SERVICE BATTERY CHARGING SYSTEM | Charging System Description and Operation
SERVICE BRAKE SYSTEM | Brake Warning System Description and Operation
SERVICE COLUMN LOCK | Steering Wheel and Column Description and Operation
SERVICE POWER STEERING | Power Steering System Description and Operation
SERVICE STABILITY CONTROL | ABS Description and Operation
SERVICE TIRE MONITOR SYSTEM | Tire Pressure Monitor Description and Operation
SERVICE THEFT DETERENT SYSTEM | Keyless Entry System Description and Operation
SERVICE TRACTION CONTROL | ABS Description and Operation
SERVICE VEHICLE SOON | The DIC displays this message when the BCM detects certain malfunctions that are not related to the vehicle emission system.
SHIFT DENIED | Automatic Transmission Shift Lock Control Description and Operation
SPEED LIMITED TO XXX | Cruise Control Description and Operation
STABILITY CONTROL NOT READY | ABS Description and Operation
STABILITY CONTROL OFF | ABS Description and Operation
STARTING DISABLED SERVICE THROTTLE | Throttle Actuator Control (TAC) System Description
THEFT ATTEMPTED | Content Theft Deterrent (CTD) Description and Operation
TIGHTEN GAS CAP | Fuel System Description
TIRE LEARNING ACTIVE | Tire Pressure Monitor Description and Operation
TRACTION CONTROL OFF | ABS Description and Operation
TRACTION CONTROL ON | ABS Description and Operation
TURN SIGNAL ON | Exterior Lighting Systems Description and Operation
VEHICLE OVERSPEED | The driver information center (DIC) displays VEHICLE OVERSPEED message when the instrument panel cluster (IPC) determines that the vehicle speed is more than 120 km/h (75 mph).
WAIT TO START | Content Theft Deterrent (CTD) Description and Operation