For 1990-2009 cars

Connector 1: | A/C Compressor Clutch
Connector 2: | A/C Refrigerant Pressure Sensor
Connector 3: | Accelerator Pedal Position (APP) Sensor
Connector 4: | Accessory Power Outlet - Center Console 1
Connector 5: | Accessory Power Outlet - Center Console 2
Connector 6: | Accessory Power Outlet - Rear
Connector 7: | Air Temperature Actuator
Connector 8: | Air Temperature Actuator - Auxiliary (C69)
Connector 9: | Air Temperature Sensor - Lower
Connector 10: | Air Temperature Sensor - Upper
Connector 11: | Ambient Air Temperature Sensor
Connector 12: | Ambient Light Sensor
Connector 13: | Audio Amplifier X1 (U65)
Connector 14: | Audio Amplifier X2 (U65)
Connector 15: | Audio Amplifier X3 (U65)
Connector 16: | Audio/Video Adapter (UUC)
Connector 17: | Automatic Transmission Fluid Temperature (TFT) Sensor
Connector 18: | Automatic Transmission Shift Lock Control Solenoid
Connector 19: | Backup Lamp - Left
Connector 20: | Backup Lamp - Right
Connector 21: | Battery (-)
Connector 22: | Battery (+)
Connector 23: | Battery Current Sensor
Connector 24: | Blower Motor
Connector 25: | Blower Motor - Auxiliary (C69)
Connector 26: | Blower Motor Control Module X1
Connector 27: | Blower Motor Control Module X2
Connector 28: | Blower Motor Control Module - Auxiliary X1 (C69)
Connector 29: | Blower Motor Control Module - Auxiliary X2 (C69)
Connector 30: | Body Control Module (BCM) X1
Connector 31: | Body Control Module (BCM) X2
Connector 32: | Body Control Module (BCM) X3
Connector 33: | Body Control Module (BCM) X4
Connector 34: | Body Control Module (BCM) X5
Connector 35: | Body Control Module (BCM) X6
Connector 36: | Body Control Module (BCM) X7
Connector 37: | Brake Fluid Level Switch
Connector 38: | Brake Pedal Position Sensor
Connector 39: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust
Connector 40: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake
Connector 41: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust
Connector 42: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake
Connector 43: | Camshaft Position (CMP) Sensor - Bank 1 Exhaust
Connector 44: | Camshaft Position (CMP) Sensor - Bank 1 Intake
Connector 45: | Camshaft Position (CMP) Sensor - Bank 2 Exhaust
Connector 46: | Camshaft Position (CMP) Sensor - Bank 2 Intake
Connector 47: | Cargo Lamp
Connector 48: | Cellular Telephone Microphone (UE1)
Connector 49: | Center High Mounted Stop Lamp (CHMSL)
Connector 50: | Cigar Lighter
Connector 51: | Crankshaft Position (CKP) Sensor
Connector 52: | Data Link Connector (DLC)
Connector 53: | Data Link Resistor (without MH6)
Connector 54: | Digital Radio Receiver (U2K)
Connector 55: | Dome Lamp (UUC)
Connector 56: | Dome Lamp (without UUC)
Connector 57: | Dome Lamp Switch (UUC)
Connector 58: | Door Latch - Driver
Connector 59: | Door Latch - Left Rear
Connector 60: | Door Latch - Passenger
Connector 61: | Door Latch - Right Rear
Connector 62: | Door Lock Switch - Driver
Connector 63: | Door Lock Switch - Passenger
Connector 64: | Driver Information Center (DIC) Switch
Connector 65: | Electronic Brake Control Module (EBCM)
Connector 66: | Electronic Compass Module (U80)
Connector 67: | Engine Control Module (ECM) X1
Connector 68: | Engine Control Module (ECM) X2
Connector 69: | Engine Coolant Temperature (ECT) Sensor
Connector 70: | Engine Cooling Fan - Left
Connector 71: | Engine Cooling Fan - Right
Connector 72: | Engine Oil Pressure (EOP) Switch
Connector 73: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 74: | Evaporative Emissions (EVAP) Canister Vent Solenoid Valve
Connector 75: | Evaporator Temperature Sensor
Connector 76: | Fog Lamp - Left Front (T96)
Connector 77: | Fog Lamp - Right Front (T96)
Connector 78: | Fuel Injector 1
Connector 79: | Fuel Injector 2
Connector 80: | Fuel Injector 3
Connector 81: | Fuel Injector 4
Connector 82: | Fuel Injector 5
Connector 83: | Fuel Injector 6
Connector 84: | Fuel Pump and Sender Assembly
Connector 85: | Fuel Tank Pressure (FTP) Sensor
Connector 86: | Generator X1
Connector 87: | Generator X2
Connector 88: | Hazard Switch
Connector 89: | Headlamp - Left
Connector 90: | Headlamp - Right
Connector 91: | Headlamp Dimmer Switch
Connector 92: | Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 1
Connector 93: | Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 2
Connector 94: | Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 1
Connector 95: | Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 2
Connector 96: | Heated Seat Control Module X1 (KA1)
Connector 97: | Heated Seat Control Module X2 (KA1)
Connector 98: | Heated Seat Control Module X3 (KA1)
Connector 99: | Heated Seat Control Module X4 (KA1)
Connector 100: | Heated Seat Element - Driver Back (KA1)
Connector 101: | Heated Seat Element - Driver Cushion (KA1)
Connector 102: | Heated Seat Element - Passenger Back (KA1)
Connector 103: | Heated Seat Element - Passenger Cushion (KA1)
Connector 104: | Hood Ajar Switch
Connector 105: | Horn
Connector 106: | Horn Switch
Connector 107: | HVAC Control Module X1
Connector 108: | HVAC Control Module X2
Connector 109: | HVAC Control Module X3
Connector 110: | HVAC Control Module X4 (C69)
Connector 111: | HVAC Control Module - Auxiliary (C69)
Connector 112: | Ignition Coil 1
Connector 113: | Ignition Coil 2
Connector 114: | Ignition Coil 3
Connector 115: | Ignition Coil 4
Connector 116: | Ignition Coil 5
Connector 117: | Ignition Coil 6
Connector 118: | Ignition Lock Cylinder Control Solenoid
Connector 119: | Ignition Switch
Connector 120: | Inflatable Restraint Front End Sensor - Left
Connector 121: | Inflatable Restraint Front End Sensor - Right
Connector 122: | Inflatable Restraint Front Passenger Presence System (PPS) Module
Connector 123: | Inflatable Restraint I/P Module X1
Connector 124: | Inflatable Restraint I/P Module X2
Connector 125: | Inflatable Restraint I/P Module Indicator
Connector 126: | Inflatable Restraint Roof Rail Module - Left (ASF)
Connector 127: | Inflatable Restraint Roof Rail Module - Right (ASF)
Connector 128: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 129: | Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)
Connector 130: | Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)
Connector 131: | Inflatable Restraint Steering Wheel Module X1
Connector 132: | Inflatable Restraint Steering Wheel Module X2
Connector 133: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 134: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 135: | Inflatable Restraint Steering Wheel Module Coil X3
Connector 136: | Inflatable Restraint Vehicle Rollover Sensor (ASF)
Connector 137: | Infrared Transmitter (UUC)
Connector 138: | Input Speed Sensor (ISS)
Connector 139: | Inside Air Temperature Sensor
Connector 140: | Inside Rearview Mirror (ISRVM)
Connector 141: | Instrument Panel Cluster (IPC)
Connector 142: | Knock Sensor (KS) 1
Connector 143: | Knock Sensor (KS) 2
Connector 144: | License Lamp - Left
Connector 145: | License Lamp - Right
Connector 146: | Liftgate Latch
Connector 147: | Liftgate Release Switch
Connector 148: | Marker Lamp - Left Front
Connector 149: | Marker Lamp - Right Front
Connector 150: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 151: | Mode Actuator
Connector 152: | Mode Actuator - Auxiliary (C69)
Connector 153: | Noise Compensation Microphone (U3U)
Connector 154: | Output Speed Sensor (OSS)
Connector 155: | Outside Rearview Mirror - Driver (DK2)
Connector 156: | Outside Rearview Mirror - Driver (without DK2)
Connector 157: | Outside Rearview Mirror - Passenger (DK2)
Connector 158: | Outside Rearview Mirror - Passenger (without DK2)
Connector 159: | Outside Rearview Mirror Switch
Connector 160: | Overhead Console Courtesy/Reading Lamp
Connector 161: | Park Brake Switch
Connector 162: | Park Lamp - Left Front
Connector 163: | Park Lamp - Right Front
Connector 164: | Park Position Switch
Connector 165: | Park/Turn Signal Lamp - Left Front
Connector 166: | Park/Turn Signal Lamp - Left Rear
Connector 167: | Park/Turn Signal Lamp - Right Front
Connector 168: | Park/Turn Signal Lamp - Right Rear
Connector 169: | Pressure Control (PC) Solenoid Valve
Connector 170: | Radio X1
Connector 171: | Radio X2
Connector 172: | Radio X3 (UUC)
Connector 173: | Radio X4 (U3U)
Connector 174: | Rear Differential Clutch Control Module X1 (MH6)
Connector 175: | Rear Differential Clutch Control Module X2 (MH6)
Connector 176: | Rear Wheel Drive Module Clutch (MH6)
Connector 177: | Rear Window Defogger Grid X1
Connector 178: | Rear Window Defogger Grid X2
Connector 179: | Rear Window Wiper Motor
Connector 180: | Rear Window Wiper/Washer/Fog Lamp Switch
Connector 181: | Recirculation Actuator
Connector 182: | Remote Control Door Lock Receiver (RCDLR)
Connector 183: | Seat Adjuster Switch - Driver (AG1)
Connector 184: | Seat Belt Buckle - Driver
Connector 185: | Seat Belt Buckle - Passenger
Connector 186: | Seat Belt Pretensioner - Left
Connector 187: | Seat Belt Pretensioner - Right
Connector 188: | Seat Front Vertical Motor - Driver (AG1)
Connector 189: | Seat Rear Vertical Motor - Driver (AG1)
Connector 190: | Shift Pressure Control (PC) Solenoid Valve
Connector 191: | Shift Solenoid (SS) Valve 1
Connector 192: | Shift Solenoid (SS) Valve 2
Connector 193: | Shift Solenoid (SS) Valve 3
Connector 194: | Shift Solenoid (SS) Valve 4
Connector 195: | Shift Solenoid (SS) Valve 5
Connector 196: | Speaker - Left Front
Connector 197: | Speaker - Left Front Tweeter
Connector 198: | Speaker - Left Rear
Connector 199: | Speaker - Right Front
Connector 200: | Speaker - Right Front Tweeter
Connector 201: | Speaker - Right Rear
Connector 202: | Speaker - Subwoofer (U65)
Connector 203: | Starter Motor X1
Connector 204: | Starter Motor X2 (Battery Positive Cable)
Connector 205: | Starter Motor X2 (Engine)
Connector 206: | Steering Angle Sensor
Connector 207: | Steering Wheel Control Switch - Left (K34)
Connector 208: | Steering Wheel Control Switch - Right (UK3)
Connector 209: | Sunroof Control Module (CF5)
Connector 210: | Sunroof Switch (CF5)
Connector 211: | Tail/Stop Lamp - Left
Connector 212: | Tail/Stop Lamp - Right
Connector 213: | Theft Deterrent Module (TDM)
Connector 214: | Throttle Body
Connector 215: | Torque Converter Clutch (TCC) Solenoid Valve
Connector 216: | Traction Control Switch (TCS)
Connector 217: | Transmission Control Module (TCM) X1
Connector 218: | Transmission Control Module (TCM) X2
Connector 219: | Transmission Control Module (TCM) X3
Connector 220: | Turn Signal/Multifunction Switch X1
Connector 221: | Turn Signal/Multifunction Switch X2
Connector 222: | Video Display (UUC)
Connector 223: | Wheel Speed Sensor (WSS) - Left Front
Connector 224: | Wheel Speed Sensor (WSS) - Left Rear
Connector 225: | Wheel Speed Sensor (WSS) - Right Front
Connector 226: | Wheel Speed Sensor (WSS) - Right Rear
Connector 227: | Window Motor - Driver
Connector 228: | Window Motor - Left Rear
Connector 229: | Window Motor - Passenger
Connector 230: | Window Motor - Right Rear
Connector 231: | Window Switch - Driver
Connector 232: | Window Switch - Left Rear
Connector 233: | Window Switch - Passenger
Connector 234: | Window Switch - Right Rear
Connector 235: | Windshield Washer Fluid Pump
Connector 236: | Windshield Wiper Motor
Connector 237: | Windshield Wiper/Washer Switch
Connector 238: | Yaw and Lateral Accelerometer Sensor

### A/C Compressor Clutch

#### Connector Part Information

- OEM: 7283-5448
- Service: 89046838
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### A/C Compressor Clutch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 59 | A/C Compressor Clutch Control
2 | 0.5 BK | 150 | Ground

### A/C Refrigerant Pressure Sensor

#### Connector Part Information

- OEM: 12110192
- Service: 88988301
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12103881/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12180559-1/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 5514 | Low Reference
B | 0.5 GY | 2700 | 5-Volt Reference
C | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15326829
- Service: 88988944
- Description: 6-Way F 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | Accelerator Pedal Position (APP) Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | Accelerator Pedal Position (APP) Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference

### Accessory Power Outlet - Center Console 1

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Center Console 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 650 | Ground

### Accessory Power Outlet - Center Console 2

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Center Console 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 650 | Ground

### Accessory Power Outlet - Rear

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 850 | Ground

### Air Temperature Actuator

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
3 | 0.35 GY | 598 | 5-Volt Reference
4 | 0.35 L-BU | 1316 | Air Temperature Door Control
5 | 0.35 D-BU | 1199 | Air Temperature Door Control

### Air Temperature Actuator - Auxiliary (C69)

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Actuator - Auxiliary (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY/BK | 1798 | Ground
2 | 0.35 PK | 2145 | Air Temperature Switch Signal - Right
3 | 0.35 GY | 596 | 5-Volt Reference
4 | 0.35 BN | 6555 | Rear Temperature Motor Control
5 | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control

### Air Temperature Sensor - Lower

#### Connector Part Information

- OEM: 15380927
- Service: See Catalog
- Description: 2-Way F Timer Micro II Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Sensor - Lower

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal
2 | 0.35 YE | 61 | Low Reference

### Air Temperature Sensor - Upper

#### Connector Part Information

- OEM: 15380927
- Service: See Catalog
- Description: 2-Way F Timer Micro II Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Sensor - Upper

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal
2 | 0.35 YE | 61 | Low Reference

### Ambient Air Temperature Sensor

#### Connector Part Information

- OEM: 12052642
- Service: 12101856
- Description: 2-Way F Metri-Pack 150 Series, Sealed (L-GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ambient Air Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
B | 0.35 YE | 61 | Low Reference

### Ambient Light Sensor

#### Connector Part Information

- OEM: 12064760
- Service: 12085208
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ambient Light Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU/BK | 590 | Driver Sunload Sensor Signal
B | 0.35 GY | 1548 | Passenger Sunload Sensor Signal
C | 0.35 BK/WH | 1551 | Ground
D | 0.35 L-GN/BK | 1137 | Daytime Running Lamp (DRL) Ambient Light Sensor Signal

### Audio Amplifier X1 (U65)

#### Connector Part Information

- OEM: 6098-4713
- Service: 88988652
- Description: 8-Way F 2.8 Series (BK)

#### Terminal Part Information

- Pins: 1-4
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 5, 8
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Audio Amplifier X1 (U65)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 L-GN/BK | 1794 | Subwoofer Speaker Coil 2 Output (-)
2 | 1.0 D-BU/WH | 346 | Subwoofer Speaker Coil 2 Output (+)
3 | 1.0 D-GN | 1795 | Subwoofer Speaker Coil 1 Output (+)
4 | 1.0 L-BU/BK | 315 | Subwoofer Speaker Coil 1 Output (-)
5 | 2.0 BK | 850 | Ground
6-7 | -- | -- | Not Used
8 | 2.0 RD/WH | 2040 | Battery Positive Voltage

### Audio Amplifier X2 (U65)

#### Connector Part Information

- OEM: 7283-5534-60
- Service: 89047090
- Description: 16-Way M YESC/USCAR Class II Sealed Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Audio Amplifier X2 (U65)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 YE | 116 | Left Rear Speaker Output (-)
2 | 0.8 BN | 199 | Left Rear Speaker Output (+)
3 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
4 | 0.8 L-BU | 115 | Right Rear Speaker Output (-)
5-8 | -- | -- | Not Used
9 | 0.8 D-GN | 117 | Right Front Speaker Output (-)
10 | 0.8 L-GN | 200 | Right Front Speaker Output (+)
11 | 0.8 TN | 201 | Left Front Speaker Output (+)
12 | 0.8 GY | 118 | Left Front Speaker Output (-)
13-16 | -- | -- | Not Used

### Audio Amplifier X3 (U65)

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F 0.64 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Audio Amplifier X3 (U65)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 1999 | Left Rear Low Level Audio Signal (-)
2 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-)
3 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+)
4 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+)
5-7 | -- | -- | Not Used
8 | 0.5 WH | 1487 | Antenna Enable Signal
9 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
10 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
11 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
12 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
13-15 | -- | -- | Not Used
16 | 0.5 OG | 5748 | Radio Audio Mute Signal

### Audio/Video Adapter (UUC)

#### Connector Part Information

- OEM: 15480082
- Service: 19149303
- Description: 8-Way F Micro 64 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Audio/Video Adapter (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BARE | 5346 | Drain Wire
2 | -- | -- | Not Used
3 | 0.5 PU | 2056 | Auxiliary Video High Signal
4 | -- | -- | Not Used
5 | 0.5 WH | 2058 | Auxiliary Audio Right Signal
6 | 0.5 YE | 2059 | Auxiliary Audio Left Signal
7 | 0.5 BARE | 5345 | Video Drain Wire
8 | -- | -- | Not Used

### Automatic Transmission Fluid Temperature (TFT) Sensor

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2-Way M (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Fluid Temperature (TFT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | -- | Transmission Fluid Temperature Sensor Signal
2 | 0.35 OG | -- | Low Reference

### Automatic Transmission Shift Lock Control Solenoid

#### Connector Part Information

- OEM: 90000223
- Service: See Catalog
- Description: 3-Way F (WH)

#### Automatic Transmission Shift Lock Control Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN/WH | 1135 | Automatic Transmission Shift Lock Control Solenoid Control
2 | -- | -- | Not Used
3 | 0.35 BK | 1450 | Ground

### Backup Lamp - Left

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-GN | 24 | Backup Lamp Control
2 | 0.5 BK | 550 | Ground

### Backup Lamp - Right

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-GN | 24 | Backup Lamp Control
2 | 0.8 BK | 850 | Ground

### Battery (-)

#### Terminal Part Information

- Terminal/Tray: 7106-2036
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (-)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
- | 32 BK | 50 | Ground
19 BK | 50 | Ground
8 BK | 50 | Ground

### Battery (+)

#### Terminal Part Information

- Terminal/Tray: 7106-2035
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (+)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 32 RD | 1 | Battery Positive Voltage
19 RD | 1 | Battery Positive Voltage

### Battery Current Sensor

#### Connector Part Information

- OEM: 13519047
- Service: See Catalog
- Description: 3-Way F GT 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Battery Current Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 5076 | 5-Volt Reference
B | 0.35 BN | 5077 | Low Reference
C | 0.35WH | 5075 | Current Sensor Signal

### Blower Motor

#### Connector Part Information

- OEM: 15226103
- Service: 88988507
- Description: 2-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 BK | 2150 | Ground
2 | 3.0 PU | 65 | Blower Motor Control

### Blower Motor - Auxiliary (C69)

#### Connector Part Information

- OEM: 10846816
- Service: 88988507
- Description: 2-Way F 6.3 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor - Auxiliary (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 OG | 5988 | Low Reference
2 | 2.0 PU | 65 | Blower Motor Control

### Blower Motor Control Module X1

#### Connector Part Information

- OEM: 15226103
- Service: 88988507
- Description: 2-Way F (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Blower Motor Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 PU | 65 | Blower Motor Control
2 | 3.0 BK | 2150 | Ground

### Blower Motor Control Module X2

#### Connector Part Information

- OEM: 7283-9749-30
- Service: See Catalog
- Description: 6-Way F YESC Kaizen series (BK)

#### Terminal Part Information

- Pins: 3
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 5, 6
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Blower Motor Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 GY/BK | 754 | Blower Motor Speed Control
4 | -- | -- | Not Used
5 | 3.0 BK | 1450 | Ground
6 | 3.0 RD/BK | 442 | Battery Positive Voltage

### Blower Motor Control Module - Auxiliary X1 (C69)

#### Connector Part Information

- OEM: 10846816
- Service: 88988507
- Description: 2-Way F 6.3 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor Control Module - Auxiliary X1 (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 PU | 65 | Blower Motor Control
2 | 2.0 OG | 5988 | Low Reference

### Blower Motor Control Module - Auxiliary X2 (C69)

#### Connector Part Information

- OEM: 13520671
- Service: See Catalog
- Description: 6-Way F GT 150 6.3 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor Control Module - Auxiliary X2 (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 D-GN | 2211 | Auxiliary Blower Motor Speed Control
4 | -- | -- | Not Used
5 | 2.0 BK | 550 | Ground
6 | 2.0 RD/WH | 2640 | Battery Positive Voltage

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: HITPB-27-AL-M
- Service: 88988838
- Description: 27-Way F 0.64 Unsealed (L-GN)

#### Terminal Part Information

- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35WH | 1390 | Ignition Voltage
3 | 0.35 GY | 1884 | Cruise Control Switch Signal
4 | 0.35WH/BK | 1073 | Ignition Key Resistor Signal
5 | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
6 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
7 | -- | -- | Not Used
8 | 0.35 BK/WH | 1251 | Ground
9 | 0.35 L-BU | 1714 | Windshield Wiper Switch Low Signal
10-13 | -- | -- | Not Used
14 | 0.35 PK | 3 | Ignition Voltage
15 | 0.35 L-BU/WH | 1414 | Left Turn Signal Switch Signal
16 | 0.35 D-BU/WH | 1415 | Right Turn Signal Switch Signal
17 | 0.35 PU | 1375 | 12-Volt Reference
18 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
19 | 0.35 TN | 2144 | Hazard Switch Signal
20 | 0.35 PU | 5526 | Tap Up/Tap Down Switch Signal
21 | 0.35 BN | 4 | Ignition Voltage
22-23 | -- | -- | Not Used
24 | 0.35 PK | 94 | Rear Wiper Switch Signal
25 | 0.35 BN | 1356 | Flash To Pass Switch Signal
26 | 0.35 D-GN/WH | 1135 | Automatic Transmission Shift Lock Control Solenoid Control
27 | -- | -- | Not Used

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: HITPB-25-B-S
- Service: 88988839
- Description: 25-Way F Receptacle 0.64 2.8 Unsealed (WH)

#### Terminal Part Information

- Pins: 1-3
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

- Pins: 8, 11-12, 17, 21
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 OG | 1732 | Inadvertent Power Control
2 | 0.8 RD/WH | 1240 | Battery Positive Voltage
3 | 0.8 GY | 8 | Instrument Panel Lamp Control
4-7 | -- | -- | Not Used
8 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
9-10 | -- | -- | Not Used
11 | 0.35 L-GN/BK | 1137 | Daytime Running Lamp (DRL) Ambient Light Sensor Signal
12 | 0.35 WH | 103 | Headlamp Switch On Signal
13-16 | -- | -- | Not Used
17 | 0.35 D-GN | 306 | Headlamp Switch OFF Signal
18-20 | -- | -- | Not Used
21 | 0.35 L-BU | 1788 | Traction Control Switch Signal
22 | 0.35 PU/WH | 5905 | Key Capture/Column Lock Shift Position Signal
23-25 | -- | -- | Not Used

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: HITPB-25-C-LE
- Service: 88988840
- Description: 25-Way F HIT Series (L-BU)

#### Terminal Part Information

- Pins: 1-3, 5
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

- Pins: 7-19, 21-22
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 1551 | Ground
2 | 0.8 RD/WH | 240 | Battery Positive Voltage
3 | 0.8 RD/WH | 1040 | Battery Positive Voltage
4 | -- | -- | Not Used
5 | 0.8 BK/WH | 1551 | Ground
6 | -- | -- | Not Used
7 | 0.35 YE | 749 | Security Indicator Control
8 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
9 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
10 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
11 | 0.35 D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal
12 | 0.35 OG/WH | 812 | 12-Volt Reference
13 | 0.5 D-BU | 6037 | Brake Pedal Position Sensor Signal
14 | 0.5 OG/BK | 6035 | Low Reference
15 | 0.5 GY | 6036 | 5-Volt Reference
16 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
17 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
18 | 0.5 PU/WH | 1382 | LED Dimming Supply
19 | 0.35 L-BU | 5986 | Serial Data Communication Enable
20 | -- | -- | Not Used
21 | 0.35 OG | 192 | Front Fog Lamp Switch Signal
22 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
23-25 | -- | -- | Not Used

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: HITPB-25-D-K
- Service: 88988841
- Description: 25-Way F Receptacle 0.64 2.8 (BK)

#### Terminal Part Information

- Pins: 1-5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 7, 9-13, 15-17, 19, 21-23
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 RD/WH | 340 | Battery Positive Voltage
2 | 0.8 RD/WH | 240 | Battery Positive Voltage
3 | 0.8 RD/WH | 440 | Battery Positive Voltage
4 | 0.8 RD/WH | 1240 | Battery Positive Voltage
5 | 0.8 D-BU/WH | 1315 | Right Front Turn Signal Lamp Control
6 | -- | -- | Not Used
7 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
8 | -- | -- | Not Used
9 | 0.5 BK | 50 | Ground
10 | 0.35 RD/WH | 2440 | Battery Positive Voltage
11 | 0.35 D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
12 | 0.5 YE | 5187 | Right Trailer Turn Signal Lamp (V92)
13 | 0.5 OG | 5186 | Left Trailer Turn Signal Lamp (V92)
14 | -- | -- | Not Used
15 | 0.35 OG | 2268 | Windshield Washer Relay Control
16 | 0.35 TN/WH | 1969 | Headlamp High Beam Relay Control
17 | 0.35 PK/BK | 109 | Hood Ajar Switch Signal (AP3)
18 | -- | -- | Not Used
19 | 0.35 BN | 4 | Ignition Voltage
20 | -- | -- | Not Used
21 | 0.35 PK | 1439 | Ignition Voltage
22 | 0.35 YE | 5704 | Liftgate Latch Relay Coil Control
23 | 0.35 PU | 544 | DRL Relay Control
24-25 | -- | -- | Not Used

### Body Control Module (BCM) X5

#### Connector Part Information

- OEM: HITPB-25-E-N
- Service: 88988837
- Description: 25-Wat F Receptacle Unsealed 0.64 2.8 (BN)

#### Terminal Part Information

- Pins: 1-2, 4-5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 6, 8-10, 11, 14-16, 18, 20-21, 23-24
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 YE | 18 | Left Rear Stop/Turn Lamp Control
2 | 0.8 D-GN | 19 | Right Rear Stop/Turn Lamp Control
3 | -- | -- | Not Used
4 | 0.8 L-BU/WH | 1314 | Left Front Turn Signal Lamp Control
5 | 0.8 L-BU | 1320 | Center High Mounted Stop Lamp (CHMSL) Control
6 | 0.5 WH | 17 | Stop Lamp Switch Signal
7 | -- | -- | Not Used
8 | 0.35 PK | 5076 | 5-Volt Reference
9 | 0.35 WH | 5075 | Current Sensor Signal
10 | 0.35 BN | 5077 | Low Reference
11 | 0.35 TN | 707 | RAP Relay Coil Control
12-13 | -- | -- | Not Used
14 | 0.5 YE | 243 | Ignition Voltage
15 | 0.35 PU | 5531 | Hood Closed Switch Signal (AP3)
16 | 0.5 OG/BK | 233 | Park Brake Switch Signal
17 | -- | -- | Not Used
18 | 0.35 TN | 28 | Horn Relay Control
19 | -- | -- | Not Used
20 | 0.35 GY | 91 | Windshield Wiper Switch Signal 2
21 | 0.35 TN | 860 | Front Windshield Wiper Switch High Signal
22 | -- | -- | Not Used
23 | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
24 | 0.35 WH | 1080 | Park Lamp Relay Control
25 | -- | -- | Not Used

### Body Control Module (BCM) X6

#### Connector Part Information

- OEM: HITPB-25-F-PK
- Service: 88988842
- Description: 25-WAY F Receptacle Unsealed 0.64 2.8 (PK)

#### Terminal Part Information

- Pins: 1-2
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 8-10, 12, 15, 18
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-BU/WH | 149 | Courtesy Lamp Control
2 | 0.8 L-GN | 24 | Backup Lamp Control
3-7 | -- | -- | Not Used
8 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
9 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Signal
10 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
11 | -- | -- | Not Used
12 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal
13-14 | -- | -- | Not Used
15 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal
16-17 | -- | -- | Not Used
18 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Signal
19-25 | -- | -- | Not Used

### Body Control Module (BCM) X7

#### Connector Part Information

- OEM: HITPB-28-G-H
- Service: 88988806
- Description: 28-Way F Receptacle 0.64 (GY)

#### Terminal Part Information

- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X7

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 YE | 356 | Driver Door Lock Relay Unlock Control
7 | 0.35 L-GN | 1391 | Driver Door Unlock Relay Control
8 | -- | -- | Not Used
9 | 0.35 L-BU | 5921 | Driver Door Unlock Relay Control
10 | -- | -- | Not Used
11 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal
12 | 0.35 PK/BK | 780 | Driver Door Lock Switch Lock Signal
13 | 0.35 D-GN | 5706 | Liftgate Latch Relay Control
14-28 | -- | -- | Not Used

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 12162195
- Service: 88987993
- Description: 2-Way F Metri-Pack 150.2 Series, Sealed, Pull To Seat (BK)

#### Terminal Part Information

- Terminal/Tray: 12124075/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12180559-1/J-35616-2A (GY)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | 0.35 TN/WH | 33 | Brake Warning Indicator Control

### Brake Pedal Position Sensor

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Brake Pedal Position Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 6035 | Low Reference
B | 0.5 D-BU | 6037 | Brake Pedal Position Sensor Signal
C | 0.5 GY | 6036 | 5-Volt Reference

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust

#### Connector Part Information

- OEM: 7283-7526-30
- Service: 88988588
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PK/BK | 5293 | Ignition Voltage
2 | 0.8 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid - 1

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake

#### Connector Part Information

- OEM: 7283-7526-30
- Service: 88988588
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PK/BK | 5293 | Ignition Voltage
2 | 0.8 PU | 5284 | Camshaft Phaser Intake Solenoid - 1

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust

#### Connector Part Information

- OEM: 7283-7526-30
- Service: 88988588
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PK/BK | 5293 | Ignition Voltage
2 | 0.8 WH/BK | 5283 | Camshaft Phaser Exhaust Solenoid - 2

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake

#### Connector Part Information

- OEM: 7283-7526-30
- Service: 88988588
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PK/BK | 5293 | Ignition Voltage
2 | 0.8 OG/BK | 5272 | Camshaft Phaser Intake Solenoid - 2

### Camshaft Position (CMP) Sensor - Bank 1 Exhaust

#### Connector Part Information

- OEM: 1928403968
- Service: 88988595
- Description: 3-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-4A (PU)

#### Camshaft Position (CMP) Sensor - Bank 1 Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor - 1
3 | 0.5 GY | 705 | 5-Volt Reference

### Camshaft Position (CMP) Sensor - Bank 1 Intake

#### Connector Part Information

- OEM: 1928403968
- Service: 88988595
- Description: 3-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-4A (PU)

#### Camshaft Position (CMP) Sensor - Bank 1 Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 OG | 5275 | Camshaft Position Intake Sensor - 1
3 | 0.5 GY | 705 | 5-Volt Reference

### Camshaft Position (CMP) Sensor - Bank 2 Exhaust

#### Connector Part Information

- OEM: 1928403968
- Service: 88988595
- Description: 3-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-4A (PU)

#### Camshaft Position (CMP) Sensor - Bank 2 Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 PU | 5274 | Camshaft Position Exhaust Sensor - 2
3 | 0.5 GY | 705 | 5-Volt Reference

### Camshaft Position (CMP) Sensor - Bank 2 Intake

#### Connector Part Information

- OEM: 1928403968
- Service: 88988595
- Description: 3-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616- 4A (PU)

#### Camshaft Position (CMP) Sensor - Bank 2 Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 YE | 5276 | Camshaft Position Intake Sensor - 2
3 | 0.5 GY | 705 | 5-Volt Reference

### Cargo Lamp

#### Connector Part Information

- OEM: 12045813
- Service: 12101889
- Description: 4-Way F Metri-pack 150 Series (CM)

#### Cargo Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.8 GY | 157 | Courtesy Lamp Control
C | -- | -- | Not Used
D | 0.8 BK | 850 | Ground

### Cellular Telephone Microphone (UE1)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Cellular Telephone Microphone (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 1489 | Drain Wire
B | 0.5 GY | 655 | Cellular Microphone Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: 7223-1324
- Service: 88988460
- Description: 2-Way F 090 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 7116-1420/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 1320 | Center High Mounted Stop Lamp (CHMSL) Control
2 | 0.5 BK | 850 | Ground

### Cigar Lighter

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Cigar Lighter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 650 | Ground

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 89047365
- Service: 88988337
- Description: 3-Way F Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 452 | Low Reference
2 | 0.5 YE | 573 | Crankshaft Position Sensor (CKP) 1 Signal
3 | 0.5 GY | 605 | 5-Volt Reference

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 348822-2
- Service: 89046778
- Description: 16-Way F Diagnostic Connector (BK)

#### Terminal Part Information

- Terminal/Tray: 776001-1/16
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | 0.5 BK | 1450 | Ground
5 | 0.35 BK/WH | 1551 | Ground
6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
7-13 | -- | -- | Not Used
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | -- | -- | Not Used
16 | 0.35 RD/WH | 1840 | Battery Positive Voltage

### Data Link Resistor (without MH6)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Data Link Resistor (without MH6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
B | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM: 15394150
- Service: See Catalog
- Description: 16-Way F Micro 64 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 372 | Remote Radio Audio Output (-)
2 | 0.5 BN/WH | 367 | Remote Radio Left Audio Signal (+)
3 | 0.5 D-GN/WH | 368 | Remote Radio Right Audio Signal (+)
4 | 0.5 GY | 388 | Remote Radio Right Audio Signal (-)
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-8 | -- | -- | Not Used
9 | 0.5 BK/WH | 651 | Ground
10 | -- | -- | Not Used
11 | 0.35 GY | 6759 | Discrete Audio Drain Wire
12-15 | -- | -- | Not Used
16 | 0.5 RD/WH | 2340 | Battery Positive Voltage

### Dome Lamp (UUC)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Dome Lamp (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 1732 | Courtesy Lamp Control
B | 0.8 BK | 850 | Ground
C | 0.8 GY | 157 | Courtesy Lamp Control

### Dome Lamp (without UUC)

#### Connector Part Information

- OEM: 12045813
- Service: 12101889
- Description: 4-Way F Metri-pack 150 Series (CM)

#### Dome Lamp (without UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 YE | 149 | Courtesy Lamp Control
B | 0.8 GY | 157 | Courtesy Lamp Control
C | 0.8 OG | 1732 | Courtesy Lamp Control
D | 0.8 BK | 850 | Ground

### Dome Lamp Switch (UUC)

#### Connector Part Information

- OEM: 12047782
- Service: 12117371
- Description: 3-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Dome Lamp Switch (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-BU/WH | 149 | Courtesy Lamp Control
B | 0.8 GY | 157 | Courtesy Lamp Control
C | 0.8 OG | 1732 | Courtesy Lamp Control

### Door Latch - Driver

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
2 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 1.0 GY | 295 | Door Lock Actuator Lock Control
4 | 0.5 RD/BK | 745 | Left Front Door Ajar Switch Signal
5 | 1.0 PU | 294 | Door Lock Actuator Unlock Control
6 | 0.35 BK | 651 | Ground

### Door Latch - Left Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
2 | 1.0 TN | 294 | Door Lock Actuator Unlock Control
3 | 1.0 GY | 295 | Door Lock Actuator Lock Control
4 | 0.5 RD/BK | 746 | Right Front Door Ajar Switch Signal
5 | 0.35 PU | 294 | Door Lock Actuator Unlock Control
6 | 0.35 BK | 651 | Ground

### Door Latch - Passenger

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
2 | 0.35 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 0.35 GY | 651 | Ground
4 | 0.35 RD/BK | 745 | Left Front Door Ajar Switch Signal
5 | 0.35 PU | 294 | Door Lock Actuator Unlock Control
6 | 0.35 BK | 295 | Door Lock Actuator Lock Control

### Door Latch - Right Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 746 | Right Front Door Ajar Switch Signal
2 | 0.35 PU | 294 | Door Lock Actuator Unlock Control
3 | 0.35 GY | 651 | Ground
4 | 0.5 RD/BK | 746 | Right Front Door Ajar Switch Signal
5 | 1.0 PU | 294 | Door Lock Actuator Unlock Control
6 | 1.0 BK | 295 | Door Lock Actuator Lock Control

### Door Lock Switch - Driver

#### Connector Part Information

- OEM: 6098-0241
- Service: See Catalog
- Description: 3-Way F HD 090 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Lock Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/BK | 780 | Driver Door Lock Switch Lock Signal
2 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal
3 | 0.35 OG | 651 | Ground

### Door Lock Switch - Passenger

#### Connector Part Information

- OEM: 6098-0241
- Service: See Catalog
- Description: 3-Way F HD 090 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Lock Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/BK | 244 | Passenger Door Lock Switch Lock Signal
2 | 0.35 OG/BK | 245 | Passenger Door Lock Switch Unlock Signal
3 | 0.35 OG | 651 | Ground

### Driver Information Center (DIC) Switch

#### Connector Part Information

- OEM: HCMPB-A05-K
- Service: 88988747
- Description: 5-Way F HCM Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Driver Information Center (DIC) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN/WH | 1358 | Driver Information Center (DIC) Switch Signal
2 | 0.5 BN | 897 | Low Reference
3 | 0.5 PK | 893 | Driver Information Center (DIC) Select Menu Switch Signal
4 | 0.35 PU/WH | 1382 | LED Dimming Supply
5 | 0.35 BK | 1450 | Ground

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 7-1355628-6
- Service: See Catalog
- Description: 47-Way F MK25/60 Series (BK)

#### Terminal Part Information

- Pins: 32
- Terminal/Tray: 7116-4141-02/10
- Core/Insulation Crimp: 4/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 1, 16
- Terminal/Tray: 7116-4142-02/10
- Core/Insulation Crimp: Pins 1 - A/3
- Core/Insulation Crimp: Pins 16 - D/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 3-4, 8, 11-14, 18-19, 22, 29, 33-34, 36-37, 42-43, 45
- Terminal/Tray: 638551-1/16
- Core/Insulation Crimp: Pins: 3, 11-14, 18-19, 22, 29, 33-34, 36-37, 42-43, 45-96 - K/K
- Core/Insulation Crimp: Pins 8 - J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Electronic Brake Control Module (EBCM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 RD/BK | 142 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal
4-7 | -- | -- | Not Used
8 | 0.35 L-BU | 5986 | Serial Data Communication Enable
9-10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
13 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | -- | -- | Not Used
16 | 5.0 BK | 250 | Ground
17 | -- | -- | Not Used
18 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
19 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
20-21 | -- | -- | Not Used
22 | 0.5 GY | 6044 | 12-Volt Reference
23-28 | -- | -- | Not Used
29 | 0.5 OG/BK | 6045 | Low Reference
30-31 | -- | -- | Not Used
32 | 2.0 RD/WH | 140 | Battery Positive Voltage
33 | 0.5 TN | 833 | Low Reference
34 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
35 | -- | -- | Not Used
36 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
37 | 0.5 OG | 885 | Low Reference
38-41 | -- | -- | Not Used
42 | 0.5 WH | 883 | Low Reference
43 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
44 | -- | -- | Not Used
45 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal
46 | 0.5 YE | 873 | Low Reference
47 | -- | -- | Not Used

### Electronic Compass Module (U80)

#### Connector Part Information

- OEM: 13541539
- Service: See Catalog
- Description: 4-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Electronic Compass Module (U80)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 643 | Ignition Voltage
2 | 0.35 BK | 850 | Ground
3 | 0.35 D-GN | 6134 | Local Interconnect Network 3
4 | -- | -- | Not Used

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM: 1928404927
- Service: See Catalog
- Description: 96-Way F 1.2 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid - 1
2 | 0.8 PU | 5284 | Camshaft Phaser Intake Solenoid - 1
3 | -- | -- | Not Used
4 | 0.8 YE/BK | 846 | Fuel Injector 6 Control
5 | 0.8 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
6 | -- | -- | Not Used
7 | 0.5 OG | 5275 | Camshaft Position Intake Sensor - 1
8 | -- | -- | Not Used
9 | 0.5 PU | 5274 | Camshaft Position Exhaust Sensor - 2
10 | 0.5 OG | 225 | Generator Turn On Signal
11-12 | -- | -- | Not Used
13 | 0.5 BN/WH | 2130 | Low Reference
14 | -- | -- | Not Used
15 | 0.5 GY | 705 | 5-Volt Reference 2
16 | -- | -- | Not Used
17 | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
18-23 | -- | -- | Not Used
24 | 0.8 YE | 581 | Throttle Actuator Control Motor Control - 1
25 | 0.8 WH/BK | 5283 | Camshaft Phaser Exhaust Solenoid - 2
26 | 0.8 PK/BK | 1746 | Fuel Injector 3 Control
27 | -- | -- | Not Used
28 | 0.8 TN/WH | 845 | Fuel Injector 5 Control
29 | -- | -- | Not Used
30 | 0.5 GY | 23 | Generator Field Duty Cycle Signal
31-32 | -- | -- | Not Used
33 | 0.5 YE | 5276 | Camshaft Position Intake Sensor - 2
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor - 1
35 | 0.5 YE | 573 | Crankshaft Position Sensor (CKP) 1 Signal
36-38 | -- | -- | Not Used
39 | 0.5 GY | 2701 | 5-Volt Reference 3
40 | -- | -- | Not Used
41 | 0.5 TN | 552 | Low Reference
42 | -- | -- | Not Used
43 | 0.5 TN | 470 | Low Reference
44 | 0.5 TN | 2761 | Low Reference
45 | 0.5 GY | 605 | 5-Volt Reference 3
46 | 0.5 TN | 452 | Low Reference
47 | -- | -- | Not Used
48 | 0.8 BN | 582 | Throttle Actuator Control (TAC) Motor Control - 2
49 | 0.8 OG/BK | 5272 | Camshaft Phaser Intake Solenoid - 2
50 | 0.8 L-BU/BK | 844 | Fuel Injector 4 Control
51 | 0.8 TN | 1744 | Fuel Injector 1 Control
52 | 0.8 L-GN/BK | 1745 | Fuel Injector 2 Control
53-54 | -- | -- | Not Used
55 | 0.5 PU | 2121 | Ignition Control 1
56 | 0.5 L-BU | 2123 | Ignition Control 3
57 | 0.5 D-GN | 2125 | Ignition Control 5
58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | Knock Sensor 1 Signal
60 | 0.5 GY | 2303 | Knock Sensor 2 Signal
61-66 | -- | -- | Not Used
67 | 0.5 TN | 1664 | Heated Oxygen Sensor Low Signal - Bank 1 Sensor 1
68-69 | -- | -- | Not Used
70 | 0.5 PU | 1666 | Heated Oxygen Sensor High Signal - Bank 2 Sensor 1
71 | -- | -- | Not Used
72 | 0.5 L-GN | 3212 | Heated Oxygen Sensor Heater Low Control - Bank 2 Sensor 1
73-77 | -- | -- | Not Used
78 | 0.5 BN | 2129 | Low Reference
79 | 0.5 OG/WH | 2122 | Ignition Control 2
80 | 0.5 D-GN/WH | 2124 | Ignition Control 4
81 | 0.5 L-BU/WH | 2126 | Ignition Control 6
82 | 0.5 YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
83 | 0.5 GY | 1716 | Knock Sensor 1 Signal
84 | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
85-87 | -- | -- | Not Used
88 | 0.5 TN | 2752 | Low Reference
89 | 0.5 PU | 486 | Throttle Position Sensor 2 Signal
90 | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
91 | -- | -- | Not Used
92 | 0.5 PU/WH | 1665 | Heated Oxygen Sensor High Signal - Bank 1 Sensor 1
93 | 0.5 TN | 1667 | Heated Oxygen Sensor Low Signal - Bank 2 Sensor 1
94-95 | -- | -- | Not Used
96 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control - Bank 1 Sensor 1

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: 1928404916
- Service: 19115599
- Description: 58-Way F 2.8 Series Sealed (BK)

#### Terminal Part Information

- Pins: 1-2, 4-5
- Terminal/Tray: 1928498058/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616- 4A (PU)

- Pins: 7, 9, 10-15, 17, 19-20, 22-25, 27, 34-36, 38-39, 41-42, 44-52, 54-58
- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 451 | Ground
2 | 0.8 BK/WH | 451 | Ground
3 | -- | -- | Not Used
4 | 0.8 BK/WH | 451 | Ground
5 | 1.0 PK/BK | 5290 | Ignition Voltage
6 | -- | -- | Not Used
7 | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control - Bank 2 Sensor 1
8 | -- | -- | Not Used
9 | 0.5 TN | 2759 | Low Reference
10 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
11 | 0.5 TN | 5514 | Low Reference
12 | 0.5 BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
13 | 0.5 YE | 492 | Mass Air Flow (MAF) Sensor Signal
14 | 0.5 GY | 2709 | 5-Volt Reference 1
15 | 0.5 D-BU | 1161 | Accelerator Pedal Position (APP) Sensor 1 Signal
16 | -- | -- | Not Used
17 | 0.5 OG/BK | 1786 | Park/Neutral Signal
18 | -- | -- | Not Used
19 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
20 | 0.5 OG/WH | 3223 | Heated Oxygen Sensor Heater Low Control Bank 2 Sensor 2
21 | -- | -- | Not Used
22 | 0.5 TN | 2760 | Low Reference
23 | 0.5 TN/WH | 1669 | Heated Oxygen Sensor Low Signal - Bank 1 Sensor 2
24 | 0.5 TN | 1671 | Heated Oxygen Sensor Low Signal - Bank 2 Sensor 2
25 | 0.5 L-BU | 1162 | Accelerator Pedal Position (APP) Sensor 2 Signal
26 | -- | -- | Not Used
27 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
28-33 | -- | -- | Not Used
34 | 0.5 BN | 1271 | Low Reference
35 | 0.5 GY | 2700 | 5-Volt Reference 3
36 | 0.5 PU | 1589 | Fuel Level Sensor Signal
37 | -- | -- | Not Used
38 | 0.5 PU/WH | 1668 | Heated Oxygen Sensor High Signal - Bank 1 Sensor 2
39 | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
40 | -- | -- | Not Used
41 | 0.5 BN | 4 | Ignition Voltage
42 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
43 | -- | -- | Not Used
44 | 0.5 D-GN/WH | 459 | A/C Compressor Clutch Relay Control
45 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
46 | 0.5 D-GN | 335 | Low Speed Cooling Fan Relay Control
47 | 0.5 PU | 1272 | Low Reference
48 | 0.5 TN | 1274 | 5-Volt Reference 3
49 | 0.5 WH/BK | 1164 | 5-Volt Reference 2
50 | 0.5 TN | 472 | Intake Air Temperature (IAT) Sensor Signal
51 | 0.5 PU | 1670 | Heated Oxygen Sensor High Signal - Bank 2 Sensor 2
52 | 0.5 WH | 17 | Stop Lamp Switch Signal
53 | -- | -- | Not Used
54 | 0.5 PK | 439 | Ignition Voltage
55 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
56 | 0.5 RD/WH | 1540 | Battery Positive Voltage
57 | 0.5 YE | 447 | Starter Relay Coil Control
58 | 0.5 BN | 5069 | Engine Main Relay Coil Control

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 1928403874
- Service: 88988963
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498054/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616- 4A (PU)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 410 | Engine Coolant Temperature Sensor Signal
2 | 0.5 TN | 2761 | Low Reference

### Engine Cooling Fan - Left

#### Connector Part Information

- OEM: 7283-5596-10
- Service: 88953307
- Description: 2-Way F YESC/USCAR Class III (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Engine Cooling Fan - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 GY | 532 | Cooling Fan Motor Control
2 | 3.0 WH | 504 | Low Reference

### Engine Cooling Fan - Right

#### Connector Part Information

- OEM: 7283-5596-10
- Service: 88953307
- Description: 2-Way F YESC/USCAR Class III (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Engine Cooling Fan - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 L-BU | 409 | Cooling Fan Motor Control
2 | 3.0 BK | 1250 | Ground

### Engine Oil Pressure (EOP) Switch

#### Connector Part Information

- OEM: 12065400
- Service: 12126436
- Description: 4-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
B | 0.5 TN | 470 | Low Reference
C-D | -- | -- | Not Used

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 1928404072
- Service: 88988586
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-4A (PU)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PK/BK | 5293 | Ignition Voltage
2 | 0.8 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 2840 | Battery Positive Voltage
B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control

### Evaporator Temperature Sensor

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporator Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 2622 | Evaporator Temperature Sensor Signal
B | 0.35 TN | 552 | Low Reference

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Left Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Control
B | 0.5 BK | 1250 | Ground

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Right Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Control
B | 0.5 BK | 1250 | Ground

### Fuel Injector 1

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 TN | 1744 | Fuel Injector 1 Control

### Fuel Injector 2

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 3

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 4

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injector 5

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 TN/WH | 845 | Fuel Injector 5 Control

### Fuel Injector 6

#### Connector Part Information

- OEM: 15305086
- Service: 15306318
- Description: 2-Way F Metri-Pack Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 5291 | Ignition Voltage
B | 0.5 YE/BK | 846 | Fuel Injector 6 Control

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 12162210
- Service: 12167121
- Description: 6-Way F Metri-Pack 150.2 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 GY | 120 | Fuel Pump Control
B | 0.5 TN | 2759 | Low Reference
C | 0.5 PU | 30 | Fuel Level Sensor Signal
D | 0.35 PU | 1589 | Fuel Level Sensor Signal
E | 0.35 PU | 30 | Fuel Level Sensor Signal
F | 1.0 BK | 850 | Ground

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 13522407
- Service: See Catalog
- Description: 3-Way F 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.5 BK | 2759 | Low Reference
3 | 0.5 GY | 2709 | 5-Volt Reference

### Generator X1

#### Connector Part Information

- OEM: 12186308
- Service: 89046837
- Description: 2-Way F JPT Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Generator X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 225 | Generator Turn On Signal
2 | 0.5 GY | 23 | Generator Field Duty Cycle Signal

### Generator X2

#### Terminal Part Information

- Terminal: 12146365
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Generator X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 19 RD | 1 | Battery Positive Voltage

### Hazard Switch

#### Connector Part Information

- OEM: 7183-7201-80
- Service: See Catalog
- Description: 8-Way F (BN)

#### Terminal Part Information

- Pins: B, C, J
- Terminal/Tray: 8240-4412/22
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: I
- Terminal/Tray: 8240-4422/6
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 TN | 2144 | Hazard Switch Signal
C | 0.35 BK/WH | 1551 | Ground
D-H | -- | -- | Not Used
I | 0.8 GY | 8 | Instrument Panel Lamp Control
J | 0.35 BK | 1450 | Ground

### Headlamp - Left

#### Connector Part Information

- OEM: 15203303
- Service: See Catalog
- Description: 3-Way F Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 712 | Left Headlamp Low Beam Control
2 | 0.5 BK | 1250 | Ground
3 | 0.5 WH | 711 | Left Headlamp High Beam Control

### Headlamp - Right

#### Connector Part Information

- OEM: 15203303
- Service: See Catalog
- Description: 3-Way F Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 312 | Right Headlamp Low Beam Control
2 | 0.5 BK | 1250 | Ground
3 | 0.5 WH | 311 | Right Headlamp High Beam Control

### Headlamp Dimmer Switch

#### Connector Part Information

- OEM: 12020299
- Service: 12102566
- Description: 5-Way F P/C Edgeboard - Standard (CM)

#### Terminal Part Information

- Terminal/Tray: 12040511/3
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

#### Headlamp Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
C | 0.35 BK/WH | 1551 | Ground
D | 0.35 OG/WH | 812 | 12-Volt Reference
E | -- | -- | Not Used

### Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 1

#### Connector Part Information

- OEM: 12160482
- Service: 88988598
- Description: 4-Way F Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 1664 | Heated Oxygen Sensor Low Signal - Bank 1 Sensor 1
B | 0.5 PU/WH | 1665 | Heated Oxygen Sensor High Signal - Bank 1 Sensor 1
C | 0.5 PK/BK | 5293 | Ignition Voltage
D | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control - Bank 1 Sensor 1

### Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 2

#### Connector Part Information

- OEM: 12160825
- Service: 15305801
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) - Bank 1 Sensor 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 1669 | Heated Oxygen Sensor Low Signal - Bank 1 Sensor 2
B | 0.5 PU/WH | 1668 | Heated Oxygen Sensor High Signal - Bank 1 Sensor 2
C | 0.8 PK/BK | 5294 | Ignition Voltage
D | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control - Bank 1 Sensor 2

### Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 1

#### Connector Part Information

- OEM: 12160482
- Service: 88988598
- Description: 4-Way F Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 1667 | Heated Oxygen Sensor Low Signal - Bank 2 Sensor 1
B | 0.5 PU | 1666 | Heated Oxygen Sensor High Signal - Bank 2 Sensor 1
C | 0.5 PK/BK | 5293 | Ignition Voltage
D | 0.5 L-GN | 3212 | Heated Oxygen Sensor Heater Low Control - Bank 2 Sensor 1

### Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 2

#### Connector Part Information

- OEM: 12160825
- Service: 15305801
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) - Bank 2 Sensor 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 1671 | Heated Oxygen Sensor Low Signal - Bank 2 Sensor 2
B | 0.5 PU | 1670 | Heated Oxygen Sensor High Signal - Bank 2 Sensor 2
C | 0.5 PK/BK | 5294 | Ignition Voltage
D | 0.5 OG/WH | 3223 | Heated Oxygen Sensor Heater Low Control - Bank 2 Sensor 2

### Heated Seat Control Module X1 (KA1)

#### Connector Part Information

- OEM: 6098-4606
- Service: 15134095
- Description: 6-Way F (BN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module X1 (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control
3 | 0.8 RD/WH | 2077 | Heated Seat Cushion Element Control
4 | -- | -- | Not Used
5 | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
6 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Control

### Heated Seat Control Module X2 (KA1)

#### Connector Part Information

- OEM: 6098-4787
- Service: 88988653
- Description: 8-Way F (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module X2 (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 OG | 640 | Battery Positive Voltage
2 | 0.8 BK | 650 | Ground
3-5 | -- | -- | Not Used
6 | 0.35 YE | 2080 | Low Reference
7 | -- | -- | Not Used
8 | 0.35 PK | 2435 | Low Reference

### Heated Seat Control Module X3 (KA1)

#### Connector Part Information

- OEM: 7283-9040
- Service: 15127042
- Description: 10-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module X3 (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 D-GN | 5060 | Ground
7-10 | -- | -- | Not Used

### Heated Seat Control Module X4 (KA1)

#### Connector Part Information

- OEM: 31410-1200
- Service: 15126711
- Description: 20-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module X4 (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-8 | -- | -- | Not Used
9 | 0.35 YE | 2079 | Heated Seat Cushion Temperature Sensor Signal
10-19 | -- | -- | Not Used
20 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal

### Heated Seat Element - Driver Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way M Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Driver Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 2432 | Driver Heated Seat Back Element Control
B | 0.8 PU | 2424 | Driver Heated Seat Back Element Control

### Heated Seat Element - Driver Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Driver Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal
B | 0.8 RD/WH | 2077 | Heated Seat Cushion Element Control
C | 0.35 YE | 2080 | Low Reference
D | 0.8 BN | 2432 | Driver Heated Seat Back Element Control

### Heated Seat Element - Passenger Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way M Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Passenger Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 TN | 2481 | Passenger Heated Seat Back Element Control
B | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control

### Heated Seat Element - Passenger Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Passenger Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal
B | 0.8 D-BU | 2479 | Passenger Heated Seat Element Control
C | 0.35 PK | 2435 | Low Reference
D | 0.8 TN | 2481 | Passenger Heated Seat Back Element Control

### Hood Ajar Switch

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F GT 150 Sealed 4.5 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Hood Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 109 | Hood Ajar Switch Signal
B | 0.5 PU | 5531 | Hood Closed Switch Signal
C | 0.35 BK | 1250 | Ground

### Horn

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A - E/A
- Core/Insulation Crimp: Pins B - 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Horn

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1250 | Ground
B | 0.8 D-GN | 29 | Horn Control

### Horn Switch

#### Connector Part Information

- OEM: 50-57-9402
- Service: 15306026
- Description: 2-Way F SL Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 28 | Horn Relay Control
2 | 0.35 BK | 1450 | Ground

### HVAC Control Module X1

#### Connector Part Information

- OEM: 15126709
- Service: See Catalog
- Description: 20-Way F Receptacle 0.64 Unsealed (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 D-GN | 734 | Inside Air Temperature Sensor Signal
3 | 0.35 L-BU/BK | 590 | Driver Sunload Sensor Signal
4 | 0.35 GY | 1548 | Passenger Sunload Sensor Signal
5-7 | -- | -- | Not Used
8 | 0.35 PK | 2145 | Air Temperature Switch Signal - Right (C69)
9 | 0.35 OG | 2615 | Auxiliary Mode Door Control (C69)
10 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control (C69)
11-14 | -- | -- | Not Used
15 | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal
16 | -- | -- | Not Used
17 | 0.35 GY | 5954 | Inside Air Temperature Sensor Motor Control
18 | 0.35 GY | 2599 | Auxiliary Mode Door Control (C69)
19 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control (C69)
20 | -- | -- | Not Used

### HVAC Control Module X2

#### Connector Part Information

- OEM: 7283-9080-90
- Service: See Catalog
- Description: 16-Way F 064 Series Unsealed (BU)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU/WH | 1382 | LED Dimming Supply
2 | 0.35 PK | 1139 | Ignition Voltage
3 | 0.35 BK/WH | 1551 | Ground
4 | 0.35 RD/WH | 1840 | Battery Positive Voltage
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-7 | -- | -- | Not Used
8 | 0.35 WH | 193 | Rear Defog Relay Control
9 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
10 | 0.5 BK | 1450 | Ground
11 | -- | -- | Not Used
12 | 0.35 YE | 61 | Low Reference
13-16 | -- | -- | Not Used

### HVAC Control Module X3

#### Connector Part Information

- OEM: 15126710
- Service: See Catalog
- Description: 20-Way F Receptacle 0.64 Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal
2 | 0.35 L-GN | 2275 | Mode Door Position Signal
3 | 0.35 PU | 1838 | Recirculation Door Position Signal
4 | 0.35 GY/BK | 754 | Blower Motor Speed Control
5 | 0.35 TN | 2273 | Mode Door Control
6 | -- | -- | Not Used
7 | 0.35 D-GN | 1614 | Recirculation Door Control
8 | 0.35 D-BU | 1199 | Air Temperature Door Control
9 | -- | -- | Not Used
10 | 0.35 GY | 598 | 5-Volt Reference
11-12 | -- | -- | Not Used
13 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
14 | 0.35 WH | 2622 | 5-Volt Reference
15 | 0.35 WH | 119 | Mode Door Control
16 | -- | -- | Not Used
17 | 0.35 TN/BK | 2274 | Recirculation Door Control
18 | 0.35 L-BU | 1316 | Air Temperature Door Control
19 | 0.35 TN | 552 | Low Reference
20 | 0.35 YE | 1791 | Low Reference

### HVAC Control Module X4 (C69)

#### Connector Part Information

- OEM: 7283-9079-60
- Service: See Catalog
- Description: 16-Way F 064 Series Unsealed (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X4 (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 GY | 597 | 5-Volt Reference
3 | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control
4 | 0.35 BN | 6555 | Rear Temperature Motor Control
5 | 0.35 GY | 720 | Low Reference
6-9 | -- | -- | Not Used
10 | 0.35 GY/BK | 754 | Blower Motor Speed Control
11 | 0.35 OG | 2215 | Auxiliary Mode Door Control
12 | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control
13-16 | -- | -- | Not Used

### HVAC Control Module - Auxiliary (C69)

#### Connector Part Information

- OEM: 89047355
- Service: See Catalog
- Description: 10-Way F 0.64 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module - Auxiliary (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 8 | Instrument Panel Lamp Control
2 | 0.35 BK/WH | 1551 | Ground
3 | 0.35 GY | 597 | 5-Volt Reference
4 | 0.35 GY | 720 | Low Reference
5-6 | -- | -- | Not Used
7 | 0.35 PU/WH | 760 | Auxiliary Blower Motor Speed Control
8 | 0.35 YE | 2214 | Auxiliary Air Temperature Door Control
9 | -- | -- | Not Used
10 | 0.35 OG | 2615 | Auxiliary Mode Door Control

### Ignition Coil 1

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 1550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 PU | 2121 | Ignition Control 1
D | 1.0 PK/BK | 5291 | Ignition Voltage

### Ignition Coil 2

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 150 | Ground
B | 0.5 BN/WH | 2130 | Low Reference
C | 0.5 OG/WH | 2122 | Ignition Control 2
D | 1.0 PK/BK | 5292 | Ignition Voltage

### Ignition Coil 3

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 1550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 L-BU | 2123 | Ignition Control 3
D | 1.0 PK/BK | 5291 | Ignition Voltage

### Ignition Coil 4

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 150 | Ground
B | 0.5 BN/WH | 2130 | Low Reference
C | 0.5 D-GN/WH | 2124 | Ignition Control 4
D | 1.0 PK/BK | 5292 | Ignition Voltage

### Ignition Coil 5

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 1550 | Ground
B | 0.5 BN | 2129 | Low Reference
C | 0.5 D-GN | 2125 | Ignition Control 5
D | 1.0 PK/BK | 5291 | Ignition Voltage

### Ignition Coil 6

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal/150 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, D - 2/A
- Core/Insulation Crimp: Pins B, C - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil 6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 150 | Ground
B | 0.5 BN/WH | 2130 | Low Reference
C | 0.5 L-BU/WH | 2126 | Ignition Control 6
D | 1.0 PK/BK | 5292 | Ignition Voltage

### Ignition Lock Cylinder Control Solenoid

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ignition Lock Cylinder Control Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 1450 | Ground
B | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control

### Ignition Switch

#### Connector Part Information

- OEM: HCMPBC06K
- Service: See Catalog
- Description: 6-Way F HCM Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PK | 3 | Ignition Voltage
2 | 0.35 BN | 4 | Ignition Voltage
3 | 0.35 RD/WH | 3340 | Battery Positive Voltage
4 | 0.35 WH/BK | 1073 | 5-Volt Reference
5 | 0.35WH | 1390 | Ignition Voltage
6 | -- | -- | Not Used

### Inflatable Restraint Front End Sensor - Left

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/OG | 5045 | Low Reference
B | 0.35 YE | 354 | Front End Sensor - Left - Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 5600 | Low Reference
B | 0.35 D-GN | 1409 | Front End Sensor - Right - Signal

### Inflatable Restraint Front Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15332142
- Service: 89046638
- Description: 6-Way M GT 150/280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Front Passenger Presence System (PPS) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 840 | Battery Positive Voltage
B | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
C | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
D | 0.35 BK | 651 | Ground
E-F | -- | -- | Not Used

### Inflatable Restraint I/P Module X1

#### Connector Part Information

- OEM: 252922343
- Service: See Catalog
- Description: 2-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control
B | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control

### Inflatable Restraint I/P Module X2

#### Connector Part Information

- OEM: 252922343
- Service: See Catalog
- Description: 2-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control
B | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control

### Inflatable Restraint I/P Module Indicator

#### Connector Part Information

- OEM: 15398877
- Service: See Catalog
- Description: 5-Way F HCM Series (WH)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Inflatable Restraint I/P Module Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
2 | 0.35 BK | 1450 | Ground
3 | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
4 | 0.35 PK | 1139 | Ignition Voltage
5 | 0.35 PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Roof Rail Module - Left (ASF)

#### Connector Part Information

- OEM: Not Available
- Service: Not Available
- Description: 2-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 2137 | Side Impact Module - Left Front - High Control
B | 0.5 WH | 2138 | Side Impact Module - Left Front - Low Control

### Inflatable Restraint Roof Rail Module - Right (ASF)

#### Connector Part Information

- OEM: Not Available
- Service: Not Available
- Description: 2-Way F (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 2135 | Side Impact Module - Right Front - High Control
B | 0.5 WH | 2136 | Side Impact Module - Right Front - Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 2-184464-4
- Service: See Catalog
- Description: 60-Way F GET Series (YE)

#### Terminal Part Information

- Terminal/Tray: 1393365-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 651 | Ground
2 | 0.5 D-GN | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
4 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
5 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
6 | 0.35 GY | 3027 | Instrument Panel Module - Stage 2 - High Control
7 | 0.35 PU | 3026 | Instrument Panel Module - Stage 2 - Low Control
8 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
9 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
10 | 0.35 YE | 3025 | Instrument Panel Module - Stage 1 - High Control
11 | 0.35 OG | 3024 | Instrument Panel Module - Stage 1 - Low Control
12 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control
13 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control
14 | 0.5 TN/WH | 2135 | Side Impact Module - Right Front - High Control
15 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control
16 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
17 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
18 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
19 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
20-27 | -- | -- | Not Used
28 | 0.35 PK | 5057 | Low Reference
29-30 | -- | -- | Not Used
31 | 0.5 RD/WH | 1340 | Battery Positive Voltage
32 | 0.5 PK | 1139 | Ignition Voltage
33-35 | -- | -- | Not Used
36 | 0.35 YE | 354 | Front End Sensor - Left - Signal
37 | 0.35 D-GN | 1409 | Front End Sensor - Right - Signal
38 | 0.35 TN/OG | 5045 | Low Reference
39 | 0.35 GY | 5600 | Low Reference
40 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
41 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
42 | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage
43 | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage
44-57 | -- | -- | Not Used
58 | 0.35 YE/BK | 5229 | Roll Over Sensor High Signal
59 | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal
60 | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
B | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage

### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
B | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 54560220
- Service: See Catalog
- Description: 2-Way F Type B (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
2 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 54560222
- Service: See Catalog
- Description: 2-Way F Type G (PK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
2 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PU | 1375 | Steering Wheel Control Control
D | 0.35 GY | 1884 | Cruise Control Switch Signal
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 D-GN/WH | 7158 | Cruise Control Indicator Dimming Signal
G | 0.35 PU/WH | 7005 | LED Dimming Signal
H | -- | -- | Not Used
J | 0.35 TN | 28 | Horn Relay Control
K | 0.35 BK | 1450 | Ground

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PU | 1375 | Steering Wheel Control Control
D | 0.35 GY | 1884 | Cruise Control Switch Signal
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 D-GN/WH | 7158 | Cruise Control Indicator Dimming Signal
G | 0.35 PU/WH | 7005 | LED Dimming Signal
H | -- | -- | Not Used
J | 0.35 TN | 28 | Horn Relay Control
K | 0.35 BK | 1450 | Ground

### Inflatable Restraint Steering Wheel Module Coil X3

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
2 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
3 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
4 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control

### Inflatable Restraint Vehicle Rollover Sensor (ASF)

#### Connector Part Information

- OEM: 6189-6936
- Service: See Catalog
- Description: 6-Way F 0.64 Series Sealed (YE)

#### Terminal Part Information

- Pins: 1, 6
- Terminal/Tray: 8100-3427/22
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

- Pins: 3, 4, 4, 5
- Terminal/Tray: 8100-3426/22
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Inflatable Restraint Vehicle Rollover Sensor (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 RD/WH | 1340 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
4 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
5 | 0.35 YE/BK | 5229 | Roll Over Sensor High Signal
6 | 0.5 BK/WH | 651 | Ground

### Infrared Transmitter (UUC)

#### Connector Part Information

- OEM: 15429806
- Service: See Catalog
- Description: 16-Way F Micro 64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Infrared Transmitter (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 5826 | Left DVD Audio Signal (+)
2 | 0.5 PU | 6979 | DVD Audio Common
3 | 0.5 WH | 5828 | Right DVD Audio Signal (+)
4 | 0.35 YE | 343 | Ignition Voltage
5-7 | -- | -- | Not Used
8 | 0.5 OG/BK | 5831 | Remote Infra Red Signal (+)
9-11 | -- | -- | Not Used
12 | 0.5 BK/WH | 1551 | Ground
13-15 | -- | -- | Not Used
16 | 0.5 TN/WH | 5830 | Remote Infra Red Signal (-)

### Input Speed Sensor (ISS)

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2F (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Input Speed Sensor (ISS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 1230 | Automatic Transmission Input Speed Sensor (ISS) High Signal
2 | 0.5 TN | 1231 | Automatic Transmission Input Speed Sensor (ISS) Low Signal

### Inside Air Temperature Sensor

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Inside Air Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 734 | Inside Air Temperature Sensor Signal
B | 0.35 GY | 5954 | Inside Air Temperature Sensor Motor Control
C | 0.35 BK/WH | 1551 | Ground
D | 0.35 YE | 61 | Low Reference

### Inside Rearview Mirror (ISRVM)

#### Connector Part Information

- OEM: 917981-2
- Service: 15306351
- Description: 16-Way F 0.040/0.070 HYBRID I/O (BK)

#### Terminal Part Information

- Pins: 2, 5, 8-16
- Terminal/Tray: 175266-5/15
- Core/Insulation Crimp: Pins 2, 5, 8-16 - J/J
- Core/Insulation Crimp: Pins 9 - K/K
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Inside Rearview Mirror (ISRVM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-7 | -- | -- | Not Used
8 | 0.35 BK/WH | 850 | Ground
9 | 0.5 L-GN | 24 | Backup Lamp Control
10 | -- | -- | Not Used
11 | 0.35 D-GN/WH | 2514 | Keypad Signal (UE1)
12 | 0.35 L-GN/BK | 2515 | Keypad Control (UE1)
13 | 0.35 YE | 443 | Ignition Voltage
14 | 0.35 YE/BK | 2516 | Keypad Green LED Signal (UE1)
15 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1)
16 | -- | -- | Not Used

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 1326133-1
- Service: See Catalog
- Description: 18-Way F Receptacle 0.64 Unsealed (BK)

#### Terminal Part Information

- Pins: 2-6, 8-14, 16
- Terminal/Tray: 638551-1/16
- Core/Insulation Crimp: Pins 2, 10-13 - K/K
- Core/Insulation Crimp: Pins 3-6, 8-9, 14, 16 - J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 PK | 893 | Driver Information Center (DIC) Select Menu Switch Signal
3 | 0.35 PU | 5234 | Passenger Seat Belt Indicator
4 | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
5 | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
6 | 0.35 BK/WH | 1551 | Ground
7 | -- | -- | Not Used
8 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
9 | 0.35 TN/WH | 33 | Brake Warning Indicator Control
10 | 0.5 BN | 897 | Low Reference
11 | 0.5 BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
12 | 0.5 D-GN/WH | 1358 | Driver Information Center (DIC) Switch Signal
13 | 0.5 PK | 1139 | Ignition Voltage
14 | 0.35 RD/WH | 1640 | Battery Positive Voltage
15 | -- | -- | Not Used
16 | 0.35 YE | 749 | Security Indicator Control
17-18 | -- | -- | Not Used

### Knock Sensor (KS) 1

#### Connector Part Information

- OEM: 15374222
- Service: See Catalog
- Description: 2-Way F GT 150 Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (WH)

#### Knock Sensor (KS) 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | Knock Sensor 1 Signal
B | 0.5 GY | 1716 | Knock Sensor 1 Signal

### Knock Sensor (KS) 2

#### Connector Part Information

- OEM: 15374222
- Service: See Catalog
- Description: 2-Way F GT 150 Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Knock Sensor (KS) 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
B | 0.5 GY | 2303 | Knock Sensor 2 Signal

### License Lamp - Left

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F Lamp Socket Wedge Base W2 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 309 | Right Park Lamp Control
B | 0.5 BK | 550 | Ground

### License Lamp - Right

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F Lamp Socket Wedge Base W2 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 309 | Right Park Lamp Control
0.35 BK | 309 | Right Park Lamp Control
B | 0.5 BK | 550 | Ground
0.5 BK | 550 | Ground

### Liftgate Latch

#### Connector Part Information

- OEM: 15476199
- Service: 88988358
- Description: 6-Way F GT 280 Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Liftgate Latch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control
2 | -- | -- | Not Used
3 | 0.5 BK | 550 | Ground
4 | -- | -- | Not Used
5 | 0.35 BK | 550 | Ground
6 | 0.5 PK/BK | 1303 | Liftgate Ajar Switch Signal

### Liftgate Release Switch

#### Connector Part Information

- OEM: 15366025
- Service: 15306406
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Release Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN | 5797 | Rear Closure Handle Switch Open Signal
B | -- | -- | Not Available
C | 0.35 L-GN | 550 | Ground
D | -- | -- | Not Available

### Marker Lamp - Left Front

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 709 | Left Park Lamp Control
2 | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Marker Lamp - Right Front

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 309 | Right Park Lamp Control
2 | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 13520906
- Service: 19151493
- Description: 5-Way F GT 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, B, D, E - E/A
- Core/Insulation Crimp: Pins C - 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 492 | Mass Air Flow Sensor Signal
B | 0.5 PK | 1039 | Ignition Voltage
C | 0.8 BK/WH | 451 | Ground
D | 0.5 TN | 472 | Intake Air Temperature Sensor Signal
E | 0.5 TN | 2760 | Low Reference

### Mode Actuator

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Mode Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-GN | 2275 | Mode Door Position Signal
3 | 0.35 GY | 598 | 5-Volt Reference
4 | 0.35 WH | 119 | Mode Door Control
5 | 0.35 TN | 2273 | Mode Door Control

### Mode Actuator - Auxiliary (C69)

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Mode Actuator - Auxiliary (C69)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY/BK | 1798 | Ground
2 | 0.35 GY | 2599 | Auxiliary Mode Door Control
3 | 0.35 GY | 596 | 5-Volt Reference
4 | 0.35 L-GN/WH | 5729 | Rear Mode Motor Control
5 | 0.35 OG | 2215 | Auxiliary Mode Door Control

### Noise Compensation Microphone (U3U)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Noise Compensation Microphone (U3U)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 655 | Cellular Microphone Signal
B | 0.5 BARE | 1489 | Drain Wire

### Output Speed Sensor (OSS)

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2F (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Output Speed Sensor (OSS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 RD | 400 | Output Shaft Sensor (OSS) High Signal
2 | 0.5 BK | 401 | Output Shaft Sensor (OSS) Low Signal

### Outside Rearview Mirror - Driver (DK2)

#### Connector Part Information

- OEM: 15269798
- Service: See Catalog
- Description: 6-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Driver (DK2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1499 | Driver Mirror Motor Left/Up Control
2 | 0.35 WH | 81 | Driver Mirror Motor Right Control
3 | 0.35 L-GN | 88 | Driver Mirror Motor Down Control
4 | -- | -- | Not Used
5 | 0.5 BK | 650 | Ground
6 | 0.5 OG | 2267 | Mirror Heating Element Control

### Outside Rearview Mirror - Driver (without DK2)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Driver (without DK2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1499 | Driver Mirror Motor Left/Up Control
B | 0.35 WH | 81 | Driver Mirror Motor Right Control
C | 0.35 L-GN | 88 | Driver Mirror Motor Down Control

### Outside Rearview Mirror - Passenger (DK2)

#### Connector Part Information

- OEM: 15269798
- Service: See Catalog
- Description: 6-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Passenger (DK2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1497 | Passenger Mirror Motor Left/Up Control
2 | 0.35 WH | 881 | Passenger Mirror Motor Right Control
3 | 0.35 L-GN | 889 | Passenger Mirror Motor Down Control
4 | -- | -- | Not Used
5 | 0.5 BK | 650 | Ground
6 | 0.5 OG | 2267 | Mirror Heating Element Control

### Outside Rearview Mirror - Passenger (without DK2)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Passenger (without DK2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1497 | Passenger Mirror Motor Left/Up Control
B | 0.35 WH | 881 | Passenger Mirror Motor Right Control
C | 0.35 L-GN | 889 | Passenger Mirror Motor Down Control

### Outside Rearview Mirror Switch

#### Connector Part Information

- OEM: 15327190
- Service: See Catalog
- Description: 8-Way F Ducon 0.8 Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 15326592/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Outside Rearview Mirror Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 840 | Battery Positive Voltage
2 | 0.35 BK | 1450 | Ground
3 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control
4 | 0.35 WH | 81 | Driver Mirror Motor Right Control
5 | 0.35 L-GN | 1499 | Driver Mirror Motor Left/Down Control
6 | -- | -- | Not Used
7 | 0.35 YE | 88 | Driver Mirror Motor Up Control
8 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control

### Overhead Console Courtesy/Reading Lamp

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-pack 150 Series (BK)

#### Overhead Console Courtesy/Reading Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 1732 | 12-Volt Reference
B | 0.8 BK | 850 | Ground
C | 0.8 GY | 157 | Courtesy Lamp Control

### Park Brake Switch

#### Connector Part Information

- OEM: 12047682
- Service: 12101850
- Description: 1-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 233 | Park Brake Switch Signal

### Park Lamp - Left Front

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 709 | Left Park Lamp Control
0.35 L-GN | 709 | Left Park Lamp Control
2 | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Park Lamp - Right Front

#### Connector Part Information

- OEM: 10351681
- Service: See Catalog
- Description: 2-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 309 | Right Park Lamp Control
0.35 L-GN | 309 | Right Park Lamp Control
2 | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Park Position Switch

#### Connector Part Information

- OEM: 05-1165-0937
- Service: See Catalog
- Description: 4-Way F

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park Position Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU/WH | 5905 | Key Capture/Column Lock Shift Position Signal
B | -- | -- | Not Used
C | -- | -- | Not Used
D | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control

### Park/Turn Signal Lamp - Left Front

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MIN | 0.35 D-BU | 1314 | Left Front Turn Signal Lamp Control
MAJ | 0.35 L-GN | 709 | Left Park Lamp Control
0.35 L-GN | 709 | Left Park Lamp Control
G | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Park/Turn Signal Lamp - Left Rear

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MIN | 0.8 WH | 18 | Left Rear Stop/Turn Lamp Control
MAJ | 0.35 D-GN | 709 | Left Park Lamp Control
0.35 D-GN | 709 | Left Park Lamp Control
G | 0.5 BK | 550 | Ground
0.5 BK | 550 | Ground

### Park/Turn Signal Lamp - Right Front

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MIN | 0.35 D-BU | 1315 | Right Front Turn Signal Lamp Control
MAJ | 0.35 L-GN | 309 | Right Park Lamp Control
0.35 L-GN | 309 | Right Park Lamp Control
G | 0.35 BK | 1250 | Ground
0.35 BK | 1250 | Ground

### Park/Turn Signal Lamp - Right Rear

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MIN | 0.8 WH | 19 | Right Rear Stop/Turn Lamp Control
MAJ | 0.35 D-GN | 309 | Right Park Lamp Control
0.35 D-GN | 309 | Right Park Lamp Control
G | 0.5 BK | 850 | Ground
0.5 BK | 850 | Ground

### Pressure Control (PC) Solenoid Valve

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2-Way F (BU)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Pressure Control (PC) Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 1994 | Line Pressure Control Solenoid Valve High Control
2 | GY | 5510 | Line Pressure Control Solenoid Valve Low Control

### Radio X1

#### Connector Part Information

- OEM: 7283-4490-30
- Service: 88988743
- Description: 14-Way F (BK)

#### Terminal Part Information

- Pins: 1, 8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 2-7, 9-10, 13
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: Pins 2-3, 9-10 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 4-7, 13 - P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 RD/WH | 2040 | Battery Positive Voltage
2 | 0.75 TN | 201 | Left Front Speaker Output (+)
3 | 0.75 TN | 1875 | Right Front Speaker Output (+)
4 | 0.5 GY | 655 | Cellular Microphone Signal (U3U)
5 | 0.35 BARE | 1489 | Drain Wire (U3U)
6 | 0.5 WH | 1487 | Antenna Enable Signal
7 | 0.35 PU/WH | 1382 | LED Dimming Supply
8 | 0.8 BK/WH | 1551 | Ground
9 | 0.75 GY | 118 | Left Front Speaker Output (-)
10 | 0.75 TN/WH | 1975 | Right Front Speaker Output (-)
11-12 | -- | -- | Not Used
13 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
14 | -- | -- | Not Used

### Radio X2

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Pins: 1-2, 5-6, 8-9, 13-14
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: Pins 1-2, 8-10 - P/P
- Core/Insulation Crimp: Pins 5-6, 13-14 - See Terminal Repair Kit
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 367 | Remote Radio Left Audio Signal (+) (U2K)
2 | 0.5 D-GN/WH | 368 | Remote Radio Right Audio Signal (+) (U2K)
3-4 | -- | -- | Not Used
5 | 0.75 BN | 199 | Left Rear Speaker Output (+)
6 | 0.75 D-BU | 46 | Right Rear Speaker Output (+)
7 | -- | -- | Not Used
8 | 0.5 OG | 5748 | Radio Audio Mute Signal (U65)
9 | 0.5 TN/WH | 372 | Remote Radio Audio Output (-) (U2K)
10 | 0.5 GY | 388 | Remote Radio Right Audio Signal (-) (U2K)
11-12 | -- | -- | Not Used
13 | 0.75 YE | 116 | Left Rear Speaker Output (-)
14 | 0.75 L-BU | 115 | Right Rear Speaker Output (-)
15-16 | -- | -- | Not Used

### Radio X3 (UUC)

#### Connector Part Information

- OEM: 7283-9077-40
- Service: 89047195
- Description: 14-Way F Kaizen 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X3 (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 2059 | Auxiliary Audio Left Signal
2 | 0.5 WH | 2058 | Auxiliary Audio Right Signal
3 | 0.5 L-BU | 5826 | Left DVD Audio Signal (+)
4 | 0.5 WH | 5828 | Right DVD Audio Signal (+)
5 | 0.5 OG/BK | 5831 | Remote Infra Red Signal (+)
6 | 0.5 PK/BK | 5844 | Video Bright Control
7 | 0.5 D-GN | 6975 | DVD Video Signal (+)
8 | 0.5 PU | 2056 | Auxiliary Video High Signal
9 | 0.35 BARE | 5345 | Drain Wire
10 | 0.5 BN/WH | 5846 | Video Power Mode Signal
11 | 0.5 PU | 6979 | DVD Audio Common
12 | 0.35 BARE | 6980 | DVD Drain Wire
13 | 0.5 TN/WH | 5830 | Remote Infra Red Signal (-)
14 | 0.35 BARE | 6976 | DVD Video Drain Wire
15 | 0.5 WH/BK | 5335 | DVD Video Signal (-)
16 | 0.35 BARE | 5346 | Video Drain Wire

### Radio X4 (U3U)

#### Connector Part Information

- OEM: 15394151
- Service: See Catalog
- Description: 16-Way F Micro 64 (BN)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio X4 (U3U)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3U)
6-16 | -- | -- | Not Used

### Rear Differential Clutch Control Module X1 (MH6)

#### Connector Part Information

- OEM: 89047383
- Service: See Catalog
- Description: 10-Way F 0.64 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Rear Differential Clutch Control Module X1 (MH6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 BK | 850 | Ground
4 | -- | -- | Not Used
5 | 0.5 L-BU | 5986 | Serial Data Communication Enable
6 | 0.5 RD/WH | 1740 | Battery Positive Voltage
7 | -- | -- | Not Used
8 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
9 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
10 | -- | -- | Not Used

### Rear Differential Clutch Control Module X2 (MH6)

#### Connector Part Information

- OEM: 89047382
- Service: See Catalog
- Description: 5-Way F 0.64 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Rear Differential Clutch Control Module X2 (MH6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 YE | 9998 | Low Reference
3 | 0.5 YE | 9996 | Low Reference
4 | 0.5 YE | 9999 | All Wheel Drive Temperature Sensor Signal
5 | 0.5 YE | 9997 | All Wheel Drive Coil Control

### Rear Wheel Drive Module Clutch (MH6)

#### Connector Part Information

- OEM:90980-10942
- Service: See Catalog
- Description: 4-Way F

#### Rear Wheel Drive Module Clutch (MH6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 9996 | Low Reference
2 | 0.5 YE | 9997 | AWD Coil Supply Voltage
3 | 0.5 YE | 9999 | AWD Temperature Sensor Signal
4 | 0.5 YE | 9998 | Low Reference

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 7123-5014-30
- Service: 88988465
- Description: 1-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-2951-02/27
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 BK | 293 | Rear Defog Element Control

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 7123-5014-30
- Service: 88988465
- Description: 1-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-2951-02/27
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 550 | Ground

### Rear Window Wiper Motor

#### Connector Part Information

- OEM: 15332141
- Service: 88986249
- Description: 6-Way F GT 150 Series, Unsealed (BK)

#### Terminal Part Information

- Pins: A-F
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins A, C - C/A
- Core/Insulation Crimp: Pins B, D-F - E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Rear Window Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 550 | Ground
B | 0.35 L-GN | 2270 | Rear Window Washer Relay Control
C | 1.0 RD/WH | 2140 | Battery Positive Voltage
D | 0.5 YE | 243 | Ignition Voltage
E | 0.35 GY | 391 | Rear Window Wiper Switch Signal
F | 0.5 PK/BK | 1303 | Liftgate Ajar Switch Signal

### Rear Window Wiper/Washer/Fog Lamp Switch

#### Connector Part Information

- OEM: HCMPB-06-K
- Service: 19115655
- Description: 6-Way F HCM Series (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Rear Window Wiper/Washer/Fog Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 1551 | Ground
2 | 0.35 GY | 391 | Rear Window Wiper Switch Signal
3 | 0.35 L-GN | 2270 | Rear Window Washer Relay Control
4 | 0.35 OG | 192 | Front Fog Lamp Switch Signal (T96)
5 | 0.35 BK | 1450 | Ground
6 | 0.35 PU/WH | 1382 | LED Dimming Supply (T96)

### Recirculation Actuator

#### Connector Part Information

- OEM: 12064982
- Service: 12102633
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Recirculation Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 PU | 1838 | Recirculation Door Position Signal
3 | 0.35 GY | 598 | 5-Volt Reference
4 | 0.35 TN/BK | 2274 | Recirculation Door Control
5 | 0.35 D-GN | 1614 | Recirculation Door Control

### Remote Control Door Lock Receiver (RCDLR)

#### Connector Part Information

- OEM: IL-AG5-4S-S3C1
- Service: 88988745
- Description: 4-Way F ILAG5 Series (GN)

#### Terminal Part Information

- Terminal/Tray: IL-AG5-C1-5000/20
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: J-38125-211/J-35616-64B (L-BU)

#### Remote Control Door Lock Receiver (RCDLR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1840 | Battery Positive Voltage
2 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | 0.35 BK/WH | 651 | Ground

### Seat Adjuster Switch - Driver (AG1)

#### Connector Part Information

- OEM: 15326924
- Service: 15306174
- Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Adjuster Switch - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
B | 3.0 BK | 284 | Driver Seat Horizontal Motor Rearward Control
C | 3.0 RD | 285 | Driver Seat Horizontal Motor Forward Control
D | 2.0 RD/BK | 542 | Battery Positive Voltage
E | 3.0 YE | 282 | Driver Seat Rear Vertical Motor Up Control
F | 2.0 BK | 650 | Ground
G | 3.0 L-BU | 283 | Driver Seat Rear Vertical Motor Down Control
H | 3.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control

### Seat Belt Buckle - Driver

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/WH | 5057 | Low Reference
B | 0.35 D-BU | 5016 | Seat Belt Switch - Left - Signal

### Seat Belt Buckle - Passenger

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 5057 | Low Reference
B | 0.35 RD | 1362 | Seat Belt Switch - Right - Signal

### Seat Belt Pretensioner - Left

#### Connector Part Information

- OEM: 252922346
- Service: See Catalog
- Description: 2-Way F (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Pretensioner - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
2 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control

### Seat Belt Pretensioner - Right

#### Connector Part Information

- OEM: 252922347
- Service: See Catalog
- Description: 2-Way F (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Pretensioner - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
2 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control

### Seat Front Vertical Motor - Driver (AG1)

#### Connector Part Information

- OEM: 12020556
- Service: 12101820
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Front Vertical Motor - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control
2 | 3.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control

### Seat Rear Vertical Motor - Driver (AG1)

#### Connector Part Information

- OEM: 12020556
- Service: 12101820
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Rear Vertical Motor - Driver (AG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 L-BU | 283 | Driver Seat Rear Vertical Motor Down Control
2 | 3.0 YE | 282 | Driver Seat Rear Vertical Motor Up Control

### Shift Pressure Control (PC) Solenoid Valve

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2-Way F (GN)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Pressure Control (PC) Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD | 2880 | Shift Pressure Control Solenoid Valve High Control
2 | 0.35 BU | 5508 | Shift Pressure Control Solenoid Valve Low Control

### Shift Solenoid (SS) Valve 1

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 1-Way F (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Solenoid (SS) Valve 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 1222 | Shift Solenoid Valve 1 High Control

### Shift Solenoid (SS) Valve 2

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 1-Way F (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Solenoid (SS) Valve 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 1223 | Shift Solenoid Valve 2 High Control

### Shift Solenoid (SS) Valve 3

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 1-Way F (GY)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Solenoid (SS) Valve 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 898 | Shift Solenoid Valve 3 High Control

### Shift Solenoid (SS) Valve 4

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 1-Way F (BU)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Solenoid (SS) Valve 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU | 2879 | Shift Solenoid Valve 4 High Control

### Shift Solenoid (SS) Valve 5

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 1-Way F (BN)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Shift Solenoid (SS) Valve 5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 2527 | Shift Solenoid Valve 5 High Control

### Speaker - Left Front

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 201 | Left Front Speaker Output (+)
2 | 0.35 TN | 118 | Left Front Speaker Output (-)

### Speaker - Left Front Tweeter

#### Connector Part Information

- OEM: 626064-0
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Left Front Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 201 | Left Front Speaker Output (+)
2 | 0.35 TN | 118 | Left Front Speaker Output (-)

### Speaker - Left Rear

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BN | 116 | Left Rear Speaker Output (-)
2 | 0.8 YE | 199 | Left Rear Speaker Output (+)

### Speaker - Right Front

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 GY | 200 | Right Front Speaker Output (+)
2 | 0.8 TN | 117 | Right Front Speaker Output (-)

### Speaker - Right Front Tweeter

#### Connector Part Information

- OEM: 626064-0
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Front Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 GY | 200 | Right Front Speaker Output (+)
2 | 0.8 TN | 117 | Right Front Speaker Output (-)

### Speaker - Right Rear

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BN | 115 | Right Rear Speaker Output (-)
2 | 0.8 YE | 46 | Right Rear Speaker Output (+)

### Speaker - Subwoofer (U65)

#### Connector Part Information

- OEM: 12064760
- Service: 12085208
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Subwoofer (U65)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 L-GN/BK | 1794 | Subwoofer Speaker Coil 2 Output (-)
B | 1.0 D-BU/WH | 346 | Subwoofer Speaker Coil 2 Output (+)
C | 1.0 L-BU/BK | 315 | Subwoofer Speaker Coil 1 Output (-)
D | 1.0 D-GN | 1795 | Subwoofer Speaker Coil 1 Output (+)

### Starter Motor X1

#### Connector Part Information

- OEM: 12089916
- Service: 12101763
- Description: 1-Way F Metri-Pack 280 Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12176387/3
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Starter Motor X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 5 PU | 6 | Starter Solenoid Crank Voltage

### Starter Motor X2 (Battery Positive Cable)

#### Terminal Part Information

- Harness: Battery Positive Cable
- Terminal/Tray: 7003-1849-02
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter Motor X2 (Battery Positive Cable)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 32 RD | 1 | Battery Positive Voltage

### Starter Motor X2 (Engine)

#### Terminal Part Information

- Harness: Engine
- Terminal/Tray: 7003-1849-02
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter Motor X2 (Engine)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 19 RD | 1 | Battery Positive Voltage

### Steering Angle Sensor

#### Connector Part Information

- OEM: 1488752-1
- Service: 88988374
- Description: 6-Way F Receptacle 0.64 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1393365-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Steering Angle Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 6044 | 12-Volt Reference
2 | 0.5 BN/WH | 6437 | CAN Bus High Serial Data
3 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
4 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
5 | 0.5 WH/BK | 6436 | CAN Bus Low Serial Data
6 | 0.5 OG/BK | 6045 | Low Reference

### Steering Wheel Control Switch - Left (K34)

#### Connector Part Information

- OEM: 30700-1100
- Service: See Catalog
- Description: 10-Way F HDAC64 DR Series (GY)

#### Steering Wheel Control Switch - Left (K34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU | 1375 | 12-Volt Reference
2 | -- | -- | Not Used
3 | 0.35 GY | 1884 | Cruise Control Switch Signal
4-5 | -- | -- | Not Used
6 | 0.35 PU/WH | 7005 | LED Dimming Signal
7 | -- | -- | Not Used
8 | 0.35 BK | 1450 | Ground
9 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
10 | -- | -- | Not Used

### Steering Wheel Control Switch - Right (UK3)

#### Connector Part Information

- OEM: 31068-1010
- Service: See Catalog
- Description: 4-Way F HDAC64 SR Housing (BK)

#### Steering Wheel Control Switch - Right (UK3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 1450 | Ground
2 | 0.35 PU/WH | 7005 | LED Dimming Signal
3 | 0.35 PU | 1375 | 12-Volt Reference
4 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal

### Sunroof Control Module (CF5)

#### Connector Part Information

- OEM: 7283-8398-40
- Service: See Catalog
- Description: 14-Way F 64 2.8 YESC Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Control Module (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 RD/WH | 4440 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | 0.35 YE | 643 | Ignition Voltage
4 | 3.0 BK | 850 | Ground
5 | 0.35 OG/BK | 144 | Sunroof Switch Open Vent Signal
6 | 0.35 BN | 100 | Sunroof Switch Open Signal
7 | 0.35 D-GN | 2074 | Sunroof Switch Express Signal
8-10 | -- | -- | Not Used
11 | 0.35 D-BU | 128 | Low Reference
12 | 0.35 BN/WH | 9061 | Not Used
13 | 0.35 BK/WH | 9062 | Not Used
14 | 0.35 WH | 9063 | Not Used

### Sunroof Switch (CF5)

#### Connector Part Information

- OEM: 12064978
- Service: 12125678
- Description: 6-Way F Metri-Pack 100 Series (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Switch (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN | 100 | Sunroof Switch Open Signal
3 | 0.35 OG/BK | 144 | Sunroof Switch Open Vent Signal
4 | -- | -- | Not Used
5 | 0.35 D-BU | 128 | Low Reference
6 | 0.35 D-GN | 2074 | Sunroof Switch Express Signal

### Tail/Stop Lamp - Left

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MAJ | 0.35 D-GN | 709 | Left Park Lamp Control
MIN | 0.5 D-BU | 20 | Stop Lamp Control
G | 0.5 BK | 550 | Ground
0.5 BK | 550 | Ground

### Tail/Stop Lamp - Right

#### Connector Part Information

- OEM: 1999370
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MAJ | 0.35 D-GN | 309 | Right Park Lamp Control
MIN | 0.5 D-BU | 20 | Stop Lamp Control
G | 0.5 BK | 850 | Ground
0.5 BK | 850 | Ground

### Theft Deterrent Module (TDM)

#### Connector Part Information

- OEM: 50-57-9705
- Service: 88988353
- Description: 5-Way F SL Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 16-02-1110/20
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Theft Deterrent Module (TDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1040 | Battery Positive Voltage
2 | 0.35 BN | 4 | Ignition Voltage
3 | 0.35 BK/WH | 1551 | Ground
4 | -- | -- | Not Used
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data

### Throttle Body

#### Connector Part Information

- OEM: 15355297
- Service: 19115594
- Description: 6-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326427/5
- Core/Insulation Crimp: Pins A-B - 2/A
- Core/Insulation Crimp: Pins C-F - E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Body

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 582 | Throttle Actuator Control Motor Control - 2
B | 0.8 YE | 581 | Throttle Actuator Control Motor Control - 1
C | 0.5 TN | 2752 | Low Reference
D | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
E | 0.5 GY | 2701 | 5-Volt Reference
F | 0.5 PU | 486 | Throttle Position Sensor 2 Signal

### Torque Converter Clutch (TCC) Solenoid Valve

#### Connector Part Information

- OEM: Aisin AW
- Service: Non-Serviceable
- Description: Conn 2-Way F (BK)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Torque Converter Clutch (TCC) Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 5509 | Torque Converter Clutch Pressure Control Solenoid Valve Low Control
2 | L-GN | 5511 | Torque Converter Clutch Pressure Control Solenoid Valve High Control

### Traction Control Switch (TCS)

#### Connector Part Information

- OEM: 50-57-9403
- Service: See Catalog
- Description: 3-Way F Receptacle 0.64 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 16-02-1110/20
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Traction Control Switch (TCS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 1788 | Traction Control Switch Signal
2 | 0.35 BK/WH | 1551 | Ground
3 | 0.35 PU/WH | 1382 | LED Dimming Supply

### Transmission Control Module (TCM) X1

#### Connector Part Information

- OEM: 15476346
- Service: 19151494
- Description: 20-Way F GT 150 Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Pins: 1-2, 5, 12-16
- Core/Insulation Crimp: E/4
- Pins: 18-19
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Transmission Control Module (TCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 451 | Ground
2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
3-4 | -- | -- | Not Used
5 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
6-9 | -- | -- | Not Used
10 | 0.5 RD/WH | 540 | Battery Positive Voltage
11 | -- | -- | Not Used
12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
13 | 0.5 PK | 1339 | Ignition Voltage
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | 0.5 BN | 4 | Ignition Voltage
16 | 0.5 WH | 17 | Stop Lamp Switch Signal
17 | -- | -- | Not Used
18 | 0.8 BK/WH | 451 | Ground
19 | -- | -- | Not Used
20 | 0.5 OG/BK | 1786 | Park/Neutral Signal

### Transmission Control Module (TCM) X2

#### Connector Part Information

- OEM: 7183-6563-30
- Service: Non-Serviceable
- Description: 4-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Transmission Control Module (TCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 401 | Output Speed Sensor (OSS) Low Signal
2 | 0.5 RD | 400 | Output Speed Sensor (OSS) High Signal
3 | 0.5 L-BU | 1230 | Input Speed Sensor (ISS) High Signal
4 | 0.5 TN | 1231 | Input Speed Sensor (ISS) Low Signal

### Transmission Control Module (TCM) X3

#### Connector Part Information

- OEM: 61890031
- Service: Non-Serviceable
- Description: Conn 22-Way M (D-GR)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp:
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Transmission Control Module (TCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 1222 | Shift Solenoid Valve 1 High Control
2 | BK | 1223 | Shift Solenoid Valve 2 High Control
3 | L-GN | 1994 | Line Pressure Control Solenoid Valve High Control
4-5 | -- | -- | Not Used
6 | GY | 5510 | Line Pressure Control Solenoid Valve Low Control
7 | BN | 5509 | TCC Pressure Control Solenoid Valve Low Control
8 | -- | -- | Not Used
9 | L-GN | 5511 | TCC Pressure Control Solenoid Valve High Control
10 | BU | 5508 | Shift Pressure Control Solenoid Valve Low Control
11-12 | -- | -- | Not Used
13 | OG | N/A | Low Reference
14 | OG | N/A | Trasnsmission Fluid Temperature Sensor Signal
15 | -- | -- | Not Used
16 | RD | 2880 | Shift Pressure Control Solenoid Valve High Control
17 | YE | 898 | Shift Solenoid Valve 3 High Control
18-20 | -- | -- | Not Used
21 | L-BU | 2527 | Shift Solenoid Valve 5 High Control
22 | PU | 2879 | Shift Solenoid Valve 4 High Control

### Turn Signal/Multifunction Switch X1

#### Connector Part Information

- OEM: 15450317
- Service: 88987843
- Description: 8-Way F Unsealed (WH)

#### Terminal Part Information

- Terminal/Tray: SNAC-A03T-M040/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-12 (BU)

#### Turn Signal/Multifunction Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 1551 | Ground
2 | 0.35 WH | 103 | Headlamp Switch On Signal
3 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
4 | 0.35 D-GN | 306 | Headlamp Switch Off Signal
5-8 | -- | -- | Not Used

### Turn Signal/Multifunction Switch X2

#### Connector Part Information

- OEM: 15393435
- Service: 88986438
- Description: 10-Way F Micro 64 (GY)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Turn Signal/Multifunction Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK/WH | 1551 | Ground
C | 0.35 BN | 1356 | Flash To Pass Switch Signal
D | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
E | -- | -- | Not Used
F | 0.35 BK/WH | 1551 | Ground
G | 0.35 L-BU/WH | 1414 | Left Front Turn Signal Switch Signal
H | 0.35 D-BU/WH | 1415 | Right Front Turn Signal Switch Signal
J-K | -- | -- | Not Used

### Video Display (UUC)

#### Connector Part Information

- OEM: 7283-9088-30
- Service: See Catalog
- Description: 10-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Video Display (UUC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 6975 | DVD Video Signal (+)
2 | 0.5 WH/BK | 5335 | DVD Video Signal (-)
3-5 | -- | -- | Not Used
6 | 0.5 BK/WH | 1551 | Ground
7 | 0.5 RD/WH | 2340 | Battery Positive Voltage
8 | 0.5 WH | 1487 | Antenna Enable Signal
9 | 0.5 PK/BK | 5844 | Video Bright Control
10 | 0.5 BN/WH | 5846 | Video Power Mode Signal

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 YE | 873 | Low Reference
B | 0.8 L-BU | 830 | Left Front Wheel Speed Sensor Signal

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

- OEM: 12162343
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Wheel Speed Sensor (WSS) - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 885 | Low Reference
B | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 TN | 833 | Low Reference
B | 0.8 D-GN | 872 | Right Front Wheel Speed Sensor Signal

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

- OEM: 12162343
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Wheel Speed Sensor (WSS) - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 883 | Low Reference
B | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal

### Window Motor - Driver

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F YESC/USCAR Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Motor - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 165 | Power Window Motor Left Front Down Control
2 | 2.0 D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Left Rear

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F YESC/USCAR Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Motor - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 669 | Power Window Motor Left Rear Down Control
2 | 2.0 D-BU | 668 | Power Window Motor Left Rear Up Control

### Window Motor - Passenger

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F YESC/USCAR Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Motor - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 167 | Power Window Master Switch Right Front Down Signal
2 | 2.0 D-BU | 166 | Power Window Master Switch Right Front Up Signal

### Window Motor - Right Rear

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F YESC/USCAR Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Motor - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 671 | Power Window Motor Right Rear Down Control
2 | 2.0 D-BU | 670 | Power Window Motor Right Rear Up Control

### Window Switch - Driver

#### Connector Part Information

- OEM: 12191825
- Service: 15306048
- Description: 8-Way Metri-Pack 280 Series (BN)

#### Terminal Part Information

- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal
B | 2.0 D-BU | 164 | Power Window Motor Left Front Up Control
C | 2.0 BN | 165 | Power Window Motor Left Front Down Control
D | 2.0 YE | 143 | Ignition Voltage
E | 2.0 PU | 169 | Power Window Master Switch Left Rear Down Signal
F | 2.0 BK | 650 | Ground
G | 2.0 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
H | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal

### Window Switch - Left Rear

#### Connector Part Information

- OEM: 6098-0245
- Service: See Catalog
- Description: 6-Way F HD Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Switch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 669 | Power Window Motor Left Rear Down Control
2 | 2.0 PU | 169 | Power Window Master Switch Left Rear Down Signal
3 | -- | -- | Not Used
4 | 2.0 D-BU | 668 | Power Window Motor Left Rear Up Control
5 | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal
6 | 2.0 D-GN | 168 | Power Window Master Switch Left Rear Up Signal

### Window Switch - Passenger

#### Connector Part Information

- OEM: 15326924
- Service: 15306174
- Description: 8-Way F GT 280 (BK)

#### Terminal Part Information

- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 2.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
C | 2.0 TN | 167 | Power Window Master Switch Right Front Down Signal
D | 2.0 YE | 143 | Ignition Voltage
E | -- | -- | Not Used
F | 2.0 L-GN | 170 | Power Window Master Switch Right Rear Up Signal
G | 2.0 BK | 650 | Ground
H | 2.0 PU | 171 | Power Window Master Switch Right Rear Down Signal

### Window Switch - Right Rear

#### Connector Part Information

- OEM: 6098-0245
- Service: See Catalog
- Description: 6-Way F HD Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Window Switch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BN | 671 | Power Window Motor Right Rear Down Control
2 | 2.0 PU | 171 | Power Window Master Switch Right Rear Down Signal
3 | -- | -- | Not Used
4 | 2.0 D-BU | 670 | Power Window Motor Right Rear Up Control
5 | 2.0 D-BU | 1307 | Power Window Master Switch Lockout Signal
6 | 2.0 D-GN | 170 | Power Window Master Switch Right Rear Up Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: 12185025
- Service: 89046634
- Description: 2-Way F Mini Timer (BK)

#### Terminal Part Information

- Terminal/Tray: 60012941/21
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12122378/J-35616-4A (PU)

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-GN | 392 | Rear Window Washer Pump Control
2 | 0.8 D-BU | 298 | Rear Window Washer Pump Control

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 12084891
- Service: 15305874
- Description: 5-Way F Metri-Pack 280 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
C | 1.0 BK | 1250 | Ground
D | 1.0 PU | 92 | Windshield Wiper Motor High Speed
E | 1.0 D-GN | 95 | Windshield Wiper Motor Low Speed

### Windshield Wiper/Washer Switch

#### Connector Part Information

- OEM: 12059800
- Service: 15306169
- Description: 5-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Wiper/Washer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 PK | 94 | Rear Wiper Switch Signal
C | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
D | 0.35 BK/WH | 1251 | Ground
E | 0.35 L-BU | 1714 | Windshield Wiper Switch Low Signal

### Yaw and Lateral Accelerometer Sensor

#### Connector Part Information

- OEM: 1-967640-1
- Service: See Catalog
- Description: 4-Way F MQS Socket Housing Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Yaw and Lateral Accelerometer Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/BK | 6045 | Low Reference
2 | 0.5 WH/BK | 6436 | CAN Bus Low Terminated Serial Data
3 | 0.5 BN/WH | 6437 | CAN Bus High Terminated Serial Data
4 | 0.5 GY | 6044 | 12-Volt Reference