For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat belt adjuster cover, bolt and guide ONLY, from the center pillar. Refer to Seat Belt Retractor Pretensioner Replacement - Front .
2. Remove the center pillar lower garnish molding. Refer to Center Pillar Lower Garnish Molding Replacement .

1 | Center Pillar Upper Trim Panel Tip Starting at the top, gently pull on the garnish molding to disengage the attaching clips.