For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Instrument Panel Outer Trim Cover Refer to Instrument Panel Outer Trim Cover Replacement .
2 | Instrument Panel Air Outlet Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Instrument Panel Air Outlet - Right

#### Procedure

Use a flat-bladed plastic trim to in order to release the outlet from the I/P.