For 1990-2009 cars

### Removal Procedure

1. Set the parking brake.
2. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
3. Ensure that the shift control range select lever is in the park (P) position.
4. Disconnect the shift control cable (1) from the transmission range selector lever.
5. Depress the range selector cable retainer clip tabs (2) and remove the range selector cable from the range selector cable bracket.
6. Remove the shift control lever knob. Refer to Transmission Control Lever Knob Replacement.
7. Remove the console. Refer to Console Replacement.
8. Disconnect the shift control cable (1) from the shift control range select lever pin.
9. Depress the shift control cable retainer clip tabs and remove the cable (2) from the shift control.
10. Remove the shift control cable grommet from the cowl.
11. Note the shift control cable routing and remove the shift control cable from the vehicle.

### Installation Procedure

Note: Ensure the shift control cable is routed exactly as originally positioned in the vehicle to avoid coming into contact with potential hazards such as hot, sharp, and moving objects.

1. Secure the shift control cable grommet by pressing the cable into the pass-thru hole in the cowl.
2. Ensure that the shift control range select lever is in the park (P) position.
3. Install the shift control cable (2) to the shift control.
4. Install the shift control cable (1) onto the shift control range select lever pin.
5. Install the console. Refer to Console Replacement.
6. Install the shift control lever knob. Refer to Transmission Control Lever Knob Replacement.
7. Install the shift control cable (2) to the range selector cable bracket. Ensure the range selector cable retaining tabs fully engage the range selector cable bracket.
8. Connect the range selector cable (1) to the transmission range selector lever.
9. Adjust the range selector cable. Refer to Range Selector Lever Cable Adjustment.
10. Enable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
11. Release the parking brake.