For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the right wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement.

1 | Transfer Case Brace Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Tighten fasteners in specified sequential order. Tighten
50 N·m (37 lb ft)

2 | Transfer Case Brace Bolt Tip Tighten fasteners in specified sequential order. Tighten 50 N·m (37 lb ft)
3 | Transfer Case Brace Bolt (Qty: 3) Tip Tighten fasteners in specified sequential order. Tighten 23 N·m (17 lb ft)
4 | Transfer Case Brace