For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Washer Solvent Container Screws | 2.5 N·m | 22 lb in
Wiper Arm Retaining Nut - Front | 28 N·m | 21 lb ft
Wiper Arm Retaining Nut - Rear | 10 N·m | 89 lb in
Wiper Module Bolts to Plenum - Front | 12 N·m | 9 lb ft
Wiper Motor Bolts - Rear | 10 N·m | 89 lb in
Wiper Motor to Crank Nut | 9 N·m | 80 lb in
Wiper Motor to Module Bolts | 9 N·m | 80 lb in