For 1990-2009 cars

## Secondary Camshaft Drive Chain Installation - Right Side Second Design - 2007

1. Ensure that the crankshaft is in the stage 2 timing drive assembly position (1).
2. Install the right secondary camshaft drive chain.
3. Place the secondary camshaft drive chain around the right camshaft intermediate drive chain idler outer sprocket, aligning the timing camshaft drive chain link (1) with the alignment access hole (2) made in the right camshaft intermediate drive chain idler inner sprocket.
4. Wrap the secondary camshaft drive chain around both right actuator drive sprockets.
5. Ensure there are 10 links (1) between the timing camshaft drive chain links for the camshaft position actuator sprockets.
6. Align the right exhaust camshaft position actuator sprocket alignment triangle mark (1) with the timing camshaft drive chain link (2).
7. Align the right intake camshaft position actuator sprocket alignment triangle mark (2) with the timing camshaft drive chain link (1).
8. There will be 22 links (1) between the right camshaft intermediate drive chain idler timing camshaft drive chain link and each right camshaft position actuator sprocket timing camshaft drive chain link.

## Secondary Camshaft Drive Chain Installation - Right Side First Design - 2007

1. Ensure that the crankshaft is in the stage 2 timing drive assembly position (1).
2. Install the right secondary camshaft drive chain.
3. Place the secondary camshaft drive chain around the right camshaft intermediate drive chain idler outer sprocket, aligning the timing camshaft drive chain link (1) with the alignment access hole (2) made in the right camshaft intermediate drive chain idler inner sprocket.
4. Wrap the secondary camshaft drive chain around both right actuator drive sprockets.
5. Ensure there are 7 links (1) between the timing camshaft drive chain links for the camshaft position actuator sprockets.
6. Align the right exhaust camshaft position actuator sprocket alignment triangle mark (1) with the timing camshaft drive chain link (2).
7. Align the right intake camshaft position actuator sprocket alignment triangle mark (2) with the timing camshaft drive chain link (1).
8. There will be 18 links (1) between the right camshaft intermediate drive chain idler timing camshaft drive chain link and each right camshaft position actuator sprocket timing camshaft drive chain link.