For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .
2. Remove the turn signal multifunction switch. Refer to Turn Signal Multifunction Switch Replacement .
3. Remove the wipers/washer switch. Refer to Windshield Wiper and Washer Switch Replacement .

1 | Multifunction Turn Signal Switch Housing

#### Procedure

Release the 2 retaining tabs to remove the housing from the steering column.