For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Recliner Handle Tip Pull firmly forward on the handle to remove.
2 | Front Seat Outer Adjuster Finish Cover Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Seat Outer Adjuster Finish Cover Tip Disconnect the electrical connector.
4 | Front Seat Adjuster Switch Knob Tip Using a flat-bladed tool, remove the knob from the seat switch.
5 | Front Seat Adjuster Switch Tip Use a small flat-bladed tool to remove the switch from the trim panel.