For 1990-2009 cars

### Removal Procedure

1. Remove the front wiper motor. Refer to Windshield Wiper System Module Replacement .
2. Remove the grommets and the bushings from the module.

### Installation Procedure

Important: The metal bushing inserts need to be installed with the flat side underneath the module bolts.

1. Install the grommets and the bushings to the module.
2. Install the front wiper motor. Refer to Windshield Wiper System Module Replacement .