For 1990-2009 cars

Connector 1: | C101 Body Harness to the Forward Lamp Harness
Connector 2: | C102 Body Harness to the Battery Cable Harness
Connector 3: | C103 LF Wheel Speed Sensor Harness to the Body Harness
Connector 4: | C104 RF Wheel Speed Sensor Harness to the Body Harness
Connector 5: | C105 Engine Harness to the Fuel Injector Harness
Connector 6: | C106 Body Harness to the Engine Harness
Connector 7: | C108 Forward Lamp Harness to the Right Cooling Fan Harness
Connector 8: | C109 Forward Lamp Harness to the Left Headlamp Harness
Connector 9: | C110 Forward Lamp Harness to the Right Headlamp Harness
Connector 10: | C202 Console Harness to the I/P Harness (UUC w/C69)
Connector 11: | C203 I/P Harness to the Console Harness (C69 w/o UUC)
Connector 12: | C204 I/P Harness to the Body Harness
Connector 13: | C206 I/P Harness to the Body Harness
Connector 14: | C207 Console Harness to the I/P Harness (UUC w/o C69)
Connector 15: | C210 I/P Harness to the Body Harness
Connector 16: | C214 Passenger Airbag Jumper Harness to the I/P Harness
Connector 17: | C216 I/P Harness to the HVAC Harness
Connector 18: | C218 I/P Harness to the Body Harness
Connector 19: | C219 Body Harness to the I/P Harness
Connector 20: | C223 Sunload/Ambient Light Sensor Harness to the I/P Harness
Connector 21: | C226 I/P Harness to the Shifter Jumper Harness
Connector 22: | C275 I/P Harness to the Steering Wheel Module Coil Harness
Connector 23: | C276 I/P Harness to the Steering Wheel Module Coil Harness
Connector 24: | C277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness
Connector 25: | C305 Console Harness to the Body Harness
Connector 26: | C307 Body Harness to the I/P Harness (C69)
Connector 27: | C308 Body Harness to the Power Seat Harness (AG1 w/o KA1)
Connector 28: | C308 Body Harness to the Driver Seat Harness (KA1)
Connector 29: | C309 Body Harness to the Passenger Seat Harness (w/o KA1)
Connector 30: | C309 Body Harness to the Passenger Seat Harness (KA1)
Connector 31: | C310 Body Harness to the Fuel Sender Harness
Connector 32: | C311 Headliner Harness to the Sunshade Harness (UUC)
Connector 33: | C312 Driver Seat Harness to the Power Seat Harness (AG1 w/KA1)
Connector 34: | C313 Passenger Presence Harness to the Passenger Seat Harness
Connector 35: | C314 Headliner Harness to the Sunroof Harness (CF5)
Connector 36: | C400 Body Harness to the Chassis Harness
Connector 37: | C403 Body Harness to the Left Tail Lamp Harness
Connector 38: | C404 Body Harness to the Right Tail Lamp Harness
Connector 39: | C409 Body Harness to the Trailer Jumper Harness (V92)
Connector 40: | C410 Trailer Harness to the Trailer Jumper Harness (V92)
Connector 41: | C412 Headliner Harness to the I/P Harness (UUC)
Connector 42: | C415 Headliner Harness to the Body Harness
Connector 43: | C417 Headliner Harness to the Body Harness (U3U)
Connector 44: | C419 Body Harness to the Rear HVAC Harness (C69)
Connector 45: | C420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)
Connector 46: | C421 Body Harness to the Right Inflatable Restraint Roof Rail Module Harness (ASF)
Connector 47: | C500 Body Harness to the LF Door Harness
Connector 48: | C600 Body Harness to the RF Door Harness
Connector 49: | C700 Body Harness to the LR Door Harness
Connector 50: | C800 Body Harness to the RR Door Harness
Connector 51: | C900 Body Harness to the Liftgate Harness
Connector 52: | C901 Body Harness to the Liftgate Harness
Connector 53: | C906 Licence Lamp Harness to the Liftgate Harness

### C101 Body Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 7283-5684-10
- Service: See Catalog
- Description: 8-Way F Receptacle 1.5 Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5684-10
- Service: See Catalog
- Description: 8-Way M 1.5 Sealed (D-GY)

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 7, 8
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 6
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 7, 8
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C101 Body Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (UH9) | 1 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (UH9)
2 | YE | 61 | Low Reference (UH9) | 2 | YE | 61 | Low Reference (UH9)
3 | TN/OG | 5045 | Discriminating Sensor - Low Reference | 3 | TN/OG | 5045 | Discriminating Sensor - Low Reference
4 | YE | 354 | Discriminating Sensor - Signal | 4 | YE | 354 | Discriminating Sensor - Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BK | 1250 | Ground | 6 | BK | 1250 | Ground
7 | GY | 5600 | Right Front Discriminating Sensor Low Reference | 7 | GY | 5600 | Right Front Discriminating Sensor Low Reference
8 | D-GN | 1409 | Discriminating Sensor - Right - Signal | 8 | D-GN | 1409 | Discriminating Sensor - Right - Signal

### C102 Body Harness to the Battery Cable Harness

#### Connector Part Information

- OEM: 7283-5548-30
- Service: 88953306
- Description: 2-Way F YESC Weather Pack (BK)

#### Connector Part Information

- OEM: 7282-5548-30
- Service: 88953303
- Description: 2-Way M YESC Weather Pack (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C102 Body Harness to the Battery Cable Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 50 | Ground | 1 | BK | 50 | Ground
2 | -- | -- | Not Used | 2 | -- | -- | Not Used

### C103 LF Wheel Speed Sensor Harness to the Body Harness

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12162000
- Service: 12167120
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### C103 LF Wheel Speed Sensor Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YE | 873 | Left Front Wheel Speed Sensor Low Reference | A | YE | 873 | Left Front Wheel Speed Sensor Low Reference
B | L-BU | 830 | Left Front Wheel Speed Sensor Signal | B | L-BU | 830 | Left Front Wheel Speed Sensor Signal

### C104 RF Wheel Speed Sensor Harness to the Body Harness

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12162000
- Service: 12167120
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### C104 RF Wheel Speed Sensor Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 833 | Right Front Wheel Speed Sensor Low Reference | A | TN | 833 | Right Front Wheel Speed Sensor Low Reference
B | D-GN | 872 | Right Front Wheel Speed Sensor Signal | B | D-GN | 872 | Right Front Wheel Speed Sensor Signal

### C105 Engine Harness to the Fuel Injector Harness

#### Connector Part Information

- OEM: 1-967189-1
- Service: See Catalog
- Description: 10-Way F Timer Junior Power Timer Sealed (BK)

#### Connector Part Information

- OEM: 1-962352-1
- Service: See Catalog
- Description: 10-Way M Junior Power Timer Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C105 Engine Harness to the Fuel Injector Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | 5291 | Ignition 1 Voltage | 1 | WH | 5291 | Ignition 1 Voltage
2 | PK/BK | 5292 | Ignition 1 Voltage | 2 | WH | 5292 | Ignition 1 Voltage
3 | TN | 1744 | Fuel Injector 1 Control | 3 | TN | 1744 | Fuel Injector 1 Control
4 | PK/BK | 1746 | Fuel Injector 3 Control | 4 | PK/BK | 1746 | Fuel Injector 3 Control
5 | TN/WH | 845 | Fuel Injector 5 Control | 5 | TN/WH | 845 | Fuel Injector 5 Control
6 | L-GN/BK | 1745 | Fuel Injector 2 Control | 6 | L-GN/BK | 1745 | Fuel Injector 2 Control
7 | L-BU/BK | 844 | Fuel Injector 4 Control | 7 | L-BU/BK | 844 | Fuel Injector 4 Control
8 | YE/BK | 846 | Fuel Injector 6 Control | 8 | YE/BK | 846 | Fuel Injector 6 Control
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used

### C106 Body Harness to the Engine Harness

#### Connector Part Information

- OEM: 7283-5546-30
- Service: See Catalog
- Description: 12-Way F 1.5 Series Sealed (BK)

#### Connector Part Information

- OEM: 7282-5545-30
- Service: See Catalog
- Description: 12-Way M 1.5 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C106 Body Harness to the Engine Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 1589 | Fuel Level Sensor Signal [- Primary] | 1 | PU | 1589 | Fuel Level Sensor Signal [- Primary]
2 | PU | 1272 | Low Reference | 2 | PU | 1272 | Low Reference
3 | L-BU | 1162 | APP Sensor 2 Signal | 3 | L-BU | 1162 | APP Sensor 2 Signal
4 | WH/BK | 1164 | 5-Volt Reference | 4 | WH/BK | 1164 | 5-Volt Reference
5 | BN | 1271 | Low Reference | 5 | BN | 1271 | Low Reference
6 | D-GN | 890 | Fuel Tank Pressure Sensor Signal | 6 | D-GN | 890 | Fuel Tank Pressure Sensor Signal
7 | GY | 2709 | 5-Volt Reference | 7 | GY | 2709 | 5-Volt Reference
8 | D-BU | 1161 | APP Sensor 1 Signal | 8 | D-BU | 1161 | APP Sensor 1 Signal
9 | TN | 1274 | 5-Volt Reference | 9 | TN | 1274 | 5-Volt Reference
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 11 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | TN | 2501 | High Speed GMLAN Serial Data Bus- | 12 | TN | 2501 | High Speed GMLAN Serial Data Bus-

### C108 Forward Lamp Harness to the Right Cooling Fan Harness

#### Connector Part Information

- OEM: 7283-5596-10
- Service: 88953307
- Description: 2-Way F YESC/USCAR Class III (D-GY)

#### Connector Part Information

- OEM: 7282-5596-10
- Service: 88953304
- Description: 2-Way M 250 Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Terminal/Tray: 7114-4142-02/10
- Core/Insulation Crimp: A/3
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### C108 Forward Lamp Harness to the Right Cooling Fan Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 409 | Cooling Fan Motor Supply Voltage | 1 | L-BU | 409 | Cooling Fan Motor Supply Voltage
2 | BK | 1250 | Ground | 2 | BK | 1250 | Ground

### C109 Forward Lamp Harness to the Left Headlamp Harness

#### Connector Part Information

- OEM: 15326822
- Service: 19151498
- Description: 5-Way F GT 150 Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C109 Forward Lamp Harness to the LH Headlamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 1250 | Ground | A | BK | 1250 | Ground
B | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | B | WH | 711 | Left Headlamp High Beam Supply Voltage
C | YE | 712 | Left Headlamp Low Beam Supply Voltage | C | D-GN | 712 | Left Headlamp Low Beam Supply Voltage
D | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage | D | D-BU | 1314 | Left Front Turn Signal Lamp Supply Voltage
E | PU | 709 | Left Park Lamp Supply Voltage | E | L-GN | 709 | Left Park Lamp Supply Voltage

### C110 Forward Lamp Harness to the Right Headlamp Harness

#### Connector Part Information

- OEM: 15326822
- Service: 19151498
- Description: 5-Way F GT 150 Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C110 Forward Lamp Harness to the Right Headlamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 1250 | Ground | A | BK | 1250 | Ground
B | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | B | WH | 311 | Right Headlamp High Beam Supply Voltage
C | TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | C | D-GN | 312 | Right Headlamp Low Beam Supply Voltage
D | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage | D | D-BU | 1315 | Right Front Turn Signal Lamp Supply Voltage
E | BN/WH | 309 | Right Park Lamp Supply Voltage | E | L-GN | 309 | Right Park Lamp Supply Voltage

### C202 Console Harness to the I/P Harness (UUC w/C69)

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F Receptacle 1.5 2.8 6.3 (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M 6.3 Unsealed (L-GY)

#### Terminal Part Information

- Pins: 2, 3, 4, 5, 6, 7, 10, 11, 12, 13, 14, 15
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 2, 3, 4, 5, 6, 7, 10, 11, 12, 13, 14, 15
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C202 Console Harness to the I/P Harness (UUC w/C69)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | GY | 8 | Instrument Panel Lamp Supply Voltage | 2 | GY | 8 | Instrument Panel Lamp Supply Voltage
3 | BARE | 5346 | Video Drain Wire | 3 | BARE | 5346 | Video Drain Wire
4 | PU | 2056 | Auxiliary Video High Signal | 4 | PU | 2056 | Auxiliary Video High Signal
5 | WH | 2058 | Auxiliary Audio Right Signal | 5 | WH | 2058 | Auxiliary Audio Right Signal
6 | YE | 2059 | Auxiliary Audio Left Signal | 6 | YE | 2059 | Auxiliary Audio Left Signal
7 | BARE | 5345 | Drain Wire | 7 | BARE | 5345 | Drain Wire
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Not Used
10 | OG | 2615 | Auxiliary Mode Door Control | 10 | OG | 2615 | Auxiliary Mode Door Control
11 | GY | 720 | Low Reference | 11 | GY/BK | 1798 | Low Reference
GY | 720 | Low Reference
12 | GY | 597 | 5-Volt Reference | 12 | GY | 596 | 5-Volt Reference
GY | 597 | 5-Volt Reference
13 | YE | 2214 | Auxiliary Air Temperature Door Control | 13 | YE | 2214 | Auxiliary Air Temperature Door Control
14 | BK/WH | 1551 | Ground | 14 | BK/WH | 1551 | Ground
15 | PU/WH | 760 | Auxiliary Blower Motor Speed Control | 15 | PU/WH | 760 | Auxiliary Blower Motor Speed Control
16-26 | -- | -- | Not Used | 16-26 | -- | -- | Not Used

### C203 I/P Harness to the Console Harness (C69 w/o UUC)

#### Connector Part Information

- OEM: 7283-3441-40
- Service: See Catalog
- Description: 8-Way F 1.5 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-3441-40
- Service: See Catalog
- Description: 8-Way M 1.5 Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C203 I/P Harness to the Console Harness (C69 w/o UUC)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY | 8 | Instrument Panel Lamp Supply Voltage | 1 | GY | 8 | Instrument Panel Lamp Supply Voltage
2 | BK/WH | 1551 | Ground | 2 | BK/WH | 1551 | Ground
3 | OG | 2615 | Auxiliary Mode Door Control | 3 | OG | 2615 | Auxiliary Mode Door Control
4 | GY | 720 | Low Reference | 4 | GY | 720 | Low Reference
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | GY | 597 | 5-Volt Reference | 6 | GY | 597 | 5-Volt Reference
7 | YE | 2214 | Auxiliary Air Temperature Door Control | 7 | YE | 2214 | Auxiliary Air Temperature Door Control
8 | PU/WH | 760 | Auxiliary Blower Motor Speed Control | 8 | PU/WH | 760 | Auxiliary Blower Motor Speed Control

### C204 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 88987998
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C204 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | TN | 3021 | Steering Wheel Module - Stage1 - High Control | A1 | TN | 3021 | Steering Wheel Module - Stage1 - High Control
A2 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control | A2 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
B1 | WH | 3023 | Steering Wheel Module - Stage2 - High Control | B1 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
B2 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control | B2 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control

### C206 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F Receptacle 1.5 2.8 6.3 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M 6.3 Unsealed (L-GY)

#### Terminal Part Information

- Pins: 26
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3, 4, 6, 13, 14, 15, 16, 18, 19, 21, 22, 23, 24, 25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 9, 11, 12, 10, 13, 14, 15, 16
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 26
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 11, 12, 13, 14, 15, 16
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 3, 4, 6, 13, 14, 15, 16, 18, 19, 21, 22, 23, 24, 25
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C206 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 3 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
4 | TN | 2501 | High Speed GMLAN Serial Data Bus- | 4 | TN | 2501 | High Speed GMLAN Serial Data Bus-
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | OG | 5748 | Radio Audio Mute Signal (U65) | 6 | OG | 5748 | Radio Audio Mute Signal (U65)
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used
9 | TN | 1875 | Right Front Speaker Output (+) | 9 | L-GN/WH | 512 | Right Front Low Level Audio Signal (+) (U65)
L-GN | 200 | Right Front Speaker Output (+) (Except U65)
10 | TN/WH | 1985 | 5-Volt Reference | 10 | L-GN | 1948 | Right Front Low Level Audio Signal (-) (U65)
D-GN | 117 | Right Front Speaker Output (-) (Except U65)
11 | GY | 118 | Left Front Speaker Output (-) | 11 | D-GN | 1947 | Left Front Low Level Audio Signal (-) (U65)
GY | 118 | Left Front Speaker Output (-) (Except U65)
12 | TN | 201 | Left Front Speaker Output (+) | 12 | TN | 511 | Left Front Low Level Audio Signal (+) (U65)
201 | Left Front Speaker Output (+) (Except U65)
13 | BN | 199 | Left Rear Speaker Output (+) | 13 | BN/WH | 599 | Left Rear Low Level Audio Signal (+) (U65)
BN | 199 | Left Rear Speaker Output (+) (Except U65)
14 | BN | 1999 | Left Rear Low Level Audio Signal (-) | 14 | YE | 116 | Left Rear Speaker Output (-) (Except U65)
BN | 1999 | Left Rear Low Level Audio Signal (-) (U65)
15 | L-BU | 115 | Right Rear Speaker Output (-) | 15 | L-BU | 115 | Right Rear Speaker Output (-) (Except U65)
TN | 1946 | Right Rear Low Level Audio Signal (-) (U65)
16 | D-BU | 46 | Right Rear Speaker Output (+) (Except UK6) | 16 | D-BU | 546 | Right Rear Low Level Audio Signal (+) (U65)
D-BU | 46 | Right Rear Speaker Output (+) (Except U65)
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | BARE | 1489 | Drain Wire (U3U) | 18 | BARE | 1489 | Drain Wire (U3U)
19 | GY | 655 | Cellular Microphone Signal (U3U) | 19 | GY | 655 | Cellular Microphone Signal (U3U)
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | TN/WH | 372 | Remote Radio Audio Output (-) (U2K) | 21 | TN/WH | 372 | Remote Radio Audio Output (-) (U2K)
22 | BN/WH | 367 | Remote Radio Left Audio Signal (U2K) | 22 | BN/WH | 367 | Remote Radio Left Audio Signal (U2K)
23 | GY | 388 | Remote Radio Right Audio Signal (U2K) | 23 | GY | 388 | Remote Radio Right Audio Signal (U2K)
24 | D-GN/WH | 368 | Remote Radio Right Audio Signal (U2K) | 24 | D-GN/WH | 368 | Remote Radio Right Audio Signal (U2K)
25 | BARE | 6759 | Discrete Audio Drain Wire (U2K) | 25 | BARE | 6759 | Discrete Audio Drain Wire (U2K)
26 | D-GN | 5060 | Low Speed GMLAN Serial Data | 26 | D-GN | 5060 | Low Speed GMLAN Serial Data

### C207 Console Harness to the I/P Harness (UUC w/o C69)

#### Connector Part Information

- OEM: 7283-6387-40
- Service: See Catalog
- Description: 6-Way F (L-GY)

#### Connector Part Information

- OEM: 7282-6561-40
- Service: See Catalog
- Description: 6-Way M Unsealed (L-GY)

#### Terminal Part Information

- Pins: 6, 1, 2, 3, 4, 5
- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: Pins: 6 : H/H
- Core/Insulation Crimp: Pins: 1, 2, 3, 4, 5 : J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 5
- Terminal/Tray: 7114-4721-02/14
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

- Pins: 6
- Terminal/Tray: 7114-4720-02/14
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### C207 Console Harness to the I/P Harness (UUC w/o C69)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BARE | 5346 | Video Drain Wire | 1 | BARE | 5346 | Video Drain Wire
2 | PU | 2056 | Auxiliary Video High Signal | 2 | PU | 2056 | Auxiliary Video High Signal
3 | WH | 2058 | Auxiliary Audio Right Signal | 3 | WH | 2058 | Auxiliary Audio Right Signal
4 | YE | 2059 | Auxiliary Audio Left Signal | 4 | YE | 2059 | Auxiliary Audio Left Signal
5 | BARE | 5345 | Drain Wire | 5 | BARE | 5345 | Drain Wire
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### C210 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-8391-40
- Service: See Catalog
- Description: 26-Way F Receptacle 1.5 2.8 6.3 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-8391-40
- Service: See Catalog
- Description: 26-Way M 6.3 Unsealed (L-GY)

#### Terminal Part Information

- Pins: 26, 17
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 8
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2, 3, 4, 6, 7, 5, 9, 11, 12, 10, 13, 14, 15, 16, 18, 19, 20, 21, 22, 23, 24, 25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 1
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Pins: 8
- Terminal/Tray: 7114-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 26, 17
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 2, 3, 4, 6, 7, 5, 9, 11, 12, 10, 13, 14, 15, 16, 18, 19, 20, 21, 22, 23, 24, 25
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1
- Terminal/Tray: 7114-4121-02/9
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### C210 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | RD/WH | 2740 | Battery Positive Voltage
2 | WH/BK | 6436 | CAN Bus Low Terminated Serial Data | 2 | WH/BK | 6436 | CAN Bus Low Terminated Serial Data
3 | BN/WH | 6437 | CAN Bus High Terminated Serial Data | 3 | BN/WH | 6437 | CAN Bus High Terminated Serial Data
4 | OG/BK | 6045 | Steering Angle Sensor Low Reference | 4 | OG/BK | 6045 | Steering Angle Sensor Low Reference
5 | GY | 6044 | Steering Angle Sensor 5 Volt Reference | 5 | GY | 6044 | Steering Angle Sensor 5 Volt Reference
6 | TN/WH | 6433 | CAN Bus High Serial Data | 6 | TN/WH | 6433 | CAN Bus High Serial Data
7 | L-GN/BK | 6432 | CAN Bus Low Serial Data | 7 | L-GN/BK | 6432 | CAN Bus Low Serial Data
8 | RD/WH | 2540 | Battery Positive Voltage | 8 | RD/WH | 2540 | Battery Positive Voltage
9 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal | 9 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
10 | YE | 61 | Low Reference | 10 | YE | 61 | Low Reference
11 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 11 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | TN | 2501 | High Speed GMLAN Serial Data Bus- | 12 | TN | 2501 | High Speed GMLAN Serial Data Bus-
TN | 2501 | High Speed GMLAN Serial Data Bus-
13 | BN/WH | 419 | MIL Control | 13 | BN/WH | 419 | MIL Control
14 | L-GN | 1499 | Driver Mirror Motor Left/Down Control | 14 | L-GN | 1499 | Driver Mirror Motor Left/Down Control
15 | PU/WH | 889 | Passenger Mirror Motor Down Control | 15 | PU/WH | 889 | Passenger Mirror Motor Down Control
16 | OG/WH | 881 | Passenger Mirror Motor Right Control | 16 | OG/WH | 881 | Passenger Mirror Motor Right Control
17 | D-GN/WH | 817 | Vehicle Speed Signal (U3U) | 17 | D-GN/WH | 817 | Vehicle Speed Signal (U3U)
18 | BN | 1271 | Low Reference | 18 | BN | 1271 | Low Reference
19 | D-BU | 1161 | APP Sensor 1 Signal | 19 | D-BU | 1161 | APP Sensor 1 Signal
20 | WH/BK | 1164 | 5-Volt Reference | 20 | WH/BK | 1164 | 5-Volt Reference
21 | TN | 1274 | 5-Volt Reference | 21 | TN | 1274 | 5-Volt Reference
22 | L-BU | 1162 | APP Sensor 2 Signal | 22 | L-BU | 1162 | APP Sensor 2 Signal
23 | PU | 1272 | Low Reference | 23 | PU | 1272 | Low Reference
24 | TN/WH | 33 | Brake Warning Indicator Control | 24 | TN/WH | 33 | Brake Warning Indicator Control
25 | YE | 88 | Driver Mirror Motor Up Control | 25 | YE | 88 | Driver Mirror Motor Up Control
26 | WH | 81 | Driver Mirror Motor Right Control | 26 | WH | 81 | Driver Mirror Motor Right Control

### C214 Passenger Airbag Jumper Harness to the I/P Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 88987998
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C214 Passenger Airbag Jumper Harness to the I/P Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 3025 | I/P Module - Stage 1 - High Control | A1 | YE | 3025 | I/P Module - Stage 1 - High Control
A2 | OG | 3024 | I/P Module - Stage 1 - Low Control | A2 | OG | 3024 | I/P Module - Stage 1 - Low Control
B1 | GY | 3027 | I/P Module - Stage 2 - High Control | B1 | GY | 3027 | I/P Module - Stage 2 - High Control
B2 | PU | 3026 | I/P Module - Stage 2 - Low Control | B2 | PU | 3026 | I/P Module - Stage 2 - Low Control

### C216 I/P Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15332177
- Service: See Catalog
- Description: 16-Way F GT 150 (BK)

#### Connector Part Information

- OEM: 15332182
- Service: 15306371
- Description: 16-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C216 I/P Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WH | 119 | Mode Door Control | A | WH | 119 | Mode Door Control
B | TN/BK | 2274 | Recirculation Door Control Circuit | B | TN/BK | 2274 | Recirculation Door Control Circuit
C | TN | 2273 | Mode Door Control | C | TN | 2273 | Mode Door Control
D | TN | 516 | Upper Left Air Temperature Sensor Signal | D | TN | 516 | Upper Left Air Temperature Sensor Signal
E | TN | 520 | Lower Right Air Temperature Sensor Signal | E | TN | 520 | Lower Right Air Temperature Sensor Signal
F | YE | 1791 | Air Temperature Door Control Low Reference | F | YE | 1791 | Low Reference
G | PU | 1838 | Recirculation Door Position Signal | G | PU | 1838 | Recirculation Door Position Signal
H | L-BU | 733 | Air Temperature Door Position Signal | H | L-BU | 733 | Air Temperature Door Position Signal
J | L-GN | 2275 | Mode Door Position Signal | J | L-GN | 2275 | Mode Door Position Signal
K | D-GN | 1614 | Recirculation Door Control | K | D-GN | 1614 | Recirculation Door Control
L | D-BU | 1199 | Air Temperature Door Control | L | D-BU | 1199 | Air Temperature Door Control
M | L-BU | 1316 | Air Temperature Door Control | M | L-BU | 1316 | Air Temperature Door Control
N | GY | 598 | 5-Volt Reference | N | GY | 598 | 5-Volt Reference
P | WH | 2622 | 5-Volt Reference | P | WH | 2622 | 5-Volt Reference
R | TN | 552 | Low Reference | R | TN | 552 | Low Reference
S | YE | 61 | Low Reference | S | YE | 61 | Low Reference

### C218 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: --
- Description: 4-Way M Metri-Pack 280 (YE)

#### Terminal Part Information

- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: --
- Core/Insulation Crimp: --
- Release Tool/Test Probe: --

#### C218 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 3025 | I/P Module - Stage 1 - High Control | A1 | YE | 3025 | I/P Module - Stage 1 - High Control
A2 | OG | 3024 | I/P Module - Stage 1 - Low Control | A2 | OG | 3024 | I/P Module - Stage 1 - Low Control
B1 | GY | 3027 | I/P Module - Stage 2 - High Control | B1 | GY | 3027 | I/P Module - Stage 2 - High Control
B2 | PU | 3026 | I/P Module - Stage 2 - Low Control | B2 | PU | 3026 | I/P Module - Stage 2 - Low Control

### C219 Body Harness to the I/P Harness

#### Connector Part Information

- OEM: GT13GM-1/1S-HU
- Service: See Catalog
- Description: 3-Way F GT13 Coaxial Series (GY)

#### Connector Part Information

- OEM: GT13GM-1/1PPHU
- Service: See Catalog
- Description: 3-Way M GT13 Coaxial Series (GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7114-4618-02/27
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-65B (L-BU)

#### C219 Body Harness to the I/P Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | WH | 1487 | Antenna Enable Signal | 1 | WH | 1487 | Antenna Enable Signal
C | BK | 6001 | Antenna RF Signal | C | BK | 6001 | Antenna RF Signal
S | -- | -- | Not Used | S | -- | -- | Not Used

### C223 Sunload/Ambient Light Sensor Harness to the I/P Harness

#### Connector Part Information

- OEM: 7283-6446-40
- Service: See Catalog
- Description: 4-Way F Kaizen YESC Series (GY)

#### Connector Part Information

- OEM: 7282-6446-40
- Service: See Catalog
- Description: 4-Way M Kaizen YESC Series (GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 3
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 2, 4
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C223 Sunload/Ambient Light Sensor Harness to the I/P Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY | 1548 | Passenger Sunload Sensor Signal | 1 | GY | 1548 | Passenger Sunload Sensor Signal
2 | L-BU/BK | 590 | Driver Sunload Sensor Signal | 2 | L-BU/BK | 590 | Driver Sunload Sensor Signal
3 | L-GN/BK | 1137 | DRL Ambient Light Sensor Signal | 3 | L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
4 | BK/WH | 1551 | Ground | 4 | BK/WH | 1551 | Ground

### C226 I/P Harness to the Shifter Jumper Harness

#### Connector Part Information

- OEM: 936268-1
- Service: See Catalog
- Description: 6-Way F 090 Series (WH)

#### Connector Part Information

- OEM: 936271-1
- Service: See Catalog
- Description: 6-Way M 090 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 368083-1/26
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C226 I/P Harness to the Shifter Jumper Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 1375 | Remote Radio Control Supply Voltage | 1 | YE | 1375 | Remote Radio Control Supply Voltage
PU | 1375 | Remote Radio Control Supply Voltage
2 | PU/WH | 5905 | Key Capture/Column Lock Shift Position Signal | 2 | GY | 5905 | Key Capture/Column Lock Shift Position Signal
3 | BK | 1450 | Ground | 3 | BK | 1450 | Ground
4 | PU | 5526 | Tap Up/Tap Down Switch Signal | 4 | BK | 5526 | Tap Up/Tap Down Switch Signal
5 | PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control | 5 | BN | 1630 | Steering Column Key Cylinder Lock Solenoid Control
6 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage | 6 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage

### C275 I/P Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 Series (YE)

#### Connector Part Information

- OEM: 15393425
- Service: --
- Description: 4-Way M Micro-Pack 064 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: --
- Core/Insulation Crimp: --
- Release Tool/Test Probe: --

#### C275 I/P Harness to the Steering Wheel Module Coil Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | 1 | -- | 3020 | Steering Wheel Module - Stage 1 - Low Control
2 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control | 2 | -- | 3021 | Steering Wheel Module - Stage 1 - High Control
3 | PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | 3 | -- | 3022 | Steering Wheel Module - Stage 2 - Low Control
4 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control | 4 | -- | 3023 | Steering Wheel Module - Stage 2 - High Control

### C276 I/P Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Connector Part Information

- OEM: 15393436
- Service: --
- Description: 10-Way M Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: --
- Core/Insulation Crimp: --
- Release Tool/Test Probe: --

#### C276 I/P Harness to the Steering Wheel Module Coil Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-B | -- | -- | Not Used | A-B | -- | -- | Not Used
C | PU | 1375 | Remote Radio Control Supply Voltage | C | -- | 1375 | Remote Radio Control Supply Voltage
D | GY | 1884 | Cruise Control Switch Signal | D | -- | 1884 | Cruise Control Switch Signal
E | D-BU | 1796 | Steering Wheel Controls Signal (UK3) | E | -- | 1796 | Steering Wheel Controls Signal (UK3)
F | GN/WH | 7158 | Cruise Control Indicator Dimming Signal | F | -- | 7158 | Cruise Control Indicator Dimming Signal
G | PU/WH | 7005 | LED Dimming Signal | G | -- | 7005 | LED Dimming Signal
H | -- | -- | Not Used | H | -- | -- | Not Used
J | TN | 28 | Horn Relay Control | J | -- | 28 | Horn Relay Control
K | BK | 1450 | Ground | K | -- | 1450 | Ground

### C277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness

#### Connector Part Information

- OEM: 15393433
- Service: See Catalog
- Description: 10-Way F Micro-Pack 064 Series (BK)

#### Connector Part Information

- OEM: 15393436
- Service: See Catalog
- Description: 10-Way M Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C277 Steering Wheel Controls Harness to the Steering Wheel Module Coil Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-B | -- | -- | Not Used | A-B | -- | -- | Not Used
C | PU | 1375 | Remote Radio Control Supply Voltage | C | PU | 1375 | Remote Radio Control Supply Voltage
D | GY | 1884 | Cruise Control Switch Signal | D | GY | 1884 | Cruise Control Switch Signal
E | D-BU | 1796 | Steering Wheel Controls Signal (UK3) | E | D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | GN/WH | 7158 | Cruise Control Indicator Dimming Signal | F | GN/WH | 7158 | Cruise Control Indicator Dimming Signal
G | PU/WH | 7005 | LED Dimming Signal | G | PU/WH | 7005 | LED Dimming Signal
H | -- | -- | Not Used | H | -- | -- | Not Used
J | TN | 28 | Horn Relay Control | J | TN | 28 | Horn Relay Control
K | BK | 1450 | Ground | K | BK | 1450 | Ground

### C305 Console Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-5565-40
- Service: See Catalog
- Description: 2-Way F 110 Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-5565-40
- Service: See Catalog
- Description: 2-Way M 110 Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C305 Console Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 650 | Ground | 1 | BK | 650 | Ground
2 | RD/WH | 2540 | Battery Positive Voltage | 2 | RD/WH | 2540 | Battery Positive Voltage

### C307 Body Harness to the I/P Harness (C69)

#### Connector Part Information

- OEM: 7283-9088-30
- Service: See Catalog
- Description: 10-Way F Kaizen 0.64 Series (BK)

#### Connector Part Information

- OEM: 7282-9082-30
- Service: See Catalog
- Description: 10-Way M Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4618-02/27
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-65B (L-BU)

#### C307 Body Harness to the I/P Harness (C69)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY/BK | 1798 | Low Reference | 1 | GY/BK | 1798 | Low Reference
2 | GY | 2599 | Auxiliary Mode Door Control | 2 | GY | 2599 | Auxiliary Mode Door Control
3 | GY | 596 | 5-Volt Reference | 3 | GY | 596 | 5-Volt Reference
4 | L-GN/WH | 5729 | Rear Mode Motor Supply Voltage | 4 | L-GN/WH | 5729 | Rear Mode Motor Supply Voltage
5 | OG | 2215 | Auxiliary Mode Door Control | 5 | OG | 2215 | Auxiliary Mode Door Control
6 | PK | 2145 | Air Temperature Switch Signal - Right | 6 | PK | 2145 | Air Temperature Switch Signal - Right
7 | BN | 6555 | Rear Temperature Motor Supply Voltage | 7 | BN | 6555 | Rear Temperature Motor Supply Voltage
8 | GY | 2614 | Auxiliary Air Temperature Door Control | 8 | GY | 2614 | Auxiliary Air Temperature Door Control
9 | GY/BK | 754 | Blower Motor Speed Control | 9 | GY/BK | 754 | Blower Motor Speed Control
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

### C308 Body Harness to the Power Seat Harness (AG1 w/o KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: C, D
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A, B
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C308 Body Harness to the Power Seat Harness (AG1 w/o KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/BK | 542 | Battery Positive Voltage | A | RD/BK | 542 | Battery Positive Voltage
B | BK | 650 | Ground | B | BK | 650 | Ground
C | PK | 5057 | Seat Position Sensor - Low Reference | C | TN/WH | 5057 | Seat Position Sensor - Low Reference
D | D-GN | 5016 | Seat Belt Switch - Left - Signal | D | D-BU | 5016 | Seat Belt Switch - Left - Signal

### C308 Body Harness to the Driver Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326924
- Service: 15306174
- Description: 8-Way F GT 280 (BK)

#### Connector Part Information

- OEM: 15326928
- Service: 15306176
- Description: 8-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: E, G, C, D, F, H
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins: E, G : 2/A
- Core/Insulation Crimp: Pins: C, D, F, H : E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A, B
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C308 Body Harness to the Driver Seat Harness (KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/BK | 542 | Battery Positive Voltage | A | RD/BK | 542 | Battery Positive Voltage
B | BK | 650 | Ground | B | BK | 650 | Ground
C | PK | 5057 | Seat Position Sensor - Low Reference | C | L-GN | 5057 | Seat Position Sensor - Low Reference
D | D-GN | 5016 | Seat Belt Switch - Left - Signal | D | BK | 5016 | Seat Belt Switch - Left - Signal
E | PU | 2424 | Driver Heated Seat Back Element Control | E | PU | 2424 | Driver Heated Seat Back Element Control
F | YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal | F | YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal
G | PK | 2077 | Heated Seat Cushion Element Supply Voltage | G | PK | 2077 | Heated Seat Cushion Element Supply Voltage
H | YE | 2080 | Driver Heated Seat Cushion Temperature Sensor Low Reference | H | YE | 2080 | Driver Heated Seat Cushion Temperature Sensor Low Reference

### C309 Body Harness to the Passenger Seat Harness (w/o KA1)

#### Connector Part Information

- OEM: 15332138
- Service: See Catalog
- Description: 5-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332139
- Service: See Catalog
- Description: 5-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C309 Body Harness to the Passenger Seat Harness (w/o KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 840 | Battery Positive Voltage | A | OG | 840 | Battery Positive Voltage
B | BK/WH | 651 | Ground | B | BK | 651 | Ground
C | PK | 5057 | Seat Position Sensor - Low Reference | C | PK | 5057 | Seat Position Sensor - Low Reference
D | OG | 1362 | Seat Belt Switch - Right - Signal | D | RD | 1362 | Seat Belt Switch - Right - Signal
E | D-GN | 5060 | Low Speed GMLAN Serial Data | E | D-GN | 5060 | Low Speed GMLAN Serial Data

### C309 Body Harness to the Passenger Seat Harness (KA1)

#### Connector Part Information

- OEM: 15332161
- Service: 15306416
- Description: 12-Way F GT 150 (BK)

#### Connector Part Information

- OEM: 15332166
- Service: See Catalog
- Description: 12-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: G, H, J, L, A, B, C, D, E, F, K
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins: G, H, J, L : C/A
- Core/Insulation Crimp: Pins: A, B, C, D, E, F, K : E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C309 Body Harness to the Passenger Seat Harness (KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 840 | Battery Positive Voltage | A | OG | 840 | Battery Positive Voltage
B | BK/WH | 651 | Ground | B | BK | 651 | Ground
C | PK | 5057 | Seat Position Sensor - Low Reference | C | PK | 5057 | Seat Position Sensor - Low Reference
D | OG | 1362 | Seat Belt Switch - Right - Signal | D | RD | 1362 | Seat Belt Switch - Right - Signal
E | D-GN | 5060 | Low Speed GMLAN Serial Data | E | D-GN | 5060 | Low Speed GMLAN Serial Data
F | YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal | F | YE | 2079 | Heated Seat Cushion Temperature Sensor Signal
G | PK | 2077 | Heated Seat Cushion Element Supply Voltage | G | RD/WH | 2077 | Heated Seat Cushion Element Supply Voltage
H | PU | 2424 | Driver Heated Seat Back Element Control | H | PU | 2424 | Driver Heated Seat Back Element Control
J | BK | 650 | Ground | J | BK | 650 | Ground
K | YE | 2080 | Driver Heated Seat Cushion Temperature Sensor Low Reference | K | YE | 2080 | Driver Heated Seat Cushion Temperature Sensor Low Reference
L | RD/WH | 640 | Battery Positive Voltage | L | OG | 640 | Battery Positive Voltage
M | -- | -- | Not Used | M | -- | -- | Not Used

### C310 Body Harness to the Fuel Sender Harness

#### Connector Part Information

- OEM: 12065425
- Service: 12125676
- Description: 10-Way F Metri-Pack 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 12048253
- Service: 12117372
- Description: 10-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: C, E, F, G, H, J, K, A, B
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: Pins: C, E, F, G, H, J, K : E/1
- Core/Insulation Crimp: Pins: A, B : 2/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C310 Body Harness to the Fuel Sender Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 120 | Fuel Pump Supply Voltage | A | GY | 120 | Fuel Pump Supply Voltage
B | BK | 850 | Ground | B | BK | 850 | Ground
C | PU | 1589 | Fuel Level Sensor Signal [- Primary] | C | PU | 1589 | Fuel Level Sensor Signal
D | -- | -- | Not Used | D | L-BU | 30 | Fuel Level Sensor Signal
E | GY | 2709 | 5-Volt Reference | E | GY | 2709 | 5-Volt Reference
F | D-GN | 890 | Fuel Tank Pressure Sensor Signal | F | D-GN | 890 | Fuel Tank Pressure Sensor Signal
G | TN | 2759 | Low Reference | G | BK | 2759 | Low Reference
H | TN | 2759 | Low Reference | H | BK/WH | 2759 | Low Reference
J | RD/WH | 2840 | Battery Positive Voltage | J | PK | 2840 | Battery Positive Voltage
K | WH | 1310 | EVAP Canister Vent Solenoid Control | K | WH | 1310 | EVAP Canister Vent Solenoid Control

### C311 Headliner Harness to the Sunshade Harness (UUC)

#### Connector Part Information

- OEM: 12045813
- Service: 12101889
- Description: 4-Way F Metri-Pack 150 Series (CM)

#### Connector Part Information

- OEM: 12052054
- Service: 88988619
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C311 Headliner Harness to the Sunshade Harness (UUC)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
B | GY | 157 | Courtesy Lamp Control | B | GY | 157 | Courtesy Lamp Control
C | OG | 1732 | Courtesy Lamps Supply Voltage | C | OG | 1732 | Courtesy Lamps Supply Voltage
D | BK | 850 | Ground | D | BK | 850 | Ground

### C312 Driver Seat Harness to the Power Seat Harness (AG1 w/KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C312 Driver Seat Harness to the Power Seat Harness (AG1 w/KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/BK | 542 | Battery Positive Voltage | A | RD/BK | 542 | Battery Positive Voltage
B | BK | 650 | Ground | B | BK | 650 | Ground
C | L-GN | 5057 | Seat Position Sensor - Low Reference | C | TN/WH | 5057 | Seat Position Sensor - Low Reference
D | BK | 5016 | Seat Belt Switch - Left - Signal | D | D-BU | 5016 | Seat Belt Switch - Left - Signal

### C313 Passenger Presence Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332141
- Service: 88986249
- Description: 6-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332142
- Service: 89046638
- Description: 6-Way M GT 150/280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C313 Passenger Presence Harness to the Passenger Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG | 840 | Battery Positive Voltage | A | OG | 840 | Battery Positive Voltage
B | YE | 5060 | Low Speed GMLAN Serial Data | B | D-GN | 5060 | Low Speed GMLAN Serial Data
C | WH | 5060 | Low Speed GMLAN Serial Data | C | D-GN | 5060 | Low Speed GMLAN Serial Data
D | BK | 651 | Ground | D | BK | 651 | Ground
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used

### C314 Headliner Harness to the Sunroof Harness (CF5)

#### Connector Part Information

- OEM: 12047886
- Service: 12101822
- Description: 8-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12045688
- Service: 12101827
- Description: 8-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C314 Headliner Harness to the Sunroof Harness (CF5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN | 100 | Sunroof Switch Open Signal | A | BN | 100 | Sunroof Switch Open Signal
B | D-GN | 2074 | Sunroof Switch Express Signal | B | D-GN | 2074 | Sunroof Switch Express Signal
C | OG/BK | 144 | Sunroof Switch Open Vent Signal | C | OG/BK | 144 | Sunroof Switch Open Vent Signal
D | D-BU | 128 | Sunroof Switch Low Reference | D | D-BU | 128 | Sunroof Switch Low Reference
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | BK | 850 | Ground | G | BK | 550 | Ground
H | YE | 643 | Accessory Voltage | H | OG | 643 | Accessory Voltage

### C400 Body Harness to the Chassis Harness

#### Connector Part Information

- OEM: 7283-5946-30
- Service: 88988239
- Description: 10-Way F YESC/USCAR Class III Series, Sealed (BK)

#### Connector Part Information

- OEM: 7282-5946-30
- Service: See Catalog
- Description: 10-Way M YESC/USCAR Class III Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 2, 3, 4, 6, 7, 8, 9
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 1, 10
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C400 Body Harness to the Chassis Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 850 | Ground | 1 | BK | 850 | Ground
2 | L-BU | 5986 | Serial Data Communication Enable | 2 | L-BU | 5986 | Serial Data Communication Enable
3 | TN | 884 | Left Rear Wheel Speed Sensor Signal | 3 | TN | 884 | Left Rear Wheel Speed Sensor Signal
4 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference | 4 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 6 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
7 | TN | 2501 | High Speed GMLAN Serial Data Bus- | 7 | TN | 2501 | High Speed GMLAN Serial Data Bus-
8 | BN | 882 | Right Rear Wheel Speed Sensor Signal | 8 | BN | 882 | Right Rear Wheel Speed Sensor Signal
9 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference | 9 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference
10 | RD/WH | 1740 | Battery Positive Voltage | 10 | RD/WH | 1740 | Battery Positive Voltage

### C403 Body Harness to the Left Tail Lamp Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F 090 Series, Sealed (L-GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (L-GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

- Pins: 4, 2, 6, 5
- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: Pins: 4 : E/A
- Core/Insulation Crimp: Pins: 2, 6, 5 : E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair K

#### C403 Body Harness to the LH Tail Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | 1 | WH | 18 | Left Rear Stop/Turn Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | D-GN | 709 | Left Park Lamp Supply Voltage
5 | L-BU | 20 | Stop Lamp Supply Voltage | 5 | D-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
6 | L-GN | 24 | Backup Lamp Supply Voltage | 6 | L-GN | 24 | Backup Lamp Supply Voltage

### C404 Body Harness to the Right Tail Lamp Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F 090 Series, Sealed (L-GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (L-GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

- Pins: 4, 2, 6, 5
- Terminal/Tray: 7116-4025/11
- Core/Insulation Crimp: Pins: 4 : E/A
- Core/Insulation Crimp: Pins: 2, 6, 5 : E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C404 Body Harness to the Right Tail Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | 1 | WH | 19 | Right Rear Stop/Turn Lamp Supply Voltage
2 | BK | 850 | Ground | 2 | BK | 850 | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BN/WH | 309 | Right Park Lamp Supply Voltage | 4 | D-GN | 309 | Right Park Lamp Supply Voltage
5 | L-BU | 20 | Stop Lamp Supply Voltage | 5 | D-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
6 | L-GN | 24 | Backup Lamp Supply Voltage | 6 | L-GN | 24 | Backup Lamp Supply Voltage

### C409 Body Harness to the Trailer Jumper Harness (V92)

#### Connector Part Information

- OEM: 7283-5889
- Service: See Catalog
- Description: 4-Way F 1.5 Sealed (BK)

#### Connector Part Information

- OEM: 72825889
- Service: See Catalog
- Description: 4-Way M 1.5 Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2, 3
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1, 2, 3
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C409 Body Harness to the Trailer Jumper Harness (V92)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 1618 | Trailer Left Rear Turn/Stop Lamp Supply Voltage | 1 | YE | 1618 | Trailer Left Rear Turn/Stop Lamp Supply Voltage
2 | D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Supply Voltage | 2 | D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Supply Voltage
3 | BN | 2109 | Trailer Park Lamps Supply Voltage | 3 | BN | 2109 | Trailer Park Lamps Supply Voltage
4 | BK | 550 | Ground | 4 | BK | 850 | Ground

### C410 Trailer Harness to the Trailer Jumper Harness (V92)

#### Connector Part Information

- OEM: 72835889
- Service: See Catalog
- Description: 4-Way F 1.5 Sealed (BK)

#### Connector Part Information

- OEM: 72825889
- Service: See Catalog
- Description: 4-Way M 1.5 Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2, 3
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 2, 3, 4
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 1
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C410 Trailer Harness to the Trailer Jumper Harness (V92)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 850 | Ground | 1 | BK | 850 | Ground
2 | BN | 2109 | Trailer Park Lamps Supply Voltage | 2 | BN | 2109 | Trailer Park Lamps Supply Voltage
3 | YE | 1618 | Trailer Left Rear Turn/Stop Lamp Supply Voltage | 3 | YE | 1618 | Trailer Left Rear Turn/Stop Lamp Supply Voltage
4 | D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Supply Voltage | 4 | D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Supply Voltage

### C412 Headliner Harness to the I/P Harness (UUC)

#### Connector Part Information

- OEM: 15326063
- Service: 15326063
- Description: 22-Way F GT 150 280 Series (GY)

#### Connector Part Information

- OEM: 15326064
- Service: See Catalog
- Description: 22-Way M GT 150, 280 (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A1, A2, A9, A10, A11, B1, B2, B3, B9, B10, B11
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A5, A6, A7, A8, B5, B6, B7, B8
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### 412 Headliner Harness to the I/P Harness (UUC)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | BN/WH | 5846 | Video Power Mode Signal | A1 | BN/WH | 5846 | Video Power Mode Signal
A2 | PK/BK | 5844 | Video Bright Control | A2 | PK/BK | 5844 | Video Bright Control
A3-A4 | -- | -- | Not Used | A3-A4 | -- | -- | Not Used
A5 | YE | 343 | Accessory Voltage | A5 | YE | 343 | Accessory Voltage
YE | 343 | Accessory Voltage
A6 | WH | 1487 | Antenna Enable Signal | A6 | WH | 1487 | Antenna Enable Signal
A7 | TN/WH | 5830 | Remote Infra Red Signal (-) | A7 | TN/WH | 5830 | Remote Infra Red Signal (-)
A8 | -- | -- | Not Used | A8 | BARE | 5332 | Infra Red Audio Drain Wire
A9 | -- | -- | Not Used | A9 | OG/BK | 5329 | Left Infra Red Audio Signal
A10 | -- | -- | Not Used | A10 | BN/WH | 5331 | Infra Red Audio Low Reference
A11 | -- | -- | Not Used | A11 | PU/WH | 5330 | Right Infra Red Audio Signal
B1 | WH/BK | 5335 | DVD Video Signal (-) | B1 | WH/BK | 5335 | DVD Video Signal (-)
B2 | D-GN | 6975 | DVD Video Signal (+) | B2 | D-GN | 6975 | DVD Video Signal (+)
B3 | BARE | 6976 | DVD Video Drain Wire | B3 | BARE | 6976 | DVD Video Drain Wire
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | RD/WH | 2340 | Battery Positive Voltage | B5 | RD/WH | 2340 | Battery Positive Voltage
B6 | BK/WH | 1551 | Ground | B6 | BK/WH | 1551 | Ground
B7 | OG/BK | 5831 | Remote Infra Red Signal (+) | B7 | OG/BK | 5831 | Remote Infra Red Signal (+)
B8 | BARE | 6980 | DVD Audio Shield | B8 | BARE | 6980 | DVD Audio Shield
B9 | WH | 5828 | Right DVD Audio Signal (+) | B9 | WH | 5828 | Right DVD Audio Signal (+)
B10 | PU | 6979 | DVD Audio Common | B10 | PU | 6979 | DVD Audio Common
B11 | L-BU | 5826 | Left DVD Audio Signal (+) | B11 | L-BU | 5826 | Left DVD Audio Signal (+)

### C415 Headliner Harness to the Body Harness

#### Connector Part Information

- OEM: 7283-3441-40
- Service: See Catalog
- Description: 8-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-3441-40
- Service: See Catalog
- Description: 8-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 5, 2, 3, 4, 7
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: Pins: 5 : C/A
- Core/Insulation Crimp: Pins: 2, 3, 4, 7 : E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C415 Headliner Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | OG | 1732 | Courtesy Lamps Supply Voltage | 2 | OG | 1732 | Courtesy Lamps Supply Voltage
3 | BK | 850 | Ground (CF5) | 3 | BK | 850 | Ground
4 | BK | 850 | Ground | 4 | BK | 850 | Ground
5 | YE | 643 | Accessory Voltage | 5 | YE | 643 | Accessory Voltage (CF5)
6 | L-GN | 24 | Backup Lamp Supply Voltage | 6 | L-GN | 24 | Backup Lamp Supply Voltage (DD7)
7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | 7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

### C417 Headliner Harness to the Body Harness (U3U)

#### Connector Part Information

- OEM: 7283-6387-40
- Service: See Catalog
- Description: 6-Way F 0.64 Series (L-GY)

#### Connector Part Information

- OEM: 7282-6561-40
- Service: See Catalog
- Description: 6-Way M 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C417 Headliner Harness to the Body Harness (U3U)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-4 | -- | -- | Not Used | 1-4 | -- | -- | Not Used
5 | YE | 655 | Cellular Microphone Signal | 5 | YE | 655 | Cellular Microphone Signal
6 | BARE | 1489 | Drain Wire | 6 | BARE | 1489 | Drain Wire

### C419 Body Harness to the Rear HVAC Harness (C69)

#### Connector Part Information

- OEM: 15326110
- Service: 15306171
- Description: 12-Way F 280 GT Series (BK)

#### Connector Part Information

- OEM: 15326942
- Service: 15326942
- Description: 12-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, B, C, F, G, H, J, K, L
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D, E
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C419 Body Harness to the Rear HVAC Harness (C69)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN | 6555 | Rear Temperature Motor Supply Voltage | A | BN | 6555 | Rear Temperature Motor Supply Voltage
B | GY | 2614 | Auxiliary Air Temperature Door Control | B | GY | 2614 | Auxiliary Air Temperature Door Control
C | L-GN/WH | 5729 | Rear Mode Motor Supply Voltage | C | L-GN/WH | 5729 | Rear Mode Motor Supply Voltage
D | BK | 550 | Ground | D | BK | 550 | Ground
E | RD/WH | 2640 | Battery Positive Voltage | E | RD/WH | 2640 | Battery Positive Voltage
F | GY | 596 | 5-Volt Reference | F | GY | 596 | 5-Volt Reference
G | GY/BK | 754 | Blower Motor Speed Control | G | D-GN | 2211 | Auxiliary Blower Motor Speed Control
H | GY | 2599 | Auxiliary Mode Door Control | H | GY | 2599 | Auxiliary Mode Door Control
J | PK | 2145 | Air Temperature Switch Signal - Right | J | PK | 2145 | Air Temperature Switch Signal - Right
K | OG | 2215 | Auxiliary Mode Door Control | K | OG | 2215 | Auxiliary Mode Door Control
L | GY/BK | 1798 | Low Reference | L | GY/BK | 1798 | Ground
M | -- | -- | Not Used | M | -- | -- | Not Used

### C420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12077921
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 12186799
- Service: See Catalog
- Description: 2-Way M 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN | -- | Side Impact Module - LF - High Control | A | BN | 2137 | Side Impact Module - LF - High Control
B | WH | -- | Side Impact Module - LF - Low Control | B | YE/BK | 2138 | Side Impact Module - LF - Low Control

### C421 Body Harness to the Right Inflatable Restraint Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12077921
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 12186799
- Service: See Catalog
- Description: 2-Way M 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C420 Body Harness to the Left Inflatable Restraint Roof Rail Module Harness (ASF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN | -- | Side Impact Module - RF - High Control | A | TN/WH | 2135 | Side Impact Module - RF - High Control
B | WH | -- | Side Impact Module - RF - Low Control | B | L-GN | 2136 | Side Impact Module - RF - Low Control

### C500 Body Harness to the LF Door Harness

#### Connector Part Information

- OEM: 7183-1584
- Service: See Catalog
- Description: 28-Way F 090 Class II Series, Sealed (WH)

#### Connector Part Information

- OEM: 7182-1581
- Service: See Catalog
- Description: 28-Way M 090 Class II Series Sealed (WH)

#### Terminal Part Information

- Pins: 7, 8, 9, 11, 12, 10, 19, 21
- Terminal/Tray: 7116-4020/11
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 23, 24, 3, 4
- Terminal/Tray: 7116-4021/11
- Core/Insulation Crimp: Pins: 23, 24 : 2/A
- Core/Insulation Crimp: Pins: 3, 4 : E/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 25, 26
- Terminal/Tray: 7116-4022/11
- Core/Insulation Crimp: 4/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C500 Body Harness to the LF Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | GY | 118 | Left Front Speaker Output (-) | 3 | TN | 118 | Left Front Speaker Output (-)
4 | TN | 201 | Left Front Speaker Output (+) | 4 | GY | 201 | Left Front Speaker Output (+)
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | OG/BK | 781 | Driver Door Lock Switch Unlock Signal | 7 | OG/BK | 781 | Driver Door Lock Switch Unlock Signal
8 | PK/BK | 780 | Driver Door Lock Switch Lock Signal | 8 | RD/BK | 780 | Driver Door Lock Switch Lock Signal
9 | L-GN | 1499 | Driver Mirror Motor Left/Down Control | 9 | YE | 1499 | Driver Mirror Motor Left/Down Control
10 | BK/WH | 651 | Ground | 10 | BK | 651 | Ground
11 | YE | 88 | Driver Mirror Motor Up Control | 11 | L-GN | 88 | Driver Mirror Motor Up Control
12 | WH | 81 | Driver Mirror Motor Right Control | 12 | WH | 81 | Driver Mirror Motor Right Control
13 | -- | -- | Not Used | 13 | BK | 746 | Right Front Door Ajar Switch Signal
14-18 | -- | -- | Not Used | 14-18 | -- | -- | Not Used
19 | GY/BK | 745 | Left Front Door Ajar Switch Signal | 19 | RD/BK | 745 | Left Front Door Ajar Switch Signal
20 | -- | -- | Not Used | 20 | PU | 294 | Door Lock Actuator Unlock Control
21 | BK/WH | 651 | Ground | 21 | OG | 651 | Ground
22 | -- | -- | Not Used | 22 | -- | -- | Not Used
23 | GY | 295 | Door Lock Actuator Lock Control | 23 | GY | 295 | Door Lock Actuator Lock Control
24 | TN | 694 | Driver Door Lock Actuator Unlock Control | 24 | TN | 694 | Driver Door Lock Actuator Unlock Control
25 | D-BU | 164 | Power Window Motor Left Front Up Control | 25 | D-BU | 164 | Power Window Motor Left Front Up Control
26 | BN | 165 | Power Window Motor Left Front Down Control | 26 | BN | 165 | Power Window Motor Left Front Down Control
27-28 | -- | -- | Not Used | 27-28 | -- | -- | Not Used

### C600 Body Harness to the RF Door Harness

#### Connector Part Information

- OEM: 7183-1584
- Service: See Catalog
- Description: 28-Way F 090 Class II Series, Sealed (WH)

#### Connector Part Information

- OEM: 7182-1581
- Service: See Catalog
- Description: 28-Way M 090 Class II Series Sealed (WH)

#### Terminal Part Information

- Pins: 7, 8, 9, 11, 12, 13, 21, 23
- Terminal/Tray: 7116-4020/11
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 10, 20, 3, 4
- Terminal/Tray: 7116-4021/11
- Core/Insulation Crimp: Pins: 10, 20 : 2/A
- Core/Insulation Crimp: Pins: 3, 4 : E/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

- Pins: 25, 26
- Terminal/Tray: 7116-4022/11
- Core/Insulation Crimp: 4/A
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C600 Body Harness to the RF Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | D-GN | 117 | Right Front Speaker Output (-) | 3 | TN | 117 | Right Front Speaker Output (-)
4 | L-GN | 200 | Right Front Speaker Output (+) | 4 | GY | 200 | Right Front Speaker Output (+)
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | D-BU | 245 | Passenger Door Lock Switch Unlock Supply Voltage | 7 | OG/BK | 245 | Passenger Door Lock Switch Unlock Signal
8 | L-BU | 244 | Passenger Door Lock Switch Lock Supply Voltage | 8 | RD/BK | 244 | Passenger Door Lock Switch Lock Signal
9 | L-BU/WHT | 1497 | Passenger Mirror Motor Left/Down Control | 9 | YE | 1497 | Passenger Mirror Motor Left/Down Control
10 | GY | 295 | Door Lock Actuator Lock Control | 10 | BK | 295 | Door Lock Actuator Lock Control
11 | PU/WH | 889 | Passenger Mirror Motor Down Control | 11 | L-GN | 889 | Passenger Mirror Motor Down Control
12 | OG/WH | 881 | Passenger Mirror Motor Right Control | 12 | WH | 881 | Passenger Mirror Motor Right Control
13 | TN/WH | 746 | Right Front Door Ajar Switch Signal | 13 | BK | 746 | Right Front Door Ajar Switch Signal
14-19 | -- | -- | Not Used | 14-18 | -- | -- | Not Used
|  |  |  | 19 | RD/BK | 745 | Left Front Door Ajar Switch Signal
20 | TN | 294 | Door Lock Actuator Unlock Control | 20 | PU | 294 | Door Lock Actuator Unlock Control
21 | BK/WH | 651 | Ground | 21 | OG | 651 | Ground
22 | -- | -- | Not Used | 22 | -- | -- | Not Used
23 | BK/WH | 651 | Ground | 23 | GY | 651 | Ground
24 | -- | -- | Not Used | 24 | TN | 694 | Driver Door Lock Actuator Unlock Control
25 | L-BU | 166 | Power Window Master Switch Right Front Up Signal | 25 | D-BU | 166 | Power Window Master Switch Right Front Up Signal
26 | TN | 167 | Power Window Master Switch Right Front Down Signal | 26 | BN | 167 | Power Window Master Switch Right Front Down Signal
27-28 | -- | -- | Not Used | 27-28 | -- | -- | Not Used

### C700 Body Harness to the LR Door Harness

#### Connector Part Information

- OEM: 7123-1413
- Service: 88988485
- Description: 18-Way F (WH)

#### Connector Part Information

- OEM: 7122-1413
- Service: See Catalog
- Description: 21-Way M 0.070 Series (WH)

#### Terminal Part Information

- Pins: A1, A2, A3
- Terminal/Tray: 7116-1050/27
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: B8, C2, C3, C8, B5, C6
- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: Pins: B8, C2, C3, C8 : E/A
- Core/Insulation Crimp: Pins: B5, C6 : E/4
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C700 Body Harness to the LR Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | A1 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
A2 | PU | 169 | Power Window Master Switch Left Rear Down Signal | A2 | PU | 169 | Power Window Master Switch Left Rear Down Signal
A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal | A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal
B1-B4 | -- | -- | Not Used | B1-B4 | -- | -- | Not Used
B5 | TN/WH | 746 | Right Front Door Ajar Switch Signal | B5 | RD/BK | 746 | Right Front Door Ajar Switch Signal
B6 | -- | -- | Not Used | B6 | BK | 746 | Right Front Door Ajar Switch Signal
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | GY | 295 | Door Lock Actuator Lock Control | B8 | GY | 295 | Door Lock Actuator Lock Control
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | YE | 116 | Left Rear Speaker Output (-) | C2 | BN | 116 | Left Rear Speaker Output (-)
C3 | BN | 199 | Left Rear Speaker Output (+) | C3 | YE | 199 | Left Rear Speaker Output (+)
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C5 | -- | -- | Not Used | C5 | PU | 294 | Door Lock Actuator Unlock Control
C6 | BK/WH | 651 | Ground | C6 | BK | 651 | Ground
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | TN | 294 | Door Lock Actuator Unlock Control | C8 | TN | 294 | Door Lock Actuator Unlock Control
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used

### C800 Body Harness to the RR Door Harness

#### Connector Part Information

- OEM: 7123-1413
- Service: 88988485
- Description:18 Way F (WH)

#### Connector Part Information

- OEM: 7122-1413
- Service: See Catalog
- Description: 21-Way M 0.070 Series (WH)

#### Terminal Part Information

- Pins: A1, A2, A3
- Terminal/Tray: 7116-1050/27
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: C2, C3, C6, C5, B6, B8,
- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: Pins: C2, C3, C6, C5 : E/A
- Core/Insulation Crimp: Pins: B6, B8 : E/4
- Core/Insulation Crimp: Pins: :
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C800 Body Harness to the RR Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | A1 | D-GN | 170 | Power Window Master Switch Right Rear Up Signal
A2 | PU | 171 | Power Window Master Switch Right Rear Down Signal | A2 | PU | 171 | Power Window Master Switch Right Rear Down Signal
A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal | A3 | D-BU | 307 | Headlamp Switch Flash to Pass Signal
B1-B4 | -- | -- | Not Used | B1-B4 | -- | -- | Not Used
B5 | -- | -- | Not Used | B5 | RD/BK | 746 | Right Front Door Ajar Switch Signal
B6 | TN/WH | 746 | Right Front Door Ajar Switch Signal | B6 | BK | 746 | Right Front Door Ajar Switch Signal
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | BK/WH | 651 | Ground | B8 | GY | 651 | Ground
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | L-BU | 115 | Right Rear Speaker Output (-) | C2 | BN | 115 | Right Rear Speaker Output (-)
C3 | D-BU | 46 | Right Rear Speaker Output (+) | C3 | YE | 46 | Right Rear Speaker Output (+)
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C5 | TN | 294 | Door Lock Actuator Unlock Control | C5 | PU | 294 | Door Lock Actuator Unlock Control
C6 | GY | 295 | Door Lock Actuator Lock Control | C6 | BK | 295 | Door Lock Actuator Lock Control
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | -- | -- | Not Used | C8 | TN | 294 | Door Lock Actuator Unlock Control
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used

### C900 Body Harness to the Liftgate Harness

#### Connector Part Information

- OEM: 7283-6387-30
- Service: See Catalog
- Description: 6-Way F 064 Series (BK)

#### Connector Part Information

- OEM: 7282-6561-30
- Service: See Catalog
- Description: 6-Way M 064 Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 3, 6, 5, 4
- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: Pins: 1, 2, 3, 6, 5 : H/H
- Core/Insulation Crimp: Pins: 4 : J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Pins: 1, 4
- Terminal/Tray: 7114-4721-02/14
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

- Pins: 2, 3, 6, 5
- Terminal/Tray: 7114-4720-02/14
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### C900 Body Harness to the Liftgate Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | 1303 | Liftgate Ajar Switch Signal | 1 | PK/BK | 1303 | Liftgate Ajar Switch Signal
2 | BN/WH | 309 | Right Park Lamp Supply Voltage | 2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | GY | 391 | Rear Window Wiper Switch Signal | 3 | GY | 391 | Rear Window Wiper Switch Signal
4 | YE | 243 | Accessory Voltage | 4 | YE | 243 | Accessory Voltage
5 | L-GN | 2270 | Rear Window Washer Relay Control | 5 | L-GN | 2270 | Rear Window Washer Relay Control
6 | GY | 5797 | Rear Closure Handle Switch Open Signal | 6 | GY | 5797 | Rear Closure Handle Switch Open Signal

### C901 Body Harness to the Liftgate Harness

#### Connector Part Information

- OEM: 7283-6466-40
- Service: See Catalog
- Description: 6-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-6466-40
- Service: See Catalog
- Description: 6-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Pins: 3
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 6, 5
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 4
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 1, 6, 5
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 3
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 4
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C901 Body Harness to the Liftgate Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 550 | Ground | 1 | BK | 550 | Ground
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control | 3 | L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control
4 | PU | 293 | Rear Defog Element Supply Voltage | 4 | PU | 293 | Rear Defog Element Supply Voltage
5 | BK | 550 | Ground | 5 | BK | 550 | Ground
6 | RD/WH | 2140 | Battery Positive Voltage | 6 | RD/WH | 2140 | Battery Positive Voltage

### C906 Licence Lamp Harness to the Liftgate Harness

#### Connector Part Information

- OEM: 7283-5531-40
- Service: See Catalog
- Description: 6-Way F YESC/USCAR Class III Series (L-GY)

#### Connector Part Information

- OEM: 7282-5531-40
- Service: 88988483
- Description: 4-Way M YESC/USCAR Class III Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C906 Licence Lamp Harness to the Liftgate Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | GY | 5797 | Rear Closure Handle Switch Open Signal | 3 | GY | 5797 | Rear Closure Handle Switch Open Signal
4 | GY | 5797 | Ground | 4 | BK | 550 | Ground