For 1990-2009 cars

Table 1: | SIR Scan Tool Data List
Table 2: | PPS Scan Tool Data List
Table 3: | ROS Scan Tool Data List

The SIR scan tool data list contains all the restraint system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The column, Data List, indicates the location of the parameter within the scan tool menu selections.

Use the SIR scan tool data list as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all of the diagnostic procedures with the Diagnostic System Check - SIR. Use the SIR Scan Tool Data List after the following is determined:

• | There is no published diagnostic trouble code (DTC) procedure nor published symptom procedure for the customer concern.

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The typical data values are obtained from a properly operating vehicle under the conditions specified in the second row of the scan tool data list table. Comparison of the parameter values from the suspect vehicle with the typical data values may reveal the source of the customer concern.

#### SIR Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/No DTCs Set/Driver Seat Belt Buckled/Passenger Seat Belt Unbuckled
Battery Voltage Signal | Data | Volts | 12 Volts
Driver Seat Belt Type | Sensor Data | Switch/Sensor | Switch
Psgr. Seat Belt Type | Sensor Data | Switch/Sensor | Switch
Driver Seat Belt Switch | Sensor Data | Buckled/Unbuckled | Buckled
Passenger Seat Belt Switch | Sensor Data | Buckled/Unbuckled | Unbuckled
Passenger Seat Belt Sensor | Sensor Data | mA | 9 mA
Driver Seat Position Sensor | Sensor Data | Rearward/Forward | Varies
Psgr. Seat Position Sensor | Sensor Data | Rearward/Forward | Varies
Primary Key Status | Key Identification | Invalid/Valid/Unknown | Valid
Received Primary Key | Key Identification | 4-digit number | Varies
Received VIN Digits 2-5 | Key Identification | 4-digit number | Varies
Received VIN Digits 6-7 | Key Identification | 2-digit number | Varies
Run/Crank | Data | Active/Inactive | Varies
SDM Primary Key | Key Identification | 4-digit number | Varies
Secondary Key Status | Key Identification | Invalid/Valid/Unknown | Valid
SIR Warning Indicator | Data | OFF/ON | OFF

#### PPS Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/No DTCs Set/Driver Seat Belt Buckled/Passenger Seat Belt Unbuckled
Battery Voltage Signal | Data | Volts | 12 Volts
Power Mode | Data | Off/Accessory/Run/Crank Request | Run
PPS Fault Status | Data | No Fault/Plant Mode/Fault/Mismatch/Barrier | No Fault
SDM Enable Status | Data | Disabled/Enabled | Enabled
PPS Enable Status | Data | Disabled/Enabled | Enabled
Passenger Classification | Data | Unknown/Calibrating/Empty Seat/Small 1/ Small 2/ Large/Preload | Varies
Passenger Status | Data | No Info./Valid/Invalid Class./Invalid Pos./Invalid Data/ Inval. Class&Pos | Varies
Primary Key Status | Key Identification | Invalid/Valid/Unknown | Valid
PPS Key Status | Key Identification | Invalid/Valid/Unknown | Valid
PPS Primary Key | Key Identification | 4-digit number | Varies
Received Primary Key | Key Identification | 4-digit number | Valid

#### ROS Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/No DTCs Set
Battery Voltage Signal | Data | Volts | 12 Volts
Current Power Mode | Data | Off/Accessory/Run/Crank Request | Run
ROS Primary Key | Data | 4-digit number | Varies
Received Primary Key | Data | 4-digit number | Varies
Primary Key Status | Data | Invalid/Valid/Unknown | Enabled
ROS Occupant Containment Req. | Data | Reserved/Disable/Enable | Enabled
SDM Occupant Containment Status | Data | Disable/Enable | Enabled
Average Speed | Data | km/h | Varies
Vehicle Speed Status | Data | Invalid/Valid | Valid
Engine Virtual Device | Data | Present/Not Present | Present