For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Amplifier Screw | 3 N·m | 27 lb in
Auxiliary Audio/Video Input Assembly Screw | 2 N·m | 18 lb in
Digital Radio Antenna Base Bolt | 5 N·m | 44 lb in
Digital Radio Receiver Nut | 4 N·m | 35 lb in
Front Door Speaker Screw | 2.5 N·m | 22 lb in
Mobile Telephone and Vehicle Location Antenna Assembly Bolt | 5 N·m | 44 lb in
Radio Screw | 2 N·m | 18 lb in
Radio Door Speaker Screw | 2.5 N·m | 22 lb in
Radio Rear Compartment Speaker Bolt | 2.5 N·m | 22 lb in
Radio Rear Compartment Speaker Nut | 2.5 N·m | 22 lb in
Rear Audio Control Module Screw | 2 N·m | 18 lb in
Video Display Assembly Screw | 2 N·m | 18 lb in