For 1990-2009 cars

# Airbag Light On, DTC B1000 Set (Reprogram Passenger Presence System (PPS) Module)

Subject: | Airbag Light On, DTC B1000 Set (Reprogram Passenger Presence System (PPS) Module)

Models: | 2008 Buick Enclave

| 2005-2008 Cadillac SRX

| 2005-2008 Chevrolet Equinox

| 2007-2008 GMC Acadia

| 2006-2008 Pontiac Torrent

| 2007-2008 Saturn OUTLOOK

| 2007-2008 Suzuki XL-7

### Condition

Some customers may comment on the airbag light being illuminated.

Upon investigation, the technician may find DTC B1000 with symptom code 37 set as current or in history.

### Correction

Important: You must contact Techline (1-800-828-6860 English or 1-800-503-3222 French) to obtain a VCI number.

New software for the Passenger Presence System (PPS) has been released to disable this diagnostic check to prevent false setting of DTC B1000. Reprogram the PPS module with updated calibration files using the TIS2WEB Service Programming System (SPS) application. As always, make sure your Tech 2® is updated with the latest software version.

Perform a PPS rezero/preload procedure upon a successful module reprogramming event.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C9840* | Passenger Presence System Module Reprogramming with SPS | 0.4 hr
Add | Diagnosis Time | 0.0-0.3 hr
* This labor operation number is for bulletin use only. This number will not be published in the Labor Time Guide.