For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Frame Applique Screw | 2 N·m | 18 lb in
Front Fascia Center Grille Screw | 2 N·m | 18 lb in
Liftgate Center Applique Assembly Nuts | 5 N·m | 44 lb in
Rear Side Door Front Frame Applique Screw | 2 N·m | 18 lb in
Rear Side Door Rear Frame Applique Screw | 5 N·m | 44 lb in
Rocker Molding Screw | 2 N·m | 18 lb in
Windshield Frame Filler Panel Applique Screw | 1.9 N·m | 17 lb in