For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the front of the headliner. Refer to Headlining Trim Panel Replacement

1 | Mobile Telephone and Vehicle Location Antenna Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 5 N·m (44 lb in)
2 | Mobile Telephone and Vehicle Location Antenna Expansion Sleeve
3 | Mobile Telephone and Vehicle Location Antenna Assembly

#### Procedure

Disconnect electrical connections.