For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Lift the wiper arm blade off the windshield.

1 | Arm, Windshield Wiper (Qty: 1) Tip Hold the arm and release the locking tab before sliding the blade from the wiper arm.
2 | Blade, Windshield Wiper (Qty: 1) Tip Slide the blade rearward out of the wiper arm sheep hook.