For 1990-2009 cars

## Driver or Passenger Seat Back Cushion Heater Replacement Non Fold Flat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Front Seat Replacement - Bucket .

1 | Front Seat Recliner Handle Tip Pull firmly forward on the handle to remove.
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement .
3 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement .
4 | Front Seat Head Restraint Refer to Front Seat Head Restraint Replacement .
5 | Front Seat Head Restraint Guides

#### Procedure

1. Disconnect the lower J-hook retainer from the seat back trim cover.
2. Carefully pull up the trim cover, disengaging the hoop and loop retainers, until the headrest guides are exposed.
3. Squeeze the locking tabs on the headrest guide and pull the guides up and out of the seat back pad.

6 | Front Seat Back Cushion Cover Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
7 | Front Seat Back Heater Element Tip Disconnect the electrical connector and gently pull on the heater element to remove the element from the seat foam. Be careful not to damage the foam pad.

## Driver or Passenger Seat Back Cushion Heater Replacement Fold Flat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Front Seat Replacement - Bucket.

1 | Front Seat Outer Recliner Finish Cover Refer to Front Seat Back Recliner Outer Trim Panel Replacement.
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement.
3 | Front Seat Inner Recliner Finish Cover Refer to Front Seat Back Recliner Inner Trim Panel Replacement.
4 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement.
5 | Front Seat Back Finish Panel Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement.
6 | Front Seat Head Restraint Refer to Front Seat Head Restraint Replacement.
7 | Front Seat Head Restraint Guides Tip Squeeze the bottom of the guides together and push upward to remove.
8 | Front Seat Back Cushion Cover Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.
9 | Front Seat Back Heater Element Tip Disconnect the electrical connector and gently pull on the heater element to remove the element from the seat foam. Be careful not to damage the foam pad.