For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the shift control lever knob Refer to Transmission Control Lever Knob Replacement .
2. Remove the shift control lever boot. Refer to Transmission Control Lever Boot Replacement .

1 | Instrument Panel Lower Brace Bezel Refer to Instrument Panel Lower Brace Bezel Replacement .
2 | Transmission Control Indicator Tip Release 4 retaining tabs to remove the transmission control indicator from the instrument panel lower brace bezel.