For 1990-2009 cars

### Removal Procedure

1. Cycle the sunroof window to the rear.
2. Push down on the right front side of the air deflector.
3. Do the following while holding the right side down:

• | Push the left front side of the air deflector towards the right side.

• | Pull up on the left side until the lower tab clears the roof opening.

4. Swing the air deflector in an upward arc, rearward, to disengage air deflector from the hooks on both sides of the sunroof module.
5. Remove the air deflector from the vehicle.

### Installation Procedure

1. Engage the rear of the air deflector into the side hooks on the sunroof module.
2. Arc the air deflector in a forward motion.
3. Push the right side of the air deflector down into the roof opening.
4. Push the left front side of the air deflector inward and down so the tab clears the roof opening.
5. Close the sunroof window.