For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GM LAN modules on this vehicle also support DTC Symptom information. Refer to DTC Symptom Description for additional information on DTC symptoms.

DTC | DTC Descriptor | Module that Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
Important: Do not clear any DTCs unless instructed to do so by a diagnostic procedure Important: If any DTCs are Powertrain related DTCs, select Capture Info in order to store the DTC information with the scan tool Diagnose any current DTCs in the following order:

1. DTCs that begin with a U
2. B1000, B1001, B1016, B1019, C0550, C0551, C0558, P0601, P0602, P0603, P0604, P0606, P2101, P2107, or P2610
3. B1325, B1424, B1517, C0800, C0899, C0900, P0560, P0562, or P0563
4. Component level DTCs
5. System level DTCs
6. Any remaining DTCs

B0000 | Vehicle Speed Information Circuit | Radio | DTC B0000
B0005 | In Park Switch Signal Circuit | BCM | DTC B0005
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0014 | Driver Side Frontal Deployment Loop | SDM | DTC B0014-B0045
B0015 | Driver Pretensioner Loop | SDM | DTC B0014-B0045
B0016 | Left Roof Rail Initiator 1 Deployment Loop | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0022 | Passenger Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0023 | Right Roof Rail Initiator 1 Deployment Loop | SDM | DTC B0014-B0045
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded With Loop DTCs Present | SDM | DTC B0052 or B0053
B0055 | Side Airbag Deployment Commanded | SDM | DTC B0055
B0056 | Passenger Frontal Airbag Suppressed | SDM | DTC B0056
B0057 | Passenger Side Airbag Suppressed | SDM | DTC B0057
B0058 | Passenger Pretensioner Suppressed | SDM | DTC B0058
B0073 | Passenger Seat Belt Sensor Circuit | SDM | DTC B0073
B0081 | Passenger Presence System | SDM | DTC B0081
B0083 | Front End Sensor 1 | SDM | DTC B0083 or B0084
B0084 | Front End Sensor 2 | SDM | DTC B0083 or B0084
B0085 | Left Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0086 | Right Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0090 | Rollover Sensor | SDM | DTC B0090
B0158 | Outside Air Temperature Sensor Circuit | BCM | DTC B0158
B0228 | Recirculate Position Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0285 | Electric Rear Defrost Circuit Low | BCM | DTC B0285 or B0286
B0286 | Electric Rear Defrost Circuit High | BCM | DTC B0285 or B0286
B0413 | Temperature Control 1 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0423 | Temperature Control 2 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0433 | Temperature Control 3 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0835 | Cruise Control System Active Indicator Circuit | BCM | DTC B0835
B1000 | Electronic Control Unit (ECU) Performance | BCM, DRR, IPC, PPS, Radio, RCDLR, ROS, RSA, SDM, TDM, VCIM | DTC B1000
B1001 | Option Configuration Error | BCM, HVSM, PPS, Radio, ROS, SDM, VCIM | DTC B1001
SDM | DTC B1001
B1016 | VIN Not Programmed | BCM, TDM | DTC B1016
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | Left Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Right Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Left Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Right Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit | DRR | DTC B1259
B1287 | Amplifier Control Signal Circuit | Radio | DTC B1287
B1325 | Device Power Circuit | HVSM, IPC, PPS, Radio | DTC B1325
B1370 | Device Ignition 1 ON and START Circuit | BCM | DTC B1370
Device Ignition 1 Circuit | SDM | DTC B1370
B1380 | Device Ignition Accessory Circuit | BCM | DTC B1380
B1395 | Analog Reference Voltage | HSM | DTC B1395
B1405 | Device Voltage Reference Output 2 Circuit | BCM | DTC B1405
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1428 | Ignition Switched Power Run/Crank Relay Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1441 | Device Ignition Off/Run/Crank Circuit | BCM | DTC B1441
B1475 | Retained Accessory Power Circuit | BCM | DTC B1475
B1516 | Battery Current Sensor Signal | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | High Parasitic Load Detected | BCM | DTC B1527
B1529 | Device Voltage Reference Output Circuit | BCM | DTC B1529
B1925 | Left Seat Cushion Heater Sensor Circuit | HSM | DTC B1925 or B2170
B2170 | Right Seat Cushion Heater Sensor Circuit | HSM | DTC B1925 or B2170
B2345 | Seat Heater Disable Circuit | HSM | DTC B2345
B2425 | Left Seat Heater Circuit | HSM | DTC B2425 or B2430
B2430 | Right Seat Heater Circuit | HSM | DTC B2425 or B2430
B2462 | Global Positioning System (GPS) | Navigation Radio | DTC B2462
B2474 | Navigation Display Head Backlighting Performance | Navigation Radio | DTC B2474
B2508 | Seat Heater Relay Circuit | HSM | DTC B2508 or B2509
B2530 | Front Fog Lamp Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2575 | Headlamp Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signal Mismatch | BCM | DTC B257A
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamp Control Circuit | BCM | DTC B2585
B2600 | Daytime Running Lamp Control Circuit | BCM | DTC B2600
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B2615 | Passenger Compartment Dimming 2 Circuit | BCM | DTC B2615
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2652 | Passenger Compartment Dimming 3 Circuit | BCM | DTC B2652
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2965 | Key In Ignition Circuit Open | BCM | DTC B2965
B3006 | Hood Ajar Circuit Plausibility Failure | BCM | DTC B3006
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109 | Keyless Entry Transmitter 1 Low Battery | RCDLR | DTC B3109
B3110 | Keyless Entry Transmitter 2 Low Battery | RCDLR | DTC B3110
B3111 | Keyless Entry Transmitter 3 Low Battery | RCDLR | DTC B3111
B3112 | Keyless Entry Transmitter 4 Low Battery | RCDLR | DTC B3112
B3445 | Stop Lamp Circuit | BCM | DTC B3445
B3600 | Passenger Compartment Dimming Request Signal Circuit | BCM | DTC B3600
B3622 | Steering Wheel Controls Signal Circuit | BCM | DTC B3622
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3779 | Air Flow Control 9 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B3782 | Air Flow Control 10 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3867 | Right Park Lamp Control Circuit | BCM | DTC B3867
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3884 | Center High Mounted Stop Lamp (CHMSL) Circuit | BCM | DTC B3884
B3922 | Front Wiper Function Select Circuit | BCM | DTC B3922
B3933 | Evaporator Temperature Sensor Circuit | HVAC | DTC B3933
B3935 | Transponder Authentication Error | VTD | DTC B3935
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | ABS Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS) Brake Switch/Sensor Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0196 | Yaw Rate Circuit | EBCM | DTC C0196
C0201 | Antilock Brake System (ABS) Enable Relay Contact Circuit | EBCM | DTC C0201
C0252 | Steering Wheel Position Sensor Uncorrelated | EBCM | DTC C0252
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | EBCM | DTC C0277 or C0890
C0280 | Stability System Active Too Long | EBCM | DTC C0280
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0297 | Brake Applied Output Circuit | BCM | DTC C0297
C0393 | Rear Axle Coupling Solenoid Control Circuit | CCM | DTC C0393
C0394 | Rear Axle Coupling Temperature Sensor Circuit | CCM | DTC C0394
C0460 | Steering Position Signal | EBCM | DTC C0460
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
CCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0558 | Calibration Mismatch | CCM | DTC C0558
C0561 | System Disabled Information Stored | EBCM | DTC C0561
CCM | DTC C0561
C0750 | Left Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0775 | Low Tire Pressure System Sensors Not Learned | RCDLR | DTC C0775
C0890 | Device Voltage Reference Output 3 Circuit | BCM | DTC C0277 or C0890
C0899 | Device Voltage Low | EBCM | DTC C0899
C0900 | Device Voltage High | EBCM | DTC C0900
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0036 | Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0102, or P0103
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0102, or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0102, or P0103
P0111 | Intake Air Temperature (IAT) Sensor Circuit Performance | ECM | DTC P0111, P0112 or P0113
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0111, P0112 or P0113
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0111, P0112 or P0113
P0115 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0119
P0120 | Throttle Position (TP) Sensor Circuit | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0151
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0152
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153
P0134 | HO2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0134 or P0154
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0151 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151
P0152 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0157 | HO2S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0160 | HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0306
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0306
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0306
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0306
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0306
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0328 | Knock Sensor (KS) Circuit High Frequency Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) Circuit High Frequency Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Position (CKP) Sensor A Circuit | ECM | DTC P0335, P0336, or P0338
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0338
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338
P0341 | Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0346 | Intake Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0391 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459
P0446 | Evaporative Emissions (EVAP) Vent System Performance | ECM | DTC P0446
P0449 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit | ECM | DTC P0449, P0498, or P0499
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0481 | Cooling Fan Relay 2 and 3 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0496 | Evaporative Emission (EVAP) System Flow During Non-Purge | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Low Voltage | ECM | DTC P0449, P0498, or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit High Voltage | ECM | DTC P0449, P0498, or P0499
P0506 | Idle Speed Low | ECM | DTC P0506, P0507, or P050A
P0507 | Idle Speed High | ECM | DTC P0506, P0507, or P050A
P050A | Cold Start Idle Air Control (IAC) System Performance | ECM | DTC P0506, P0507, or P050A
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0560 | System Voltage | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562 or P0563
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563
P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601, P0602, P0603, or P0604
P0602 | Control Module Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601, P0602, P0603, or P0604
P0603 | Control Module Long Term Memory Reset | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601, P0602, P0603, or P0604
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601, P0602, P0603, or P0604
P0606 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P0625 | Generator F-Terminal Circuit Low Voltage | ECM | DTC P0625
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629
P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P2100, P2101, or P2119
P0642 | 5 Volt Reference 1 Circuit Low Voltage | ECM | DTC P0642 or P0643
P0643 | 6 Volt Reference 1 Circuit High Voltage | ECM | DTC P0642 or P0643
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0652 | 5 Volt Reference 2 Circuit Low Voltage | ECM | DTC P0652 or P0653
P0653 | 6 Volt Reference 2 Circuit High Voltage | ECM | DTC P0652 or P0653
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relays 2 and 3 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relays 2 and 3 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0698 | 5 Volt Reference 3 Circuit Low Voltage | ECM | DTC P0698 or P0699
P0699 | 5 Volt Reference 3 Circuit High Voltage | ECM | DTC P0698 or P0699
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700
P0703 | Brake Switch Circuit | ECM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706-P0708
P0707 | Transmission Range (TR) Switch Circuit Low Voltage | TCM | DTC P0706-P0708
P0708 | Transmission Range (TR) Switch Circuit High Voltage | TCM | DTC P0706-P0708
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0727 | Engine Speed No Signal | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P0730 | Incorrect Gear Ratio | TCM | DTC P0730
P0731 | Incorrect 1st Gear Ratio | TCM | DTC P0731
P0732 | Incorrect 2nd Gear Ratio | TCM | DTC P0732
P0733 | Incorrect 3rd Gear Ratio | TCM | DTC P0733
P0734 | Incorrect 4th Gear Ratio | TCM | DTC P0734
P0735 | Incorrect 5th Gear Ratio | TCM | DTC P0735
P0736 | Incorrect Reverse Ratio | TCM | DTC P0736
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742
P0762 | Shift Solenoid (SS) 3 Valve Performance - Stuck On | TCM | DTC P0762
P081A | Starter Inhibit Circuit Low Voltage | TCM | DTC P081A or P081B
P081B | Starter Inhibit Circuit High Voltage | TCM | DTC P081A or P081B
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P0864 | TCM Communication Circuit Performance | ECM | DTC P0864
P0897 | Transmission Fluid Life | TCM | DTC P0897
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0966 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0967 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0970 | Shift Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0971 | Shift Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0979 | Shift Solenoid (SS) 3 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0980 | Shift Solenoid (SS) 3 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0982 | Shift Solenoid (SS) 4 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0983 | Shift Solenoid (SS) 4 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0985 | Shift Solenoid (SS) 5 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0986 | Shift Solenoid (SS) 5 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1632 | Theft Deterrent Fuel Disable Signal Received | ECM | DTC P1632
P167D | Ignition Control (IC) Performance | ECM | DTC P167D
P1719 | Incorrect Shifting Detected | TCM | DTC P1719
P1779 | Torque Delivered Signal | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2092 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2098
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 or P2099
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P2100, P2101, or P2119
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P2107
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P2231 or P2234
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2234 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P2231 or P2234
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 2 | ECM | DTC P2232 or P2235
P2270 | HO2S Signal Stuck Lean Bank 1 Sensor 2 | ECM | DTC P2270 or P2272
P2271 | HO2S Signal Stuck Rich Bank 1 Sensor 2 | ECM | DTC P2271 or P2273
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534
P2536 | Ignition Accessory Switch Circuit | TCM | DTC P2536
P2544 | Transmission Torque Request Circuit | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610
P2636 | Fuel Transfer Pump Flow Insufficient | ECM | DTC P2636
P2637 | Transmission Torque Delivered Circuit | TCM | DTC P0115, P0120, P0703, P0727, P0826, P1779, P2544, or P2637
P280A | Transmission Range (TR) Switch Circuit Not Learned | TCM | DTC P280A
U0073 | High Speed Communication Bus | BCM, DRR, HVSM, PPS, PSCM, Radio, RCDLR, ROS, RSA | DTC U0073
U0100 | Lost Communication With Engine/Powertrain Control Module (ECM/PCM) | BCM, PSCM | DTC U0100-U0299
U0101 | Lost Communication With Transmission Control Module (TCM) | BCM | DTC U0100-U0299
U0102 | Lost Communication With Transfer Case Control Module | EBCM | DTC U0100-U0299
U0104 | Lost Communication With Cruise Control Module | BCM | DTC U0100-U0299
U0121 | Lost Communication With Electronic Brake Control Module (EBCM) | BCM | DTC U0100-U0299
U0122 | Lost Communication With Vehicle Dynamics Control Module | BCM | DTC U0100-U0299
U0131 | Lost Communication With Power Steering Control Module | BCM | DTC U0100-U0299
U0140 | Lost Communication With Body Control Module (BCM) | HVSM, PPS, PSCM, RCDLR, ROS, RSA, TDM | DTC U0100-U0299
U0151 | Lost Communication With Sensing and Diagnostic Module (SDM) | PPS, ROS | DTC U0100-U0299
U0155 | Lost Communication With Instrument Panel Cluster (IPC) Control Module | BCM, HVSM, PPS, RCDLR, ROS, RSA, TDM | DTC U0100-U0299
U0164 | Lost Communication With HVAC Control Module | BCM, HVSM | DTC U0100-U0299
U0168 | Lost Communication With Vehicle Theft Deterrent (VTD) Control Module | BCM | DTC U0100-U0299
U0170 | Lost Communication With Passenger Presence System (PPS) | SDM | DTC U0100-U0299
U0184 | Lost Communication With Radio | BCM, DRR, RSA | DTC U0100-U0299
U0198 | Lost Communication With Communication Interface Module (OnStar®) | BCM | DTC U0100-U0299
U0214 | Lost Communication With Remote Function Actuator (RFA) | BCM | DTC U0100-U0299
U1500 | Inter-Device Dedicated Bus 1 | EBCM, VCIM | DTC U1500
U1814 | Powertrain High Speed Communication Enable Circuit | BCM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | Controller Area Network (CAN) Bus Communication | EBCM, IPC | DTC U2100
U2105 | Lost Communication With Engine Control System | EBCM | DTC U2105-U2199
U2106 | Lost Communications With Transmission Control System | EBCM | DTC U2105-U2199
U2107 | Lost Communications With Body Control System | EBCM | DTC U2105-U2199
U2142 | Lost Communication With Yaw Rate Sensor (YRS) | EBCM | DTC U2105-U2199
U2143 | Lost Communications With Steering Angle Sensor (SAS) | EBCM | DTC U2105-U2199